***Erreurs message backup USB tape drive DAT160 attached a serveur rx2660 OS HPUX 11.31:***

erp1 /#ioscan -fnC tape

Class I H/W Path Driver S/W State H/W Type Description

=====================================================================

tape 0 255/1/0.1.0 stape CLAIMED DEVICE HP DAT160

 /dev/rmt/0m /dev/rmt/c1t1d0BEST

 /dev/rmt/0mb /dev/rmt/c1t1d0BESTb

 /dev/rmt/0mn /dev/rmt/c1t1d0BESTn

 /dev/rmt/0mnb /dev/rmt/c1t1d0BESTnb

…………………………………………………………………………………………………………………….

erp1 /#mt -t /dev/rmt/0m status

Drive: HP DAT160

Format:

Status: [41114800] BOT online compression immediate-report-mode

File: 0

Block: 0

…………………………………………………………………………………………………………………….

erp1 /#make\_tape\_recovery -Av

 \* Creating local directories for configuration files and archive.

======= 02/20/09 11:03:40 WAT Started make\_tape\_recovery. (Fri Feb 20

 11:03:40 WAT 2009)

 @(#)Ignite-UX Revision C.7.5.142

 @(#)ignite/net\_recovery (opt) Revision:

 /branches/IUX\_RA0803/ignite/src@72866 Last Modified: 2008-02-06

 15:49:50 -0700 (Wed, 06 Feb 2008)

 \* Testing for necessary pax patch.

 \* Recovery Archive Description = Recovery Archive

 \* Recovery Archive Location = /dev/rmt/0mn

\* Number of Archives to Save = 2

 \* Pax type = tar

 In? dsk/vg name minor# Associated disks/mountpoints

 2 v /dev/vg00 0x00 /dev/disk/disk0\_p2

 /dev/vg00/lvol1 /stand 2

 /dev/vg00/lvol2

 /dev/vg00/lvol3 / 2

 /dev/vg00/lvol4 /tmp 2

 /dev/vg00/lvol5 /home 2

 /dev/vg00/lvol6 /opt 2

 /dev/vg00/lvol7 /usr 2

 /dev/vg00/lvol8 /var 2

 /dev/vg00/lvback /back 2

 0 v /dev/vgtest 0x01 /dev/disk/disk8 /dev/disk/disk10

 \*\* 0 - The Volume Group or Filesystem is Not included in the

 System Recovery Archive

 \*\* 1 - The Volume Group or Filesystem is Partially included in the

 System Recovery Archive

 \*\* 2 - The Volume Group or Filesystem is Fully included in the

 System Recovery Archive

 \* Checking Versions of Ignite-UX filesets

 \* Scanning system for IO devices...

 \* Boot device is: 0/3/0/0/0/0.0x0.0x4000000000000000

 \* Creating System Configuration.

 \* /opt/ignite/bin/save\_config -f

 /var/opt/ignite/recovery/2009-02-20,11:03/system\_cfg vg00

 \* Backing Up Volume Group /dev/vg00

 \* /usr/sbin/vgcfgbackup /dev/vg00

 \* Creating Map Files for Volume Group /dev/vg00

 \* /usr/sbin/vgexport -s -p -m /etc/lvmconf/vg00.mapfile /dev/vg00

 \* Backing Up Volume Group /dev/vgtest

 \* /usr/sbin/vgcfgbackup /dev/vgtest

 \* Creating Map Files for Volume Group /dev/vgtest

 \* /usr/sbin/vgexport -s -p -m /etc/lvmconf/vgtest.mapfile /dev/vgtest

 \* Creating Control Configuration.

 \* Creating Archive File List

 \* Creating Archive Configuration

 \* /opt/ignite/lbin/make\_arch\_config -c

 /var/opt/ignite/recovery/2009-02-20,11:03/archive\_cfg -g

 /var/opt/ignite/recovery/2009-02-20,11:03/flist -n 2009-02-20,11:03 -r

 ipf -b 64 -d Recovery\ Archive -t 22 -i 1 -m t

 \* Saving the information about archive to

 /var/opt/ignite/recovery/previews

 \* Creating The Tape Archive

 \* Checking configuration file for Syntax

WARNING: You are about to create an Itanium-based recovery tape. If this

 system does NOT support direct tape boot, you will need to perform

 "two-step media recovery" where the boot media (CD or DVD) has the

 same version of Ignite-UX as the version on this tape.

 \* Complete writing boot LIF onto tape.

 \* /opt/ignite/data/scripts/make\_sys\_image -c n -d /dev/rmt/0mn -t n -s

 local -n 2009-02-20,11:03 -m t -w

 /var/opt/ignite/recovery/2009-02-20,11:03/recovery.log -u -R -g

 /var/opt/ignite/recovery/2009-02-20,11:03/flist -a 9507890

 \* Preparing to create a system archive.

 \* Archiving contents of erp1 via tar image to local device /dev/rmt/0mn.

pax: write : Invalid argument

pax: A write error has occurred.

WARNING: The pax command returned a non-zero exit status (exit status 1.)

ERROR: The find\_files command failed (exit status 141).

ERROR: The make\_sys\_image command failed. The system recovery archive will not be created.

======= 02/20/09 11:20:21 WAT make\_tape\_recovery completed unsuccessfully

…………………………………………………………………………………………………………………….

erp1 /#tar -cv /tmp

a /tmp/.kc.trace 1 blocks

tar: /tmp/.AgentSockets/A is not a file. Not dumped

a /tmp/install.vars 4 blocks

a /tmp/krun.1453 0 blocks

a /tmp/man003502 11 blocks

a /tmp/swlist 0 blocks

a /tmp/X11\_newfonts.log 2 blocks

a /tmp/sd\_ipd\_acl.2649 1 blocks

a /tmp/ntlc.3625 20 blocks

a /tmp/rpcbind.file 5 blocks

a /tmp/portmap.file 2 blocks

a /tmp/ipv6agt.crashlog 0 blocks

a /tmp/llbdbase.dat 0 blocks

a /tmp/.s.PGSQL.10864.lock 1 blocks

tar: /tmp/.s.PGSQL.10864 is not a file. Not dumped

a /tmp/iotreeip.trc 5 blocks

a /tmp/raidsa\_log 2 blocks

a /tmp/patcheUSB/create\_depot\_hpux.11.31 12 blocks

a /tmp/patcheUSB/patch\_manifest 2 blocks

a /tmp/patcheUSB/PHCO\_37481 1618 blocks

a /tmp/patcheUSB/PHCO\_37931 3477 blocks

a /tmp/patcheUSB/PHCO\_38735 1647 blocks

a /tmp/patcheUSB/PHKL\_38544 3985 blocks

a /tmp/patcheUSB/PHKL\_38169 243 blocks

a /tmp/patcheUSB/PHKL\_37883 1344 blocks

a /tmp/patcheUSB/PHKL\_37870 274 blocks

a /tmp/patcheUSB/PHKL\_37815 1775 blocks

a /tmp/patcheUSB/PHKL\_38732 1809 blocks

a /tmp/patcheUSB/PHKL\_38733 477 blocks

a /tmp/patcheUSB/PHKL\_38734 76 blocks

a /tmp/patcheUSB/README\_hp-ux 4 blocks

a /tmp/patcheUSB/PHCO\_37481.text 10 blocks

a /tmp/patcheUSB/PHCO\_37481.depot 1140 blocks

a /tmp/patcheUSB/PHCO\_37931.text 49 blocks

a /tmp/patcheUSB/PHCO\_37931.depot 2440 blocks

a /tmp/patcheUSB/PHCO\_38735.text 11 blocks

a /tmp/patcheUSB/PHCO\_38735.depot 1160 blocks

a /tmp/patcheUSB/PHKL\_37815.text 27 blocks

a /tmp/patcheUSB/PHKL\_37815.depot 1240 blocks

a /tmp/patcheUSB/PHKL\_37870.text 10 blocks

a /tmp/patcheUSB/PHKL\_37870.depot 180 blocks

a /tmp/patcheUSB/PHKL\_37883.text 16 blocks

a /tmp/patcheUSB/PHKL\_37883.depot 940 blocks

Tar: end of tape

Tar: to continue, enter device/file name when ready or null string to quit.

/dev/rmt/0m

User opened file /dev/rmt/0m to continue.

a /tmp/patcheUSB/PHKL\_38169.text 7 blocks

a /tmp/patcheUSB/PHKL\_38169.depot 160 blocks