***** EARLY BOOT VFP : SYSTEM ALERT *****
SYSTEM NAME: uninitialized
DATE: 11/06/2008 TIME: 12:33:12
ALERT LEVEL: 6 = Boot possible, pending failure - action required

REASON FOR ALERT
SOURCE: 8 = I/O 
SOURCE DETAIL: 5 = I/O device adapter   SOURCE ID: FF
PROBLEM DETAIL: 6 = configuration error

LEDs:  RUN      ATTENTION     FAULT     REMOTE     POWER
       FLASH    FLASH         OFF       OFF        ON

0x2000006685FF2384 FFFFFFFF FFFFFFFF - type  4 = Physical Location
0x5800086685FF2384 00006C0A 060C210C - type 11 = Timestamp 11/06/2008 12:33:12
A/a: ack read of this entry - Q/q: quit Virtual Front Panel Display
Anything else redisplay the log entry
->Choice:a
*****************************************

 ***** EARLY BOOT VFP : SYSTEM ALERT *****
SYSTEM NAME: uninitialized
DATE: 11/06/2008 TIME: 12:33:12
ALERT LEVEL: 6 = Boot possible, pending failure - action required

REASON FOR ALERT
SOURCE: 8 = I/O 
SOURCE DETAIL: 5 = I/O device adapter   SOURCE ID: FF
PROBLEM DETAIL: 6 = configuration error

LEDs:  RUN      ATTENTION     FAULT     REMOTE     POWER
       FLASH    FLASH         OFF       OFF        ON

0x2000006685FF2384 FFFFFFFF FFFFFFFF - type  4 = Physical Location
0x5800086685FF2384 00006C0A 060C210C - type 11 = Timestamp 11/06/2008 12:33:12
A/a: ack read of this entry - Q/q: quit Virtual Front Panel Display
Anything else redisplay the log entry
->Choice:q
*****************************************

 Reactivating console.
 Type Ctrl-B to access Guardian Service Processor Commands  

 ************* SYSTEM ALERT **************
SYSTEM NAME: uninitialized
DATE: 11/06/2008 TIME: 12:33:12
ALERT LEVEL: 6 = Boot possible, pending failure - action required

REASON FOR ALERT
SOURCE: 8 = I/O 
SOURCE DETAIL: 5 = I/O device adapter   SOURCE ID: FF
PROBLEM DETAIL: 6 = configuration error

LEDs:  RUN      ATTENTION     FAULT     REMOTE     POWER
       FLASH    FLASH         OFF       OFF        ON

0x2000006685FF2384 FFFFFFFF FFFFFFFF - type  4 = Physical Location
0x5800086685FF2384 00006C0A 060C210C - type 11 = Timestamp 11/06/2008 12:33:12
A: ack read of this entry - X: Disable all future alert messages
Anything else skip redisplay the log entry
->Choice:x
*****************************************

CAUTION: System Alerts have been disabled. This will re-enable with 
a re-boot or power-on of the system. To re-enable system alerts now, you
may use the AC (Alert Display Configuration) command.

 ************* SYSTEM ALERT **************
Alert messages are now disabled. Enter Commands Interface AC command to enable them again
*****************************************

Firmware Version  41.39

Duplex Console IO Dependent Code (IODC) revision 1

------------------------------------------------------------------------------
   (c) Copyright 1995-2000, Hewlett-Packard Company, All rights reserved
------------------------------------------------------------------------------

  Processor   Speed            State           CoProcessor State  Cache Size
  Number                                       State              Inst    Data
  ---------  --------   ---------------------  -----------------  ------------
      0      360  MHz   Active                 Functional         512 KB   1 MB
      3      360  MHz   Idle                   Functional         512 KB   1 MB

  Central Bus Speed (in MHz)  :         82  
  Available Memory            :    6291456  KB
  Good Memory Required        :     238088  KB

   Primary boot path:    0/0/1/1.2           
   Alternate boot path:  0/0/2/0.2           
   Console path:         0/0/4/0.0           
   Keyboard path:        0/0/4/0.0           
 WARNING:  The system serial number is invalid.  

 WARNING:  The non-destructive test bit was set, so memory was not tested 
            destructively.  Information only, no action required. 

 WARNING:  One or more SCSI controllers are not configured 
            correctly for auto termination.  Check controller settings 
            using the SCSI command in the Service menu.

Service Menu: Enter command > scsi

 Path (dec)     Initiator ID     SCSI Rate     Auto Term 
0/0/46/127/194/226/1281818846574       Unknown       Misc. Error 
0/0/1/1        7                Ultra         Unknown 
0/0/2/0        7                Ultra         Unknown 
194/136/108/127/194/136/1127                Unknown       Misc. Error 
/220/104/58/32/02143455340       Unknown       Misc. Error 
0/0/46/127/194/226/1281818846574       Unknown       Misc. Error 
127/192/34/52  Unknown          Unknown       Misc. Error 
127/192/128/18846               Unknown       Misc. Error 
194/135/136/127/193/77/180Unknown          Unknown       Misc. Error 
253/220/104/58/32/0Unknown          Unknown       Misc. Error 
109/97/116/99  Unknown          Unknown       Misc. Error 
127/192/34/52  Unknown          Unknown       Unknown 
127/192/128/18846               Unknown       Unknown 
105/101/110/127/194/135/92Unknown          Unknown       Misc. Error 
109/97/116/99  Unknown          Unknown       Misc. Error 
194/136/108/127/194/136/112Unknown          Unknown       Misc. Error