npsc3:/var/tmp# /opt/hparray/bin/download -C /var/tmp/C5447A.HP60.frm 000000379D3C
 Copyright (C) 1995, 1997 Hewlett-Packard Company
 The controller is in a state that will
 not accept a microcode download.

 AutoRAID firmware download program ending.
npsc3:/var/tmp# arraydsp -a 000000379D3C                                     

   Vendor ID           = HP
   Product ID          = C5447A
   Array serial number = 000000379D3C
   ----------------------------------------------------
   Array State           = NO QUORUM
   Server name           = npsc3.sbv.org.vn
   Array type            = 3
   Mfg. Product Code     = IJMTU00003

   --- Disk space usage --------------------
   Total physical               = 104199 MB *
   Allocated to LUNs            =      0 MB *
   Used as Active Hot spare     =      0 MB *
   Used by non-included disks   = 104199 MB *
   Used for Redundancy          =      0 MB *
   Unallocated (avail for LUNs) =      0 MB *
   -----------------------------------------

   THE FOLLOWING WARNING(S) EXIST:
   - Data Unavailable
   - Redundancy Loss
   - Active Hot Spare Unavailable
   - Physical Disk Downed or Disk Problem
   - Missing Disk

   Vendor ID           = HP
   Product ID          = C5447A
   Array serial number = 000000379D3C
   ----------------------------------------------------

   Total capacity allocated to LUNs = 0 MB *

   Information for disk in slot A2:
      Disk State             = PREVIOUSLY USED
      Vendor                 = SEAGATE
      Product ID             = ST318203LC
      Capacity               = 17366 MB *
      Max. block addr        = 35566479
      Block length           = 512
      Serial number          = 72810000W016
      Firmware revision      = HP01
      Drive ID number        = FFFFFFFD104CDF10
      Volume set serial no.  = 14FBD      53

   Information for disk in slot A3:
      Disk State             = PREVIOUSLY USED
      Vendor                 = SEAGATE
      Product ID             = ST318203LC
      Capacity               = 17366 MB *
      Max. block addr        = 35566479
      Block length           = 512
      Serial number          = 14400000W016
      Firmware revision      = HP01
      Drive ID number        = FFFFFFFD1080A300
      Volume set serial no.  = 14FBD      53

   Information for disk in slot B3:
      Disk State             = PREVIOUSLY USED
      Vendor                 = SEAGATE
      Product ID             = ST318203LC
      Capacity               = 17366 MB *
      Max. block addr        = 35566479
      Block length           = 512
      Serial number          = 302900001016
      Firmware revision      = HP01
      Drive ID number        = FFFFFFFD10DA80F8
      Volume set serial no.  = 14FBD      53

   Information for disk in slot A4:
      Disk State             = PREVIOUSLY USED
      Vendor                 = SEAGATE
      Product ID             = ST318203LC
      Capacity               = 17366 MB *
      Max. block addr        = 35566479
      Block length           = 512
      Serial number          = 889200001016
      Firmware revision      = HP01
      Drive ID number        = FFFFFFFD10EBC5F8
      Volume set serial no.  = 14FBD      53

   Information for disk in slot A5:
      Disk State             = PREVIOUSLY USED
      Vendor                 = SEAGATE
      Product ID             = ST318203LC
      Capacity               = 17366 MB *
      Max. block addr        = 35566479
      Block length           = 512
      Serial number          = 703400001015
      Firmware revision      = HP01
      Drive ID number        = FFFFFFFD10A7E5F7
      Volume set serial no.  = 14FBD      53

   Information for disk in slot A6:
      Disk State             = PREVIOUSLY USED
      Vendor                 = SEAGATE
      Product ID             = ST318404LC
      Capacity               = 17366 MB *
      Max. block addr        = 35566479
      Block length           = 512
      Serial number          = FV2B00002051
      Firmware revision      = HP06
      Drive ID number        = 1247F       2
      Volume set serial no.  = 14FBD      53

   Total capacity of all installed physical disks = 104199 MB *

   Information for controller X:
      Vendor ID            = HP      
      Product ID           = C5447A          
      Array serial number  = 000000379D3C
      Primary              = FALSE
      SCSI Address         = 6
      Serial number        = R83AADF859491111
      Paired serial number = R97KADH747901111
      Product revision     = HP56

   Information for controller Y:
      Vendor ID            = HP      
      Product ID           = C5447A          
      Array serial number  = 000000379D3C
      Primary              = TRUE
      SCSI Address         = 6
      Serial number        = R97KADH747901111
      Paired serial number = R83AADF859491111
      Product revision     = HP56

   Vendor ID           = HP
   Product ID          = C5447A
   Array serial number = 000000379D3C
   ----------------------------------------------------
   Overall State of Array          = NO QUORUM
   Array configuration:
      Active Hot Spare Desired     = ENABLED
      Auto Include                 = ENABLED
      Auto Rebuild                 = ENABLED
      Rebuild Priority             = HIGH
      Capacity Depletion Threshold = 0%
      Write Working Set Interval   = 8640 seconds
      Language                     = ENGLISH
      Log Full Warning             = DISABLED
      Volume Set Partitioning      = DISABLED
      Format Pattern Fill          = DISABLED
      Subsystem Type ID            = 12
      LUN Creation Limit           = 8
      Maximum LUN Creation Limit   = 8
   Array SCSI configuration:
      Controller X SCSI Address    = 6
      Controller Y SCSI Address    = 6
      Write Cache                  = DISABLED
      Read Cache                   = DISABLED
      SCSI Parity Checking         = ENABLED
      SDTR                         = ENABLED
      WDTR                         = ENABLED
      Terminator Power             = ENABLED
      Unit Attention               = ENABLED
      Disable Remote Reset         = ENABLED
      Secondary Controller Offline = DISABLED
      Very Early Busy              = DISABLED
      Queue Full Threshold         = 1952
      Maximum Queue Full Threshold = 1952
      Simplified Resiliency Setting = Normal
      Single Controller Warning    = ENABLED
      Lock Write Cache On          = TRUE
      Disable NVRAM on WCE False   = FALSE
      Disable NVRAM with One Ctrlr = TRUE
      Disable NVRAM on UPS absent  = FALSE
      Force Unit Access Response   = 2
      Disable Read Hits            = FALSE
      Resiliency Threshold         = 4

   THE FOLLOWING WARNING(S) EXIST:
   - Data Unavailable
   - Redundancy Loss
   - Active Hot Spare Unavailable
   - Physical Disk Downed or Disk Problem
   - Missing Disk

   Vendor ID           = HP
   Product ID          = C5447A
   Array serial number = 000000379D3C
   ----------------------------------------------------
   Raid 0/1 blocks       = 80036480
   Raid 0/1 block length = 512
   Raid 0/1 capacity     = 39080 MB *

   Vendor ID           = HP
   Product ID          = C5447A
   Array serial number = 000000379D3C
   ----------------------------------------------------
   Fan F1              = GOOD
   Fan F2              = GOOD
   Fan F3              = GOOD
   Power supply PS1    = GOOD
   Power supply PS2    = GOOD
   Power supply PS3    = GOOD

   Controller X:
      Overall state    = GOOD
      Battery #0 state = GOOD
      Battery #1 state = GOOD
      DRAM    #0 state = GOOD
      NVRAM   #0 state = GOOD
      NVRAM   #1 state = GOOD
   Controller Y:
      Overall state    = GOOD
      Battery #0 state = GOOD
      Battery #1 state = GOOD
      DRAM    #0 state = GOOD
      NVRAM   #0 state = GOOD
      NVRAM   #1 state = GOOD