; J4819A Configuration Editor; Created on release #E.10.04
hostname "Switch 5001183 UP1" snmp-server contact "mis@xyz.com" snmp-server location "Upstairs Wire Closet" max-vlans 40 time timezone -300 time daylight-time-rule Continental-US-and-Canada cdp run module 7 type J4821A module 4 type J4820A module 2 type J4820A module 3 type J4820A module 1 type J4907A module 8 type J4821A module 6 type J4821A module 5 type J4821A interface G1    speed-duplex auto-1000 exitinterface G2    speed-duplex auto-1000 exitinterface G3    speed-duplex auto-1000 exitinterface G4    speed-duplex auto-1000 exitinterface D1    no lacpexitinterface D2    no lacpexitinterface D3    no lacpexitinterface D4    no lacpexitinterface D5    no lacpexitinterface D6    no lacpexitinterface D7    no lacpexitinterface D8    no lacpexitinterface D9    no lacpexitinterface D10    no lacpexitinterface D11    no lacpexitinterface D12    no lacpexitinterface D13    no lacpexitinterface D14    no lacpexitinterface D15    no lacpexitinterface D16    no lacpexitinterface D17    no lacpexitinterface D18    no lacpexitinterface D19    no lacpexitinterface D20    no lacpexitinterface D21    no lacpexitinterface D22    no lacpexitinterface D23    no lacpexitinterface D24    no lacpexitinterface B1    no lacpexitinterface B2    no lacpexitinterface B3    no lacpexitinterface B4    no lacpexitinterface B5    no lacpexitinterface B6    no lacpexitinterface B7    no lacpexitinterface B8    no lacpexitinterface B9    no lacpexitinterface B10    no lacpexitinterface B11    no lacpexitinterface B12    no lacpexitinterface B13    no lacpexitinterface B14    no lacpexitinterface B15    no lacpexitinterface B16    no lacpexitinterface B17    no lacpexitinterface B18    no lacpexitinterface B19    no lacpexitinterface B20    no lacpexitinterface B21    no lacpexitinterface B22    no lacpexitinterface B23    no lacpexitinterface B24    speed-duplex 100-half    no lacpexitinterface C1    no lacpexitinterface C2    no lacpexitinterface C3    no lacpexitinterface C4    no lacpexitinterface C5    no lacpexitinterface C6    no lacpexitinterface C7    no lacpexitinterface C8    no lacpexitinterface C9    no lacpexitinterface C10    no lacpexitinterface C11    no lacpexitinterface C12    no lacpexitinterface C13    no lacpexitinterface C14    no lacpexitinterface C15    no lacpexitinterface C16    no lacpexitinterface C17    no lacpexitinterface C18    no lacpexitinterface C19    no lacpexitinterface C20    no lacpexitinterface C21    no lacpexitinterface C22    no lacpexitinterface C23    no lacpexitinterface C24    no lacpexitinterface H1    speed-duplex auto-1000    no lacpexitinterface H2    speed-duplex auto-1000    no lacpexitinterface H3    speed-duplex auto-1000    no lacpexitinterface H4    speed-duplex auto-1000    no lacpexittrunk H1-H2 Trk1 Trunk trunk E1-E2 Trk2 Trunk interface F1    speed-duplex auto-1000    no lacpexitinterface F2    speed-duplex auto-1000    no lacpexitinterface F3    speed-duplex auto-1000    no lacpexitinterface F4    speed-duplex auto-1000    no lacpexitinterface E1    speed-duplex auto-1000    no lacpexitinterface E2    speed-duplex auto-1000    no lacpexitinterface E3    speed-duplex auto-1000    no lacpexitinterface E4    speed-duplex auto-1000    no lacpexittrunk F1-F2 Trk3 Trunk trunk F3-F4 Trk4 Trunk trunk H3-H4 Trk18 Trunk trunk E3-E4 Trk5 Trunk interface A15    no lacpexitinterface A16    no lacpexittrunk A15-A16 Trk10 Trunk ip default-gateway 172.20.10.10 ip routing no ip directed-broadcast no timesync vlan 1    name "DEFAULT_VLAN"    untagged A1-A14,B1-B24,C1-C24,G1-G4,Trk1-Trk5,Trk10,Trk18    ip address 172.20.10.100 255.255.0.0    ip helper-address 172.20.4.1    no untagged D1-D24    ip igmp    exit vlan 2    name "DMZ"    untagged D1-D11    ip address 111.222.137.253 255.255.255.0    tagged Trk2    ip igmp    exit vlan 3    name "Outside"    untagged D13-D24    ip address 111.222.136.253 255.255.255.0    ip igmp    exit vlan 15    name "Audio"    ip address 192.168.98.201 255.255.255.0    tagged A14,Trk1,Trk5    exit vlan 66    name "Wireless"    ip address 172.20.66.100 255.255.255.0    exit vlan 20    name "Unity"    ip address 192.168.56.1 255.255.255.0    tagged A14,Trk4,Trk10    exit vlan 100    name "SRCP"    ip address 172.20.200.1 255.255.255.0    tagged Trk10    exit vlan 8    name "DG-Verizon"    untagged D12    ip address 123.45.67.89 255.255.255.0    tagged Trk2    exit vlan 12    name "Avid_Project"    ip address 192.168.54.226 255.255.255.0    tagged A14,Trk2,Trk4,Trk18    exit fault-finder bad-driver sensitivity high fault-finder bad-transceiver sensitivity high fault-finder bad-cable sensitivity high fault-finder too-long-cable sensitivity high fault-finder over-bandwidth sensitivity high fault-finder broadcast-storm sensitivity high fault-finder loss-of-link sensitivity high ip route 192.168.11.0 255.255.255.0 172.20.10.9 ip route 0.0.0.0 0.0.0.0 172.20.10.10 ip icmp reply-limit ip icmp burst-normal 1 no ip icmp redirects no ip icmp unreachable no ip icmp echo broadcast-request spanning-tree Trk1 priority 4spanning-tree Trk2 priority 4spanning-tree Trk3 priority 4spanning-tree Trk4 priority 4spanning-tree Trk5 priority 4spanning-tree Trk10 priority 4spanning-tree Trk18 priority 4router rip   exitpassword managerpassword operator