interface B14

 no lacp

exit

interface B15

 no lacp

exit

interface B17

 no lacp

exit

interface C6

 no lacp

exit

ip default-gateway 192.168.10.1

sntp server 192.168.10.9

ip routing

timesync sntp

sntp unicast

sntp 1800

snmp-server community "public" Unrestricted

snmp-server community "private" Operator Unrestricte

snmp-server host 192.168.10.108 "public"

snmp-server host 192.168.10.31 "public"

snmp-server host 192.168.10.234 "public"

vlan 1

 name "DEFAULT\_VLAN"

 untagged A1-A4

 no ip address

 no untagged B1-B24,C1-C24

 exit

vlan 10

 name "VLAN10"

 untagged B1-B23,C1-C24

 ip address 192.168.10.4 255.255.255.0

 tagged A1

 exit

vlan 200

 name "VLAN200"

 tagged A1,B23

 exit

vlan 140

 name "VLAN140"

 untagged B24

 tagged A1

 exit

vlan 13

 name "VLAN13"

 no ip address

 tagged A1

 exit

fault-finder bad-driver sensitivity high

fault-finder bad-transceiver sensitivity high

fault-finder bad-cable sensitivity high

fault-finder too-long-cable sensitivity high

fault-finder over-bandwidth sensitivity high

fault-finder broadcast-storm sensitivity high

fault-finder loss-of-link sensitivity high

fault-finder duplex-mismatch-HDx sensitivity high

fault-finder duplex-mismatch-FDx sensitivity high

spanning-tree

password manager

password operator

Hangar\_8#