; J8773A Configuration Editor; Created on release #L.11.24

hostname "2ND-FLR-TOP-4208-111.13"
time timezone 60
module 6 type J8768A
module 1 type J8764A
module 5 type J8764A
module 4 type J8764A
module 2 type J8764A
module 3 type J8764A
module 7 type J9033A
trunk A1,B1,C1,D1 Trk1 Trunk
trunk G23-G24 Trk2 Trunk
ip default-gateway 192.168.111.10
sntp server 192.168.111.8
ip routing
timesync sntp
sntp unicast
snmp-server community "public" Unrestricted
snmp-server host 192.168.111.22 "public"
vlan 1
   name "DEFAULT_VLAN"
   untagged A2-A16,B2-B16,C2-C16,D2-D16,E1-E16,F1-F24,G1-G8,G13-G14,G16,G18-G22,
Trk1-Trk2
   ip address 192.168.111.13 255.255.255.0
   no untagged G9-G12,G15,G17
   exit
vlan 20
   name "WM_Data1"
   untagged G11-G12
   ip address 10.0.20.3 255.255.255.0
   tagged A2,Trk1-Trk2
   exit
vlan 30
   name "WM_Data2"
   untagged G9-G10
   ip address 10.0.30.3 255.255.255.0
   tagged A2,Trk1-Trk2
   exit
vlan 10
   name "WM_VOIP"
   untagged G15,G17
   ip address 10.0.10.3 255.255.255.0
   qos priority 6
   ip helper-address 192.168.111.9
   tagged A2,F9,Trk1-Trk2
   voice
   exit
ip route 0.0.0.0 0.0.0.0 192.168.111.10
spanning-tree
spanning-tree Trk1 priority 4
spanning-tree Trk2 priority 4
password manager

; J8773A Configuration Editor; Created on release #L.11.24

hostname "2ND-FLR-BOTTOM-4208-111.14"
time daylight-time-rule Western-Europe
module 2 type J8764A
module 3 type J8764A
module 4 type J8764A
module 5 type J8764A
module 1 type J8764A
module 6 type J8776A
trunk A1,B1,C1,D1 Trk1 Trunk
trunk A8,B8,C8,D8 Trk4 Trunk
trunk F1 Trk5 Trunk
ip default-gateway 192.168.111.10
sntp server 192.168.111.8
ip routing
timesync sntp
sntp unicast
snmp-server community "public" Unrestricted
snmp-server host 192.168.111.22 "public"
vlan 1
   name "DEFAULT_VLAN"
   untagged A2-A7,A9-A16,B2-B7,B9-B16,C2-C7,C9-C16,D2-D7,D9-D16,E1-E16,F
2-F4,Trk1,Trk4-Trk5
   ip address 192.168.111.14 255.255.255.0
   exit
vlan 20
   name "WM_Data1"
   ip address 10.0.20.4 255.255.255.0
   tagged Trk1,Trk4-Trk5
   exit
vlan 30
   name "WM_Data2"
   ip address 10.0.30.4 255.255.255.0
   tagged Trk1,Trk4-Trk5
   exit
vlan 10
   name "WM_VOIP"
   ip address 10.0.10.4 255.255.255.0
   qos priority 6
   ip helper-address 192.168.111.9
   tagged C13,E3,Trk1,Trk4-Trk5
   voice
   exit
ip route 0.0.0.0 0.0.0.0 192.168.111.10
spanning-tree
spanning-tree Trk1 priority 4
spanning-tree Trk4 priority 4
spanning-tree Trk5 priority 4
password manager

; J8773A Configuration Editor; Created on release #L.11.24

hostname "ProCurve Switch 4208vl"
time daylight-time-rule Western-Europe
module 4 type J8764A
module 1 type J8764A
module 2 type J8764A
module 3 type J8764A
module 7 type J9033A
module 8 type J9033A
interface A3
   lacp Passive
exit
trunk G24,H24 Trk2 Trunk
trunk A1,B1,G1,H1 Trk3 Trunk
ip default-gateway 192.168.111.10
sntp server 192.168.111.8
ip routing
timesync sntp
sntp unicast
snmp-server community "public" Unrestricted
snmp-server host 192.168.111.22 "public"
vlan 1
   name "DEFAULT_VLAN"
   untagged A2-A16,B2-B16,C1-C16,D1-D16,G21-G23,H2-H23,Trk2-Trk3
   ip address 192.168.111.15 255.255.255.0
   no untagged G2-G20
   exit
vlan 20
   name "WM_Data1"
   untagged G2-G20
   ip address 10.0.20.5 255.255.255.0
   ip helper-address 192.168.111.9
   tagged Trk2-Trk3
   exit
vlan 30
   name "WM_Data2"
   ip address 10.0.30.5 255.255.255.0
   tagged Trk2-Trk3
   exit
vlan 10
   name "WM_VOIP"
   ip address 10.0.10.5 255.255.255.0
   qos priority 6
   ip helper-address 192.168.111.9
   tagged Trk2-Trk3
   voice
   exit
ip route 0.0.0.0 0.0.0.0 192.168.111.10
spanning-tree
spanning-tree Trk2 priority 4
spanning-tree Trk3 priority 4
password manager

ProCurve 2910al-48G Switch# sh conf

Startup configuration:

; J9147A Configuration Editor; Created on release #W.14.38

hostname "ProCurve 2910al-48G Switch"
module 1 type J9147A
trunk 12,14,26,44 Trk3 Trunk
trunk 11,13,25,43 Trk4 Trunk
ip default-gateway 192.168.111.10
ip routing
vlan 1
   name "DEFAULT_VLAN"
   untagged 1-10,15-24,27-42,45-48,Trk3-Trk4
   ip address 192.168.111.221 255.255.255.0
   exit
vlan 20
   name "WM_Data1"
   ip address 10.0.20.1 255.255.255.0
   tagged Trk3-Trk4
   exit
vlan 30
   name "WM_Data2"
   ip address 10.0.30.1 255.255.255.0
   tagged Trk3-Trk4
   exit
vlan 10
   name "WM_VOIP"
   qos priority 6
   ip helper-address 192.168.111.9
   ip address 10.0.10.1 255.255.255.0
   tagged 2,Trk3-Trk4
   voice
   exit
timesync sntp
ip route 0.0.0.0 0.0.0.0 192.168.111.10
snmp-server community "public" unrestricted
snmp-server host 192.168.111.22 "public"
spanning-tree
spanning-tree Trk3 priority 4
spanning-tree Trk4 priority 4
no autorun
password manager