INIT: Command
"exec /usr/sbin/esmd </dev/null >/dev/null 2>&1"
 failed to execute.  errno = 5 (exec of shell failed)
^[^[rmc
RMC>halt in
½ÿoperator initiated halt
PC = fffffc00002ecb34
>>>halt out
illegal digit for specified radix
>>>mc
RMC>halt out

Returning to COM port
mc: No such command
>>>boot
Initializing...
*** keyboard not plugged in...
512 Meg of system memory
probing hose 0, PCI
probing PCI-to-ISA bridge, bus 1
probing PCI-to-PCI bridge, hose 0 bus 2
bus 0, slot 9 -- ewa -- DE500-BA Network Controller
bus 0, slot 11 -- ewb -- DE500-BA Network Controller
bus 0, slot 13 -- dqa -- Acer Labs M1543C IDE
bus 0, slot 13 -- dqb -- Acer Labs M1543C IDE
bus 2, slot 4 -- eia -- DE602-B*
bus 2, slot 5 -- eib -- DE602-B*
bus 0, slot 17 -- pka -- NCR 53C895
initializing GCT/FRU at 1ff42000
System Temperature is 41 degrees C

AlphaServer DS10 617 MHz Console V6.8-9, Jul 30 2004 09:36:47

CPU 0 booting

(boot dqa0.0.0.13.0 -flags A)
block 0 of dqa0.0.0.13.0 is a valid boot block
reading 19 blocks from dqa0.0.0.13.0
bootstrap code read in
base = 200000, image_start = 0, image_bytes = 2600(9728)
initializing HWRPB at 2000
initializing page table at 1ff2e000
initializing machine state
setting affinity to the primary CPU
jumping to bootstrap code

UNIX boot - Friday January 24, 2003

Loading vmunix ...
Loading at 0xfffffc0000230000

Sizes:
text =  6520512
data =  1132144
bss  =  1731248
Starting at 0xfffffc00002413f0

Loading vmunix symbol table ... [1605528 bytes]
Memory trolling not supported, cpu Major id 11, Minor id 14
Alpha boot: available memory from 0x1750000 to 0x1ff2c000
Compaq Tru64 UNIX V5.1A (Rev. 1885); Sun Nov 11 16:56:04 CET 2007
physical memory = 512.00 megabytes.
available memory = 487.85 megabytes.
using 1913 buffers containing 14.94 megabytes of memory
Firmware revision: 6.8-9
PALcode: UNIX version 1.92-73
AlphaServer DS10 617 MHz
pci0 (primary bus:0) at nexus
isa0 at pci0
gpc0 at isa0
gpc1 not probed
ace0 at isa0
ace1 at isa0
lp0 at isa0
fdi0 at isa0
fd0 at fdi0 unit 0
tu1: DECchip 21143: Revision: 4.1
tu1: auto negotiation capable device
tu1 at pci0 slot 9
tu1: DEC TULIP (10/100) Ethernet Interface, hardware address: 00-0F-20-D7-5E-CC
tu1: auto negotiation off: selecting 100BaseTX (UTP) port: half duplex
tu2: DECchip 21143: Revision: 4.1
tu2: auto negotiation capable device
tu2 at pci0 slot 11
tu2: DEC TULIP (10/100) Ethernet Interface, hardware address: 00-0F-20-D7-5E-CB
tu2: auto negotiation off: selecting 100BaseTX (UTP) port: half duplex
ata0 at pci0 slot 13
ata0: ACER M1543C
scsi0 at ata0 slot 0 rad 0
scsi1 at ata0 slot 1 rad 0
pci1 (primary bus:0 subordinate bus:2) at pci0 slot 14
ee0 at pci1 slot 4
ee0: COMPAQ Intel 82559 (10/100 Mbps) Ethernet Interface
ee0: Driver Rev = V1.0.23, Chip Rev = 8, hardware address: 00-0D-9D-D5-A0-FC
ee1 at pci1 slot 5
ee1: COMPAQ Intel 82559 (10/100 Mbps) Ethernet Interface
ee1: Driver Rev = V1.0.23, Chip Rev = 8, hardware address: 00-0D-9D-D5-A0-FD
itpsa0 at pci0 slot 17
IntraServer ROM Version V2.0 (c)1998
scsi2 at itpsa0 slot 0 rad 0
Created FRU table binary error log packet
kernel console: ace0
dli: configured
NetRAIN configured.
ATM Subsystem configured with 1 restart threads
ATMUNI: configured
ATMSIG: 3.x (module=uni3x) configured
ILMI: 3.x (module=ilmi) configured
ATM IP: configured
ATM LANE: configured.
ATM IFMP: configured
ee0: Autonegotiated, 100 Mbps full duplex
i2c: Server Management Hardware Present
vm_swap_init: swap is set to eager allocation mode
cam_logger: SCSI event packet
cam_logger: hardware_id=46 bus 0 target 0 lun 0 
cdisk_check_sense
 Medium Error at block number: 418160
Hard Error Detected
Hardware ID = 46
Maxtor  6E040L0         NAR6
Active CCB at time of error
CCB request completed with an error
Error, exception, or abnormal condition
MEDIUM ERROR - Nonrecoverable medium error
cam_logger: SCSI event packet
cam_logger: hardware_id=46 bus 0 target 0 lun 0 
cdisk_check_sense
 Medium Error at block number: 418160
Hard Error Detected
Hardware ID = 46
Maxtor  6E040L0         NAR6
Active CCB at time of error
CCB request completed with an error
Error, exception, or abnormal condition
MEDIUM ERROR - Nonrecoverable medium error
cam_logger: SCSI event packet
cam_logger: hardware_id=46 bus 0 target 0 lun 0 
cdisk_check_sense
 Medium Error at block number: 418160
Hard Error Detected
Hardware ID = 46
Maxtor  6E040L0         NAR6
Active CCB at time of error
CCB request completed with an error
Error, exception, or abnormal condition
MEDIUM ERROR - Nonrecoverable medium error
cam_logger: SCSI event packet
cam_logger: hardware_id=46 bus 0 target 0 lun 0 
cdisk_check_sense
 Medium Error at block number: 418160
Hard Error Detected
Hardware ID = 46
Maxtor  6E040L0         NAR6
Active CCB at time of error
CCB request completed with an error
Error, exception, or abnormal condition
MEDIUM ERROR - Nonrecoverable medium error
cam_logger: SCSI event packet
cam_logger: hardware_id=46 bus 0 target 0 lun 0 
cdisk_check_sense
 Medium Error at block number: 418160
Hard Error Detected
Hardware ID = 46
Maxtor  6E040L0         NAR6
Active CCB at time of error
CCB request completed with an error
Error, exception, or abnormal condition
MEDIUM ERROR - Nonrecoverable medium error
cam_logger: SCSI event packet
cam_logger: hardware_id=46 bus 0 target 0 lun 0 
cdisk_check_sense
 Medium Error at block number: 418160
Hard Error Detected
Hardware ID = 46
Maxtor  6E040L0         NAR6
Active CCB at time of error
CCB request completed with an error
Error, exception, or abnormal condition
MEDIUM ERROR - Nonrecoverable medium error
cam_logger: SCSI event packet
cam_logger: hardware_id=46 bus 0 target 0 lun 0 
cdisk_check_sense
 Medium Error at block number: 418160
Hard Error Detected
Hardware ID = 46
Maxtor  6E040L0         NAR6
Active CCB at time of error
CCB request completed with an error
Error, exception, or abnormal condition
MEDIUM ERROR - Nonrecoverable medium error
Checking device naming:
    Passed.
Checking local filesystems
Mounting / (root)
user_cfg_pt: reconfigured
root_mounted_rw: reconfigured
cam_logger: SCSI event packet
cam_logger: hardware_id=46 bus 0 target 0 lun 0 
cdisk_check_sense
 Medium Error at block number: 419472
Hard Error Detected
Hardware ID = 46
Maxtor  6E040L0         NAR6
Active CCB at time of error
CCB request completed with an error
Error, exception, or abnormal condition
MEDIUM ERROR - Nonrecoverable medium error
user_cfg_pt: reconfigured
root_mounted_rw: reconfigured
user_cfg_pt: reconfigured
dsfmgr: NOTE: updating kernel basenames for system at /
    scp kevm tty00 tty01 lp0 dmapi dsk0 dsk1 tape0 floppy0 cdrom0
Mounting local filesystems
exec: /sbin/mount_advfs -F 0x14000 root_domain#root /
root_domain#root on / type advfs (rw)
/proc on /proc type procfs (rw)
exec: /sbin/mount_advfs -F 0x4000 usr_domain#usr /usr
usr_domain#usr on /usr type advfs (rw)
exec: /sbin/mount_advfs -F 0x4000 var_domain#var /var
cam_logger: SCSI event packet
cam_logger: hardware_id=46 bus 0 target 0 lun 0 
cdisk_check_sense
 Medium Error at block number: 7168288
Hard Error Detected
Hardware ID = 46
Maxtor  6E040L0         NAR6
Active CCB at time of error
CCB request completed with an error
Error, exception, or abnormal condition
MEDIUM ERROR - Nonrecoverable medium error
var_domain#var on /var type advfs (rw)
Jun 29 15:57:03 esmd: Essential Services Monitor daemon started
Subsystem hwautoconfig was successfully configured.
Jun 29 15:57:04 update: started

Checking for Installation Tasks...
cam_logger: SCSI event packet
cam_logger: hardware_id=46 bus 0 target 0 lun 0 
cdisk_check_sense
 Medium Error at block number: 2261392
Hard Error Detected
Hardware ID = 46
Maxtor  6E040L0         NAR6
Active CCB at time of error
CCB request completed with an error
Error, exception, or abnormal condition
MEDIUM ERROR - Nonrecoverable medium error
cam_logger: SCSI event packet
cam_logger: hardware_id=46 bus 0 target 0 lun 0 
cdisk_check_sense
 Medium Error at block number: 2261392
Hard Error Detected
Hardware ID = 46
Maxtor  6E040L0         NAR6
Active CCB at time of error
CCB request completed with an error
Error, exception, or abnormal condition
MEDIUM ERROR - Nonrecoverable medium error
cam_logger: SCSI event packet
cam_logger: hardware_id=46 bus 0 target 0 lun 0 
cdisk_check_sense
 Medium Error at block number: 2261392
Hard Error Detected
Hardware ID = 46
Maxtor  6E040L0         NAR6
Active CCB at time of error
CCB request completed with an error
Error, exception, or abnormal condition
MEDIUM ERROR - Nonrecoverable medium error
cam_logger: SCSI event packet
cam_logger: hardware_id=46 bus 0 target 0 lun 0 
cdisk_check_sense
 Medium Error at block number: 2261392
Hard Error Detected
Hardware ID = 46
Maxtor  6E040L0         NAR6
Active CCB at time of error
CCB request completed with an error
Error, exception, or abnormal condition
MEDIUM ERROR - Nonrecoverable medium error
cam_logger: SCSI event packet
cam_logger: hardware_id=46 bus 0 target 0 lun 0 
cdisk_check_sense
 Medium Error at block number: 2261392
Hard Error Detected
Hardware ID = 46
Maxtor  6E040L0         NAR6
Active CCB at time of error
CCB request completed with an error
Error, exception, or abnormal condition
MEDIUM ERROR - Nonrecoverable medium error
cam_logger: SCSI event packet
cam_logger: hardware_id=46 bus 0 target 0 lun 0 
cdisk_check_sense
 Medium Error at block number: 2261392
Hard Error Detected
Hardware ID = 46
Maxtor  6E040L0         NAR6
Active CCB at time of error
CCB request completed with an error
Error, exception, or abnormal condition
MEDIUM ERROR - Nonrecoverable medium error
cam_logger: SCSI event packet
cam_logger: hardware_id=46 bus 0 target 0 lun 0 
cdisk_check_sense
 Medium Error at block number: 2261392
Hard Error Detected
Hardware ID = 46
Maxtor  6E040L0         NAR6
Active CCB at time of error
CCB request completed with an error
Error, exception, or abnormal condition
MEDIUM ERROR - Nonrecoverable medium error
cam_logger: SCSI event packet
cam_logger: hardware_id=46 bus 0 target 0 lun 0 
cdisk_check_sense
 Medium Error at block number: 2261392
Hard Error Detected
Hardware ID = 46
Maxtor  6E040L0         NAR6
Active CCB at time of error
CCB request completed with an error
Error, exception, or abnormal condition
MEDIUM ERROR - Nonrecoverable medium error
cam_logger: SCSI event packet
cam_logger: hardware_id=46 bus 0 target 0 lun 0 
cdisk_check_sense
 Medium Error at block number: 2261392
Hard Error Detected
Hardware ID = 46
Maxtor  6E040L0         NAR6
Active CCB at time of error
CCB request completed with an error
Error, exception, or abnormal condition
MEDIUM ERROR - Nonrecoverable medium error
cam_logger: SCSI event packet
cam_logger: hardware_id=46 bus 0 target 0 lun 0 
cdisk_check_sense
 Medium Error at block number: 2261392
Hard Error Detected
Hardware ID = 46
Maxtor  6E040L0         NAR6
Active CCB at time of error
CCB request completed with an error
Error, exception, or abnormal condition
MEDIUM ERROR - Nonrecoverable medium error
cam_logger: SCSI event packet
cam_logger: hardware_id=46 bus 0 target 0 lun 0 
cdisk_check_sense
 Medium Error at block number: 2261392
Hard Error Detected
Hardware ID = 46
Maxtor  6E040L0         NAR6
Active CCB at time of error
CCB request completed with an error
Error, exception, or abnormal condition
MEDIUM ERROR - Nonrecoverable medium error

Executing Installation Tasks...
The system is coming up. Please wait...
Checking for crash dumps
Initializing paging space
Mounting Memory filesystems
evmstart: Daemon started
Jun 29 15:58:06 esmd: Started monitoring the EVM daemon
File /etc/sia/matrix.conf updated successfully.
Successful SIA initialization

/usr/sbin/autopush: Can't push requested modules on STREAM for entry 36
/usr/sbin/autopush: Device (6,-1) already configured
Streams autopushes configured
/var/nse/arch: No such file or directory
/var/nse/arch not mounted or not properly enabled for quotas in /etc/fstab
/var/adm/data/out/GP_out: No such file or directory
mv: rename /tmp/gp.out to /var/adm/data/out/GP_out: No such file or directory
Configuring network
hostname: STATION_A
Clean-up /var/join directory
Loading LMF licenses
Combine OSF-USR ALS-IL-2000AUG14-1162 with OSF-USR UNIX-SERVER-IMPLICIT-USER
System error logger started
Binary error logger started
Jun 29 15:58:12 STATION_A syslogd: Unknown facility name: "al0"
add net default: gateway 10.168.80.108
Setting kernel timezone variable
Setting the current time and date with ntpdate
Mon Jun 29 15:58:21 GMT+3 2009
Ntpdate succeeded.
Making (r)rz devices ... 
 Done
Mapping root_domain ...Warning: changing optimization to space because minfree is less than 10%
 Done
ONC portmap service started
NFS mount daemon started
NFS export service started
Property list daemon started
NFS IO service started
NFS Locking:
  rpc.statd started
  rpc.lockd started
MAKEDEV: special file(s) for ace0: 

/dev/rrz0a is a link to /devices/rdisk/dsk0a
Mounting NFS filesystems
prpasswdd started
Preserving editor files
Node ID is 00-0d-9d-d5-a0-fc (from device ee0)
dna_netman: configured
Event Logging ... 
dna_dli: configured
Node UID is d5e392b8-64de-11de-a91d-000d9dd5a0fc
dna_base: configured
Routing ... 
Event: Circuit Change
       from: NSP ... Node 0:. Routing Circuit circuit-1 
       at  : 2009-06-29-15:58:30.497-03:00I-----

       New Circuit State                 = On

OSI Transport ... 
ncl>> set osi transport template dep_qb1 network service = CONS

Node 0 OSI Transport Template dep_qb1 
AT 2009-06-29-15:58:30.709-03:00I-----

FAILED IN DIRECTIVE: Set
DUE TO: Could not modify specified attributes

    Network Service                   = CONS

ERROR: Invalid Attribute Value

ncl>> set osi transport template dep_qb1 class = {0}

Node 0 OSI Transport Template dep_qb1 
AT 2009-06-29-15:58:30.711-03:00I-----

FAILED IN DIRECTIVE: Set
DUE TO: Could not modify specified attributes

    Classes                           = { 0 }

ERROR: Invalid Attribute Value

ncl>> set osi transport template dep_qb1 CONS template "OSI transport dep_qb1"

PROCESS ERROR: Connection lost: remote side disconnected link

ncl>> set osi transport CONS NSAP Addresses {/3700000000000456}

PROCESS ERROR: Could not decode entity's response: problem code = 7

ncl>> set osi transport CONS Filters {"OSI Transport dep_qb1"}

PROCESS ERROR: Could not decode entity's response: problem code = 7

Session Control ...
DNS ... waiting for DNS Clerk ...
waiting for DNS Clerk ...
waiting for DNS Clerk ...
waiting for DNS Clerk ...
waiting for DNS Clerk ...
waiting for DNS Clerk ...
waiting for DNS Clerk ...
waiting for DNS Clerk ...
DTSS ... Node Enabled ... Event Logging
Event: Deleted Maintained Object
       from: Node 0:. Session Control 
       at  : 2009-06-29-15:58:48.875-03:00I-----

       Name                              = LOCAL:.MFS_UTL_A
       Last Failure Reason               = 
           [
               Originator = Naming Service ,
               Naming Service = Operation not supported by LOCAL namespace
           ]
       Reason                            = Operation not supported by LOCAL namespace
       Higher Towers                     = 
           {
               (
                   [ DNA_CMIP-MICE ] ,
                   [ DNA_SessionControlV3 , number=19 ]
               )
           }
       Last Successful Update            = <undefined>
       Last Update Completed             = 2009-06-29-15:58:48.837-03:00I-----
       Last Update Started               = 2009-06-29-15:58:48.746-03:00I-----
       UID                               = E0F389EC-64DE-11DE-A91D-000D9DD5A0FC
       Update Failures                   =                    0
       Update Successes                  =                    0
       Creation Time                     = 2009-06-29-15:58:48.727-03:00I-----

dna_xti: configured
Clearing temporary files
Unlocking ptys
Clearing MFS temporary files.
Environmental Monitoring Subsystem Configured.
Using snmp service entry port 161.
Could not bind socket: Invalid argument
Extensible SNMP master agent started
Base O/S subagent started
Server System subagent started
Server Management subagent started
CIM SNMP subagent started
Performance Management subagent started
/sbin/rc3.d/S51envmon ERROR: Extensible SNMP master agent NOT RUNNING, cannot start Server System MIB sub-agent
No Master-agent (snmpd) running, cannot start pmgrd
Environmental Monitoring Daemon started.
Internet services provided.
Cron service started
cron aborted: cannot access fifo queue
Collecting last crash informations in /var/adm/nectar/2009.06.29@15:59:21
Keep the 10 last crash(s)...
Delete directory /var/adm/nectar/2009.06.21@15:08:43
S98nec_cfg: building version MFSSAW60E
Nectar will be launched within 1 minute
Nectar about to be launched
DUMP server started
Alcatel Software Control Platform (NECTAR) started
---------- craft_srv script start --------------------
NECTAR IN SITE MODE: CRAFT_SRV WILL BE LAUNCHED BY CRAFT_SUP...
Sending output to nohup.out
S99tcpstart_http: looking for active station.
TRACE server started
Starting Trace Server ...
The system is ready.

Compaq Tru64 UNIX V5.1A (Rev. 1885) (STATION_A) console

login: root
Password:
Terminal is disabled but root login is allowed.

Last   successful login for root: Sat Jun 27 10:56:53 GMT+3 2009 from Uganda1OMC
Last unsuccessful login for root: Fri Jun 26 14:11:36 GMT+3 2009 from Uganda1OMC

Compaq Tru64 UNIX V5.1A (Rev. 1885); Sun Nov 11 16:56:04 CET 2007

The installation software has successfully installed your system.

There are logfiles that contain a record of your installation.  These are:

        /var/adm/smlogs/install.cdf     - configuration description file
        /var/adm/smlogs/install.log     - general log file
        /var/adm/smlogs/install.FS.log  - file system creation logs
        /var/adm/smlogs/setld.log       - log for the setld(8) utility
        /var/adm/smlogs/fverify.log     - verification log file

****************************************************************
T64V51AB24AS0006-20031031 patches (UNIX V5.1A) installed on 04-17-06 
****************************************************************
****************************************************************
T64KIT0021260-V51AB24-20040113 patches (UNIX V5.1A) installed on 04-17-06 
****************************************************************
You have new mail.

===================================================================================
Unauthorized access to this machine is strictly forbidden and may be liable to legal proceedings

===================================================================================
# ps -ef | grep nectar
root           1442          1  0.0 16:00:44 ??           0:00.02 /usr/nectar/bin/UR_SUA
root           1444       1442  0.0 16:00:44 ??           0:00.01 /usr/nectar/bin/UR_SUA
root           1666       1482  0.0 16:02:52 console      0:00.00 grep nectar
# ps -ef | grep mfs
^[[A^[[Bps: not found
# ps -ef | grep mfs
root            732          1  0.0 15:58:23 ??           0:00.00 mfs -s128 -i65536 -m0 /etc/fdmns/root_domain
root           1434          1  0.0 16:00:42 ??           0:00.01 /usr/mfs/bin/DUMP_SRV
root           1450          1  0.0 16:00:54 ??           0:00.29 /usr/mfs/bin/start_http start
root           1480          1  0.0 16:00:56 ??           0:00.02 /usr/mfs/bin/TRACE_SERVER
root           1800       1482  0.0 16:04:13 console      0:00.00 grep mfs
# ps -edf | grep /usr/mfs/bin
ps: illegal option -- 
s: illegal option -- [
ps: illegal option -- C
Usage: 
ps [-Aedamjflr] [-oO format] [-t tlist] [-p plist] [-u ulist] [-U ulist] [-g glist] [-G glist] [-s slist] [-n nlist]
                -or-
Usage:  For BSD Compatible Syntax
ps [aexgmlvusjrSUALwhT] [Oo format] [ttty] [process number]
# ps -ef | grep /usr/mfs/bin
root           1434          1  0.0 16:00:42 ??           0:00.01 /usr/mfs/bin/DUMP_SRV
root           1450          1  0.1 16:00:54 ??           0:00.75 /usr/mfs/bin/start_http start
root           1480          1  0.0 16:00:56 ??           0:00.02 /usr/mfs/bin/TRACE_SERVER
root           2413       1482  0.0 16:10:37 console      0:00.00 grep /usr/mfs/bin
# ps -ef | grep mfs
root            732          1  0.0 15:58:23 ??           0:00.00 mfs -s128 -i65536 -m0 /etc/fdmns/root_domain
root           1434          1  0.0 16:00:42 ??           0:00.01 /usr/mfs/bin/DUMP_SRV
root           1450          1  0.0 16:00:54 ??           0:00.77 /usr/mfs/bin/start_http start
root           1480          1  0.0 16:00:56 ??           0:00.02 /usr/mfs/bin/TRACE_SERVER
root           2436       1450  0.0 16:10:50 ??           0:00.00 /usr/mfs/bin/start_http start
root           2434       1482  0.0 16:10:50 console      0:00.00 grep mfs
# ERROR: ENVMOND has failed and will exit. It will no longer monitor the system because  
 the svrSystem_mib and or snmpd are not running. A community name usable on the local host must be specified in snmpd.conf. An snmp_request has FAILED with:  No reply.
child process exited abnormally

# ps -ef | grep nectar
^[[A^[[Bps: not found
# ps -ef | grep mfs
root            732          1  0.0 15:58:23 ??           0:00.00 mfs -s128 -i65536 -m0 /etc/fdmns/root_domain
root           1434          1  0.0 16:00:42 ??           0:00.01 /usr/mfs/bin/DUMP_SRV
root           1450          1  0.0 16:00:54 ??           0:01.29 /usr/mfs/bin/start_http start
root           1480          1  0.0 16:00:56 ??           0:00.02 /usr/mfs/bin/TRACE_SERVER
root           3162       1482  0.0 16:18:31 console      0:00.00 grep mfs
#