$ MOUNT/FOR $1$DGA1550:
%MOUNT-I-MOUNTED,  mounted on _$1$DGA1550: (NRCAVA)
$
*INTERRUPT*

$ DISM $1$DGA1550:
$ INIT $1$DGA1550: scratch/LIMIT
%DCL-W-IVQUAL, unrecognized qualifier - check validity, spelling, and placement
 \LIMIT\
$ ANAL/DISK$1$DGA1550:
%DCL-W-NOVALU, value not allowed - remove value specification
 \DISK$1$DGA1550:\
$ ANAL/DISK $1$DGA1550:
%ANALDISK-F-OPENINDEX, error opening INDEXF.SYS, RVN 1
-SYSTEM-F-DEVNOTMOUNT, device is not mounted
$ $ MOUNT/FOR $1$DGA1550:
%MOUNT-I-MOUNTED,  mounted on _$1$DGA1550: (NRCAVA)
$ %MOUNT-I-MOUNTED,  mounted on _$1$DGA1550: (NRCAVA)
%DCL-W-IVVERB, unrecognized command verb - check validity and spelling
 \%MOUNT\
$ MOUNT $1$DGA1550: scratch
%MOUNT-F-DEVMOUNT, device is already mounted
$  SHOW DEVICE/FULL $1$DGA1550:

Disk $1$DGA1550: (NRCAVA), device type HP OPEN-V, is online, allocated,
    deallocate on dismount, mounted foreign, file-oriented device, shareable,
    device has multiple I/O paths, served to cluster via MSCP Server, error
    logging is enabled.

    Error count                    1    Operations completed                 10
    Owner process        "_TNA7886:"    Owner UIC                      [CONRES]
    Owner process ID        20676CA6    Dev Prot            S:RWPL,O:RWPL,G:R,W
    Reference count                2    Default buffer size                 512
    WWID   02000010:
    Total blocks           113890560    Sectors per track                   128
    Total cylinders            59318    Tracks per cylinder                  15
    Allocation class               1

    Volume label                  ""    Relative volume number                0
    Cluster size                   0    Transaction count                     1
    Free blocks                    0    Maximum files allowed                 0
    Extend quantity                0    Mount count                           1
    Mount status             Process    ACP process name                     ""

  Volume Status:  Unknown ACP type.

  I/O paths to device              2
  Path PGA0.5006-0E80-039C-5A04 (NRCAVA), primary path, current path.
    Error count                    1    Operations completed                 10
  Path PGC0.5006-0E80-039C-5A14 (NRCAVA).
    Error count                    0    Operations completed                  0

$
*INTERRUPT*

$ SHOW DEV/MULTI $1$DGA1550
Device                  Device           Error  Paths  Current
 Name                   Status           Count Avl/Tot   path
$1$DGA1550:   (NRCAVA)  Mounted alloc        1   2/ 2  PGA0.5006-0E80-039C-5A04
$