RMC>

RMC>reset

Returning to COM port

 SROM V2.0 CPU # 00 @  0500  MHz
SROM program starting
Reloading SROM

 SROM V2.12-F CPU # 00 @  0833  MHz
SROM program starting
Starting secondary on CPU #1
Starting secondary on CPU #2
Bcache data tests in progress
Bcache address test in progress
CPU parity and ECC detection in progress
Bcache ECC data tests in progress
Bcache TAG lines tests in progress
Memory sizing in progress
Memory configuration in progress
Memory data test in progress
Memory address test in progress
Memory pattern test in progress
Memory thrashing test in progress
Memory initialization
Loading console
Code execution complete (transfer control)

OpenVMS PALcode V1.97-103, Tru64 UNIX PALcode V1.91-104

starting console on CPU 0
initialized idle PCB
initializing semaphores
initializing heap
initial heap 240c0
memory low limit = 1ae000 heap = 240c0, 17fc0
initializing driver structures
initializing idle process PID
initializing file system
initializing hardware
initializing timer data structures
lowering IPL
CPU 0 speed is 833 MHz
create dead_eater
create poll
create timer
create powerup
access NVRAM
Memory size 16384 MB
testing memory
...
probe I/O subsystem
probing hose 1, PCI
bus 0, slot 1 -- pka -- NCR 53C895
bus 0, slot 2 -- pkb -- NCR 53C895
probing hose 0, PCI
probing PCI-to-ISA bridge, bus 1
bus 0, slot 3 -- ewa -- DE500-BA Network Controller
bus 0, slot 15 -- dqa -- Acer Labs M1543C IDE
bus 0, slot 15 -- dqb -- Acer Labs M1543C IDE
starting drivers

*** Error - Fan 3 failed ***

*** Error - Fan 6 failed ***
entering idle loop
starting console on CPU 1
initialized idle PCB
initializing idle process PID
lowering IPL
CPU 1 speed is 833 MHz
create powerup
starting console on CPU 2
initialized idle PCB
initializing idle process PID
lowering IPL
CPU 2 speed is 833 MHz
create powerup
Partition 0, Memory base: 000000000, size: 400000000
initializing GCT/FRU at 1d0000
Initializing pka pkb ewa dqa dqb
Memory Testing and Configuration Status
  Array       Size       Base Address    Intlv Mode
---------  ----------  ----------------  ----------
    1       8192Mb     0000000000000000    1-Way
    3       8192Mb     0000000200000000    1-Way

     16384 MB of System Memory
Testing the System
Testing the Disks (read only)
Testing the Network
AlphaServer ES40 Console V6.4-17, built on Dec 10 2002 at 08:57:31

CPU 0 booting

(boot dka0.0.0.1.1 -flags 0,0)
block 0 of dka0.0.0.1.1 is a valid boot block
reading 1142 blocks from dka0.0.0.1.1
bootstrap code read in
base = 200000, image_start = 0, image_bytes = 8ec00(584704)
initializing HWRPB at 2000
initializing page table at 3ff16000
initializing machine state
setting affinity to the primary CPU
jumping to bootstrap code

%SYSBOOT-W-FIRMREV, Firmware rev. 6.4 is below the recommended minimum of 6.5.
                   Please update your firmware to the recommended revision,
                   which can be found on the firmware CD labeled:
                   alpha systems firmware update 6.5.

    OpenVMS (TM) Alpha Operating System, Version V7.3-2
    © Copyright 1976-2003 Hewlett-Packard Development Company, L.P.

halted CPU 0

halt code = 1
operator initiated halt
PC = ffffffff84920000
P00>>>sh dfev d
P00>>>sh dev d
dka0.0.0.1.1               DKA0              COMPAQ BD036635C5  B017
dka100.1.0.1.1             DKA100            COMPAQ BF0368A4CA  HPB5
dka300.3.0.1.1             DKA300            COMPAQ BD036635C5  B017
dka400.4.0.1.1             DKA400            COMPAQ BD03685A24  HPB4
dkb0.0.0.2.1               DKB0              COMPAQ BD0366349C  3B06
dkb100.1.0.2.1             DKB100            COMPAQ BD036635C5  B017
dkb200.2.0.2.1             DKB200            COMPAQ BD018635C4  B017
dkb300.3.0.2.1             DKB300            COMPAQ BD036635C5  B017
dkb400.4.0.2.1             DKB400            COMPAQ BD0366349C  3B06
dkb500.5.0.2.1             DKB500            COMPAQ BD03685A24  HPB4
dqa0.0.0.15.0              DQA0             Compaq   CRD-8402B  1.03
dva0.0.0.1000.0            DVA0
P00>>>b -flags 0,1
(boot dka0.0.0.1.1 -flags 0,1)
block 0 of dka0.0.0.1.1 is a valid boot block
reading 1142 blocks from dka0.0.0.1.1
bootstrap code read in
base = 200000, image_start = 0, image_bytes = 8ec00(584704)
initializing HWRPB at 2000
initializing page table at 3ff16000
initializing machine state
setting affinity to the primary CPU
jumping to bootstrap code

SYSBOOT> SHOW /STARTUP
  Startup command file = SYS$SYSTEM:STARTUP.COM

SYSBOOT> SET STARTUP_P2 "CCC"

SYSBOOT> continue

%SYSBOOT-W-FIRMREV, Firmware rev. 6.4 is below the recommended minimum of 6.5.
                   Please update your firmware to the recommended revision,
                   which can be found on the firmware CD labeled:
                   alpha systems firmware update 6.5.

    OpenVMS (TM) Alpha Operating System, Version V7.3-2
    © Copyright 1976-2003 Hewlett-Packard Development Company, L.P.

%DECnet-I-LOADED, network base image loaded, version = 05.10.00

%PKA0, Copyright (c) 1998 IntraServer Technology Inc. PKW V2.1.22 ROM V2.0
%PKA0, SCSI Chip is SYM53C895, Operating mode is LVD Ultra2 SCSI
%SMP-I-SECMSG, CPU #01 message:   P01>>>START
%SMP-I-SECMSG, CPU #02 message:   P02>>>START
%SMP-I-CPUTRN, CPU #01 has joined the active set.
%SMP-I-CPUTRN, CPU #02 has joined the active set.
%SYSINIT-I- waiting to form or join an OpenVMS Cluster
%VMScluster-I-LOADSECDB, loading the cluster security database
%EWA0, FastFD mode set by console
%EWA0, Link state: UP
%PKB0, Copyright (c) 1998 IntraServer Technology Inc. PKW V2.1.22 ROM V2.0
%PKB0, SCSI Chip is SYM53C895, Operating mode is LVD Ultra2 SCSI
%MSCPLOAD-I-CONFIGSCAN, enabled automatic disk serving
%CNXMAN,  Sending VMScluster membership request to system DONALD
%CNXMAN,  Now a VMScluster member -- system ALXNDR
%SYSINIT-I- Dumps written to PAGEFILE.SYS will be lost; set parameter SAVEDUMP
%STDRV-I-STARTUP, OpenVMS startup begun at  5-AUG-2010 00:19:51.91
%STDRV-I-OPENCOMP, opening component file 0, STARTUP$STARTUP_VMS
%STDRV-I-OPENCOMP, opening component file 1, STARTUP$STARTUP_LAYERED

%STDRV-I-STRTPHAS, starting phase INITIAL at  5-AUG-2010 00:19:52.38
%STDRV-I-INDXFILE, using component file 0
%STDRV-I-DIRECT, @SYS$STARTUP:VMS$INITIAL-050_VMS.COM
%RMS-E-FNF, file not found
%SMG-F-INVKBD_ID, invalid keyboard-id
%STDRV-I-DIRECT, @SYS$STARTUP:VMS$INITIAL-050_LIB.COM
%STDRV-I-CALLED, ignoring VMS$INITIAL-050_CONFIGURE.COM
%STDRV-I-DIRECT, @SYS$STARTUP:VMS$CONFIG-050_CSP.COM
%STDRV-I-DIRECT, @SYS$STARTUP:VMS$CONFIG-050_SHADOW_SERVER.COM
%STDRV-I-INDXFILE, using component file 1
%STDRV-I-EMTYPHAS, phase INITIAL has no entries in file 1.

%STDRV-I-STRTPHAS, starting phase DEVICES at  5-AUG-2010 00:19:54.78
%STDRV-I-INDXFILE, using component file 0
%STDRV-I-DIRECT, @SYS$STARTUP:VMS$DEVICE_STARTUP.COM
%DCL-W-ACTIMAGE, error activating image SECURESHRP
-CLI-E-IMGNAME, image file ALXNDR$DKA0:[SYS0.SYSCOMMON.][SYSLIB]SECURESHRP.EXE;1
-SYSTEM-F-PROTINSTALL, protected images must be installed
%DCL-W-IVVERB, unrecognized command verb - check validity and spelling
 \IO\
%DCL-W-IVVERB, unrecognized command verb - check validity and spelling
 \IO\
%DCL-W-IVVERB, unrecognized command verb - check validity and spelling
 \IO\
%STDRV-I-INDXFILE, using component file 1
%STDRV-I-EMTYPHAS, phase DEVICES has no entries in file 1.

%STDRV-I-STRTPHAS, starting phase PRECONFIG at  5-AUG-2010 00:19:55.81
%STDRV-I-INDXFILE, using component file 0
%STDRV-I-DIRECT, @SYS$STARTUP:IPC$STARTUP.COM
%STDRV-I-INDXFILE, using component file 1
%STDRV-I-EMTYPHAS, phase PRECONFIG has no entries in file 1.

%STDRV-I-STRTPHAS, starting phase CONFIG at  5-AUG-2010 00:19:57.51
%STDRV-I-INDXFILE, using component file 0
%STDRV-I-DIRECT, @SYS$STARTUP:VMS$CONFIG-050_VMS.COM
%STDRV-I-DIRECT, @SYS$STARTUP:VMS$CONFIG-050_ERRFMT.COM
%STDRV-I-DIRECT, @SYS$STARTUP:VMS$CONFIG-050_CACHE_SERVER.COM
%STDRV-I-DIRECT, @SYS$STARTUP:VMS$CONFIG-050_OPCOM.COM
%STDRV-I-DIRECT, @SYS$STARTUP:VMS$CONFIG-050_AUDIT_SERVER.COM
%%%%%%%%%%%  OPCOM   5-AUG-2010 00:19:58.21  %%%%%%%%%%%
Operator _ALXNDR$OPA0: has been enabled, username SYSTEM

%%%%%%%%%%%  OPCOM   5-AUG-2010 00:19:58.23  %%%%%%%%%%%
Operator status for operator _ALXNDR$OPA0:
CENTRAL, PRINTER, TAPES, DISKS, DEVICES, CARDS, NETWORK, CLUSTER, SECURITY,
LICENSE, OPER1, OPER2, OPER3, OPER4, OPER5, OPER6, OPER7, OPER8, OPER9, OPER10,
OPER11, OPER12

%SET-I-NEWAUDSRV, identification of new audit server process is 20C0040C
%%%%%%%%%%%  OPCOM   5-AUG-2010 00:19:58.63  %%%%%%%%%%%
Logfile has been initialized by operator _ALXNDR$OPA0:
Logfile is ALXNDR::SYS$SYSROOT:[SYSMGR]OPERATOR.LOG;154

%STDRV-I-DIRECT, @SYS$STARTUP:VMS$CONFIG-050_JOBCTL.COM
%%%%%%%%%%%  OPCOM   5-AUG-2010 00:19:58.63  %%%%%%%%%%%
Operator status for operator ALXNDR::SYS$SYSROOT:[SYSMGR]OPERATOR.LOG;154
CENTRAL, PRINTER, TAPES, DISKS, DEVICES, CARDS, NETWORK, CLUSTER, SECURITY,
LICENSE, OPER1, OPER2, OPER3, OPER4, OPER5, OPER6, OPER7, OPER8, OPER9, OPER10,
OPER11, OPER12

%STDRV-I-DIRECT, @SYS$STARTUP:VMS$CONFIG-050_LMF.COM
%%%%%%%%%%%  OPCOM   5-AUG-2010 00:19:58.63  %%%%%%%%%%%
Message from user WBM$SERVER
%WBM-I-WBMINFO Write Bitmap has successfully completed initialization.

%%%%%%%%%%%  OPCOM   5-AUG-2010 00:19:58.63  %%%%%%%%%%%
00:19:40.33 Node ALXNDR (csid 00010006) is now a VMScluster member

%RUN-S-PROC_ID, identification of created process is 20C0040F
%STDRV-I-DIRECT, @SYS$STARTUP:VMS$CONFIG-050_SECURITY_SERVER.COM
%DCL-W-ACTIMAGE, error activating image SECURESHRP
-CLI-E-IMGNAME, image file ALXNDR$DKA0:[SYS0.SYSCOMMON.][SYSLIB]SECURESHRP.EXE;1
-SYSTEM-F-PROTINSTALL, protected images must be installed
%STDRV-I-DIRECT, @SYS$STARTUP:VMS$CONFIG-050_ACME_SERVER.COM
%DCL-W-ACTIMAGE, error activating image SECURESHRP
-CLI-E-IMGNAME, image file ALXNDR$DKA0:[SYS0.SYSCOMMON.][SYSLIB]SECURESHRP.EXE;1
-SYSTEM-F-PROTINSTALL, protected images must be installed
  SYSTEM       job terminated at  5-AUG-2010 00:20:01.89

  Accounting information:
  Buffered I/O count:               1200      Peak working set size:       6320
  Direct I/O count:                  691      Peak virtual size:         180368
  Page faults:                      1494      Mounted volumes:                0
  Charged CPU time:        0 00:00:00.75      Elapsed time:       0 00:00:10.31