script start "GbE2c Ethernet Blade Switch for HP c-Class BladeSystem" 5 /**** DO NOT EDIT THIS LINE!
/* Configuration dump taken 0:27:08 Thu Feb 2, 2006
/* Version 5.1.3, Base MAC address xx:xx:xx:xx:xx:xx
/* RackId: Default RUID, RackName: myrack
/* Enclosure: XXXXXXXXXX, EnclosureName: XX-XXXXXXXXXXXX
/* Slot: 1
/c/sys
        bootp dis
        dhcp dis
/c/sys/access
        userbbi ena
/c/port 1
        tag ena
        tagpvid dis
/c/port 2
        tag ena
        tagpvid dis
/c/port 3
        tag ena
        tagpvid dis
/c/port 4
        tag ena
        tagpvid dis
/c/port 5
        tag ena
        tagpvid dis
/c/port 6
        tag ena
        tagpvid dis
/c/port 7
        tag ena
        tagpvid dis
/c/port 8
        tag ena
        tagpvid dis
/c/port 9
        tag ena
        tagpvid dis
/c/port 10
        tag ena
        tagpvid dis
/c/port 11
        tag ena
        tagpvid dis
/c/port 12
        tag ena
        tagpvid dis
/c/port 13
        tag ena
        tagpvid dis
/c/port 14
        tag ena
        tagpvid dis
/c/port 15
        tag ena
        tagpvid dis
/c/port 16
        tag ena
        tagpvid dis
/c/port 21
        tag ena
        pvid 4091
/c/port 22
        tag ena
        pvid 4091
/c/port 23
        tag ena
        pvid 4091
/c/port 24
        tag ena
        pvid 4091
/c/l2/vlan 1
        def 1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18 20
/c/l2/vlan 4091
        ena
        name "VLAN_NORM"
        def 10 21 22 23 24
/c/l2/vlan 4093
        ena
        name "VLAN_STD"
        def 1 3 4 5 6 7 8 11 12 13 14 15 16 21 22 23 24
/c/l2/vlan 4095
        def 19
/c/l2/mrst/on
/c/l2/mrst/mode mstp
/c/l2/mrst/name "default"
/c/l2/mrst/cist/add 1 4091 4093 4095
/c/l2/mrst/cist/port 1/on 
/c/l2/mrst/cist/port 2/on 
/c/l2/mrst/cist/port 3/on 
/c/l2/mrst/cist/port 4/on 
/c/l2/mrst/cist/port 5/on 
/c/l2/mrst/cist/port 6/on 
/c/l2/mrst/cist/port 7/on 
/c/l2/mrst/cist/port 8/on 
/c/l2/mrst/cist/port 9/on 
/c/l2/mrst/cist/port 10/on 
/c/l2/mrst/cist/port 11/on 
/c/l2/mrst/cist/port 12/on 
/c/l2/mrst/cist/port 13/on 
/c/l2/mrst/cist/port 14/on 
/c/l2/mrst/cist/port 15/on 
/c/l2/mrst/cist/port 16/on 
/c/l2/stp 1/port 5/on 
/c/l2/stp 1/port 6/on 
/c/l2/stp 1/port 7/on 
/c/l2/stp 1/port 8/on 
/c/l2/stp 1/port 9/on 
/c/l2/stp 1/port 10/on 
/c/l2/stp 1/port 11/on 
/c/l2/stp 1/port 12/on 
/c/l2/stp 1/port 13/on 
/c/l2/stp 1/port 14/on 
/c/l2/stp 1/port 15/on 
/c/l2/stp 1/port 16/on 
/c/l2/stp 1/port 20/off
/c/l2/stp 1/port 22/off
/c/l2/stp 1/port 24/off
/c/l2/trunk 2
        add 21
        add 22
/c/l2/trunk 3
        add 23
        add 24
/c/l2/lacp
        timeout short
/c/l2/lacp/port 21
        mode active
        adminkey 50
/c/l2/lacp/port 22
        mode active
        adminkey 50
/c/l2/lacp/port 23
        mode active
        adminkey 100
/c/l2/lacp/port 24
        mode active
        adminkey 100
/c/l3/if 1
        ena
        addr 10.127.255.24
        mask 255.255.255.0
        broad 10.127.255.255
/c/l3/if 2
        ena
        addr 192.168.1.24
        vlan 4091
/c/rmon/event 1
/
script end /**** DO NOT EDIT THIS LINE!