
=================================================
  ===============display clock===============
=================================================
14:36:47 UTC Thu 04/27/2000
===================================================
  ===============display version===============
===================================================
3Com Corporation
3Com Baseline Switch 2952-SFP Plus Software Version 5.20 Release 1101P10
Copyright (c) 2004-2010 3Com Corp. and its licensors. All rights reserved.
3Com Baseline Switch 2952-SFP Plus uptime is 0 week, 1 day, 2 hours, 36 minutes

3Com Baseline Switch 2952-SFP Plus
128M    bytes DRAM
128M    bytes Nand Flash Memory
Config Register points to Nand Flash

Hardware Version is REV.B
CPLD Version is 002
Bootrom Version is 119
[SubSlot 0] 48GE+4SFP Hardware Version is REV.B

==================================================
  ===============display device===============
==================================================
SubSNo PortNum PCBVer  FPGAVer CPLDVer BootRomVer AddrLM Type       State
0      52      Ver.B   NULL    002     119        IVL    LS51LTSS   Normal
=================================================================
  ===============display current-configuration===============
=================================================================
#
 version 5.20 Release 1101P10
#
 sysname 3Com Baseline Switch
#
 domain default enable system
#
 ip ttl-expires enable
#
vlan 1
#
domain system
 access-limit disable
 state active
 idle-cut disable
 self-service-url disable
#
user-group system
#
local-user admin
 authorization-attribute level 3
 service-type ssh telnet terminal
#
 stp mode rstp
 stp enable
#
interface Bridge-Aggregation1
 link-aggregation mode dynamic
#
interface Bridge-Aggregation2
 link-aggregation mode dynamic
#
interface NULL0
#
interface Vlan-interface1
 ip address 192.168.250.10 255.255.255.0
#
interface GigabitEthernet1/0/1
 stp edged-port enable
 port link-aggregation group 1
#
interface GigabitEthernet1/0/2
 stp edged-port enable
 port link-aggregation group 1
#
interface GigabitEthernet1/0/3
 stp edged-port enable
 port link-aggregation group 2
#
interface GigabitEthernet1/0/4
 stp edged-port enable
 port link-aggregation group 2
#
interface GigabitEthernet1/0/5
 stp edged-port enable
#
interface GigabitEthernet1/0/6
 stp edged-port enable
#
interface GigabitEthernet1/0/7
 stp edged-port enable
#
interface GigabitEthernet1/0/8
 stp edged-port enable
#
interface GigabitEthernet1/0/9
 stp edged-port enable
#
interface GigabitEthernet1/0/10
 stp edged-port enable
#
interface GigabitEthernet1/0/11
 stp edged-port enable
#
interface GigabitEthernet1/0/12
 stp edged-port enable
#
interface GigabitEthernet1/0/13
 stp edged-port enable
#
interface GigabitEthernet1/0/14
 stp edged-port enable
#
interface GigabitEthernet1/0/15
 stp edged-port enable
 lacp port-priority 5
#
interface GigabitEthernet1/0/16
 stp edged-port enable
 lacp port-priority 5
#
interface GigabitEthernet1/0/17
 stp edged-port enable
#
interface GigabitEthernet1/0/18
 stp edged-port enable
#
interface GigabitEthernet1/0/19
 stp edged-port enable
#
interface GigabitEthernet1/0/20
 stp edged-port enable
#
interface GigabitEthernet1/0/21
 stp edged-port enable
#
interface GigabitEthernet1/0/22
 stp edged-port enable
#
interface GigabitEthernet1/0/23
 stp edged-port enable
#
interface GigabitEthernet1/0/24
 stp edged-port enable
#
interface GigabitEthernet1/0/25
 stp edged-port enable
#
interface GigabitEthernet1/0/26
 stp edged-port enable
#
interface GigabitEthernet1/0/27
 stp edged-port enable
#
interface GigabitEthernet1/0/28
 stp edged-port enable
#
interface GigabitEthernet1/0/29
 stp edged-port enable
#
interface GigabitEthernet1/0/30
 stp edged-port enable
#
interface GigabitEthernet1/0/31
 stp edged-port enable
#
interface GigabitEthernet1/0/32
 stp edged-port enable
#
interface GigabitEthernet1/0/33
 stp edged-port enable
#
interface GigabitEthernet1/0/34
 stp edged-port enable
#
interface GigabitEthernet1/0/35
 stp edged-port enable
#
interface GigabitEthernet1/0/36
 stp edged-port enable
#
interface GigabitEthernet1/0/37
 stp edged-port enable
#
interface GigabitEthernet1/0/38
 stp edged-port enable
#
interface GigabitEthernet1/0/39
 stp edged-port enable
#
interface GigabitEthernet1/0/40
 stp edged-port enable
#
interface GigabitEthernet1/0/41
 stp edged-port enable
#
interface GigabitEthernet1/0/42
 stp edged-port enable
#
interface GigabitEthernet1/0/43
 stp edged-port enable
#
interface GigabitEthernet1/0/44
 stp edged-port enable
#
interface GigabitEthernet1/0/45
 stp edged-port enable
#
interface GigabitEthernet1/0/46
 stp edged-port enable
#
interface GigabitEthernet1/0/47
 stp edged-port enable
#
interface GigabitEthernet1/0/48
 stp edged-port enable
#
interface GigabitEthernet1/0/49
 stp edged-port enable
#
interface GigabitEthernet1/0/50
 stp edged-port enable
#
interface GigabitEthernet1/0/51
 stp edged-port enable
#
interface GigabitEthernet1/0/52
 stp edged-port enable
#
 snmp-agent
 snmp-agent local-engineid 8000002B0320FDF124480F
 snmp-agent community read public
 snmp-agent community write private
 snmp-agent sys-info version all
#
 ntp-service source-interface Vlan-interface1
#
 load xml-configuration
#
user-interface aux 0
 authentication-mode scheme
user-interface vty 0 15
 authentication-mode scheme
#
return
===============================================================
  ===============display saved-configuration===============
===============================================================
#
 version 5.20 Release 1101P10
#
 sysname 3Com Baseline Switch
#
 domain default enable system 
#
 ip ttl-expires enable
#
vlan 1
#
domain system 
 access-limit disable 
 state active 
 idle-cut disable 
 self-service-url disable 
#
user-group system
#
local-user admin
 authorization-attribute level 3
 service-type ssh telnet terminal
#
 stp mode rstp
 stp enable
#
interface Bridge-Aggregation1
 link-aggregation mode dynamic
#
interface Bridge-Aggregation2
 link-aggregation mode dynamic
#
interface NULL0
#
interface Vlan-interface1
 ip address dhcp-alloc
#
interface GigabitEthernet1/0/1
 stp edged-port enable
 lacp port-priority 1
 port link-aggregation group 1
#
interface GigabitEthernet1/0/2
 stp edged-port enable
 lacp port-priority 1
 port link-aggregation group 1
#
interface GigabitEthernet1/0/3
 stp edged-port enable
 lacp port-priority 2
 port link-aggregation group 2
#
interface GigabitEthernet1/0/4
 stp edged-port enable
 lacp port-priority 2
 port link-aggregation group 2
#
interface GigabitEthernet1/0/5
 stp edged-port enable
#
interface GigabitEthernet1/0/6
 stp edged-port enable
#
interface GigabitEthernet1/0/7
 stp edged-port enable
#
interface GigabitEthernet1/0/8
 stp edged-port enable
#
interface GigabitEthernet1/0/9
 stp edged-port enable
#
interface GigabitEthernet1/0/10
 stp edged-port enable
#
interface GigabitEthernet1/0/11
 stp edged-port enable
#
interface GigabitEthernet1/0/12
 stp edged-port enable
#
interface GigabitEthernet1/0/13
 stp edged-port enable
#
interface GigabitEthernet1/0/14
 stp edged-port enable
#
interface GigabitEthernet1/0/15
 stp edged-port enable
 lacp port-priority 5
#
interface GigabitEthernet1/0/16
 stp edged-port enable
 lacp port-priority 5
#
interface GigabitEthernet1/0/17
 stp edged-port enable
#
interface GigabitEthernet1/0/18
 stp edged-port enable
#
interface GigabitEthernet1/0/19
 stp edged-port enable
#
interface GigabitEthernet1/0/20
 stp edged-port enable
#
interface GigabitEthernet1/0/21
 stp edged-port enable
#
interface GigabitEthernet1/0/22
 stp edged-port enable
#
interface GigabitEthernet1/0/23
 stp edged-port enable
#
interface GigabitEthernet1/0/24
 stp edged-port enable
#
interface GigabitEthernet1/0/25
 stp edged-port enable
#
interface GigabitEthernet1/0/26
 stp edged-port enable
#
interface GigabitEthernet1/0/27
 stp edged-port enable
#
interface GigabitEthernet1/0/28
 stp edged-port enable
#
interface GigabitEthernet1/0/29
 stp edged-port enable
#
interface GigabitEthernet1/0/30
 stp edged-port enable
#
interface GigabitEthernet1/0/31
 stp edged-port enable
#
interface GigabitEthernet1/0/32
 stp edged-port enable
#
interface GigabitEthernet1/0/33
 stp edged-port enable
#
interface GigabitEthernet1/0/34
 stp edged-port enable
#
interface GigabitEthernet1/0/35
 stp edged-port enable
#
interface GigabitEthernet1/0/36
 stp edged-port enable
#
interface GigabitEthernet1/0/37
 stp edged-port enable
#
interface GigabitEthernet1/0/38
 stp edged-port enable
#
interface GigabitEthernet1/0/39
 stp edged-port enable
#
interface GigabitEthernet1/0/40
 stp edged-port enable
#
interface GigabitEthernet1/0/41
 stp edged-port enable
#
interface GigabitEthernet1/0/42
 stp edged-port enable
#
interface GigabitEthernet1/0/43
 stp edged-port enable
#
interface GigabitEthernet1/0/44
 stp edged-port enable
#
interface GigabitEthernet1/0/45
 stp edged-port enable
#
interface GigabitEthernet1/0/46
 stp edged-port enable
#
interface GigabitEthernet1/0/47
 stp edged-port enable
#
interface GigabitEthernet1/0/48
 stp edged-port enable
#
interface GigabitEthernet1/0/49
 stp edged-port enable
#
interface GigabitEthernet1/0/50
 stp edged-port enable
#
interface GigabitEthernet1/0/51
 stp edged-port enable
#
interface GigabitEthernet1/0/52
 stp edged-port enable
#
 snmp-agent
 snmp-agent local-engineid 8000002B0320FDF124480F
 snmp-agent community read public 
 snmp-agent community write private 
 snmp-agent sys-info version all
#
 ntp-service source-interface Vlan-interface1
#
 load xml-configuration 
#
user-interface aux 0
 authentication-mode scheme
user-interface vty 0 15
 authentication-mode scheme
#
return
=====================================================
  ===============display interface===============
=====================================================
 Bridge-Aggregation1 current state: UP
 IP Packet Frame Type: PKTFMT_ETHNT_2, Hardware Address: 20fd-f124-480f
 Description: Bridge-Aggregation1 Interface
 2Gbps-speed mode, full-duplex mode
 Link speed type is autonegotiation, link duplex type is autonegotiation
 PVID: 1
 Port link-type: access
  Tagged   VLAN ID : none
  Untagged VLAN ID : 1
Last clearing of counters:  13:46:10 Thu 04/27/2000 

 Bridge-Aggregation2 current state: UP
 IP Packet Frame Type: PKTFMT_ETHNT_2, Hardware Address: 20fd-f124-4811
 Description: Bridge-Aggregation2 Interface
 2Gbps-speed mode, full-duplex mode
 Link speed type is autonegotiation, link duplex type is autonegotiation
 PVID: 1
 Port link-type: access
  Tagged   VLAN ID : none
  Untagged VLAN ID : 1
Last clearing of counters:  13:46:10 Thu 04/27/2000 

 GigabitEthernet1/0/1 current state: UP
 IP Packet Frame Type: PKTFMT_ETHNT_2, Hardware Address: 20fd-f124-480f
 Description: GigabitEthernet1/0/1 Interface
 Loopback is not set
 Media type is twisted pair, Port hardware type is 1000_BASE_T
 1000Mbps-speed mode, full-duplex mode
 Link speed type is autonegotiation, link duplex type is autonegotiation
 Flow-control is not enabled
 The Maximum Frame Length is 10240
 Broadcast MAX-ratio: 100%
 Unicast MAX-ratio: 100%
 Multicast MAX-ratio: 100%
 PVID: 1
 Mdi type: auto
 Port link-type: access
  Tagged   VLAN ID : none
  Untagged VLAN ID : 1
 Port priority: 0
 Peak value of input: 6077217 bytes/sec, at 2000-04-27 14:32:57 
 Peak value of output: 2499 bytes/sec, at 2000-04-27 13:50:57 
 Last 300 seconds input:  2906 packets/sec 4407357 bytes/sec 	4%
 Last 300 seconds output:  3 packets/sec 1217 bytes/sec 	0%
 Input (total):  2043319 packets, 3097416869 bytes
	 2042757 unicasts, 0 broadcasts, 562 multicasts
 Input (normal):  2043319 packets, 3097416869 bytes
	 2042757 unicasts, 0 broadcasts, 562 multicasts
 Input:  0 input errors, 0 runts, 0 giants, 0 throttles
	 0 CRC, 0 frame, 0 overruns, 0 aborts
	 0 ignored, 0 parity errors
 Output (total): 3679 packets, 1559732 bytes
	 1901 unicasts, 3 broadcasts, 1775 multicasts, 0 pauses
 Output (normal): 3679 packets, 1559732 bytes
	 1901 unicasts, 3 broadcasts, 1775 multicasts, 0 pauses
 Output: 0 output errors, 0 underruns, 0 buffer failures
	 0 aborts, 0 deferred, 0 collisions, 0 late collisions
	 0 lost carrier, 0 no carrier

 GigabitEthernet1/0/2 current state: UP
 IP Packet Frame Type: PKTFMT_ETHNT_2, Hardware Address: 20fd-f124-4810
 Description: GigabitEthernet1/0/2 Interface
 Loopback is not set
 Media type is twisted pair, Port hardware type is 1000_BASE_T
 1000Mbps-speed mode, full-duplex mode
 Link speed type is autonegotiation, link duplex type is autonegotiation
 Flow-control is not enabled
 The Maximum Frame Length is 10240
 Broadcast MAX-ratio: 100%
 Unicast MAX-ratio: 100%
 Multicast MAX-ratio: 100%
 PVID: 1
 Mdi type: auto
 Port link-type: access
  Tagged   VLAN ID : none
  Untagged VLAN ID : 1
 Port priority: 0
 Peak value of input: 433456 bytes/sec, at 2000-04-27 14:33:47 
 Peak value of output: 18526740 bytes/sec, at 2000-04-27 14:34:12 
 Last 300 seconds input:  3585 packets/sec 246962 bytes/sec 	0%
 Last 300 seconds output:  8453 packets/sec 10591542 bytes/sec 	9%
 Input (total):  2471682 packets, 170237699 bytes
	 2468861 unicasts, 181 broadcasts, 581 multicasts
 Input (normal):  2469623 packets, 170105923 bytes
	 2468861 unicasts, 181 broadcasts, 581 multicasts
 Input:  0 input errors, 0 runts, 0 giants, 0 throttles
	 0 CRC, 0 frame, 0 overruns, 0 aborts
	 0 ignored, 0 parity errors
 Output (total): 5847736 packets, 7300736509 bytes
	 5846383 unicasts, 480 broadcasts, 873 multicasts, 0 pauses
 Output (normal): 5847736 packets, 7300736509 bytes
	 5846383 unicasts, 480 broadcasts, 873 multicasts, 0 pauses
 Output: 0 output errors, 0 underruns, 0 buffer failures
	 0 aborts, 0 deferred, 0 collisions, 0 late collisions
	 0 lost carrier, 0 no carrier

 GigabitEthernet1/0/3 current state: UP
 IP Packet Frame Type: PKTFMT_ETHNT_2, Hardware Address: 20fd-f124-4811
 Description: GigabitEthernet1/0/3 Interface
 Loopback is not set
 Media type is twisted pair, Port hardware type is 1000_BASE_T
 1000Mbps-speed mode, full-duplex mode
 Link speed type is autonegotiation, link duplex type is autonegotiation
 Flow-control is not enabled
 The Maximum Frame Length is 10240
 Broadcast MAX-ratio: 100%
 Unicast MAX-ratio: 100%
 Multicast MAX-ratio: 100%
 PVID: 1
 Mdi type: auto
 Port link-type: access
  Tagged   VLAN ID : none
  Untagged VLAN ID : 1
 Port priority: 0
 Peak value of input: 18429058 bytes/sec, at 2000-04-27 14:34:12 
 Peak value of output: 338 bytes/sec, at 2000-04-27 14:19:37 
 Last 300 seconds input:  6972 packets/sec 10494223 bytes/sec 	9%
 Last 300 seconds output:  0 packets/sec 55 bytes/sec 	0%
 Input (total):  4805311 packets, 7231535598 bytes
	 4804669 unicasts, 28 broadcasts, 614 multicasts
 Input (normal):  4805311 packets, 7231535598 bytes
	 4804669 unicasts, 28 broadcasts, 614 multicasts
 Input:  0 input errors, 0 runts, 0 giants, 0 throttles
	 0 CRC, 0 frame, 0 overruns, 0 aborts
	 0 ignored, 0 parity errors
 Output (total): 2643 packets, 283155 bytes
	 260 unicasts, 74 broadcasts, 2309 multicasts, 0 pauses
 Output (normal): 2643 packets, 283155 bytes
	 260 unicasts, 74 broadcasts, 2309 multicasts, 0 pauses
 Output: 0 output errors, 0 underruns, 0 buffer failures
	 0 aborts, 0 deferred, 0 collisions, 0 late collisions
	 0 lost carrier, 0 no carrier

 GigabitEthernet1/0/4 current state: UP
 IP Packet Frame Type: PKTFMT_ETHNT_2, Hardware Address: 20fd-f124-4812
 Description: GigabitEthernet1/0/4 Interface
 Loopback is not set
 Media type is twisted pair, Port hardware type is 1000_BASE_T
 1000Mbps-speed mode, full-duplex mode
 Link speed type is autonegotiation, link duplex type is autonegotiation
 Flow-control is not enabled
 The Maximum Frame Length is 10240
 Broadcast MAX-ratio: 100%
 Unicast MAX-ratio: 100%
 Multicast MAX-ratio: 100%
 PVID: 1
 Mdi type: auto
 Port link-type: access
  Tagged   VLAN ID : none
  Untagged VLAN ID : 1
 Port priority: 0
 Peak value of input: 134694 bytes/sec, at 2000-04-27 14:32:57 
 Peak value of output: 6406421 bytes/sec, at 2000-04-27 14:32:37 
 Last 300 seconds input:  1481 packets/sec 97429 bytes/sec 	0%
 Last 300 seconds output:  6489 packets/sec 4653902 bytes/sec 	4%
 Input (total):  1042912 packets, 69277130 bytes
	 1041892 unicasts, 512 broadcasts, 508 multicasts
 Input (normal):  1042912 packets, 69277130 bytes
	 1041892 unicasts, 512 broadcasts, 508 multicasts
 Input:  0 input errors, 0 runts, 0 giants, 0 throttles
	 0 CRC, 0 frame, 0 overruns, 0 aborts
	 0 ignored, 0 parity errors
 Output (total): 4510240 packets, 3267140805 bytes
	 4509726 unicasts, 99 broadcasts, 415 multicasts, 0 pauses
 Output (normal): 4510240 packets, 3267140805 bytes
	 4509726 unicasts, 99 broadcasts, 415 multicasts, 0 pauses
 Output: 0 output errors, 0 underruns, 0 buffer failures
	 0 aborts, 0 deferred, 0 collisions, 0 late collisions
	 0 lost carrier, 0 no carrier

 GigabitEthernet1/0/5 current state: DOWN
 IP Packet Frame Type: PKTFMT_ETHNT_2, Hardware Address: 20fd-f124-4813
 Description: GigabitEthernet1/0/5 Interface
 Loopback is not set
 Media type is twisted pair, Port hardware type is 1000_BASE_T
 Unknown-speed mode, unknown-duplex mode
 Link speed type is autonegotiation, link duplex type is autonegotiation
 Flow-control is not enabled
 The Maximum Frame Length is 10240
 Broadcast MAX-ratio: 100%
 Unicast MAX-ratio: 100%
 Multicast MAX-ratio: 100%
 PVID: 1
 Mdi type: auto
 Port link-type: access
  Tagged   VLAN ID : none
  Untagged VLAN ID : 1
 Port priority: 0
 Peak value of input: 0 bytes/sec, at 00-00-00 00:00:00 
 Peak value of output: 0 bytes/sec, at 00-00-00 00:00:00 
 Last 300 seconds input:  0 packets/sec 0 bytes/sec 	-%
 Last 300 seconds output:  0 packets/sec 0 bytes/sec 	-%
 Input (total):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input (normal):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input:  0 input errors, 0 runts, 0 giants, 0 throttles
	 0 CRC, 0 frame, 0 overruns, 0 aborts
	 0 ignored, 0 parity errors
 Output (total): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output (normal): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output: 0 output errors, 0 underruns, 0 buffer failures
	 0 aborts, 0 deferred, 0 collisions, 0 late collisions
	 0 lost carrier, 0 no carrier

 GigabitEthernet1/0/6 current state: DOWN
 IP Packet Frame Type: PKTFMT_ETHNT_2, Hardware Address: 20fd-f124-4814
 Description: GigabitEthernet1/0/6 Interface
 Loopback is not set
 Media type is twisted pair, Port hardware type is 1000_BASE_T
 Unknown-speed mode, unknown-duplex mode
 Link speed type is autonegotiation, link duplex type is autonegotiation
 Flow-control is not enabled
 The Maximum Frame Length is 10240
 Broadcast MAX-ratio: 100%
 Unicast MAX-ratio: 100%
 Multicast MAX-ratio: 100%
 PVID: 1
 Mdi type: auto
 Port link-type: access
  Tagged   VLAN ID : none
  Untagged VLAN ID : 1
 Port priority: 0
 Peak value of input: 0 bytes/sec, at 00-00-00 00:00:00 
 Peak value of output: 0 bytes/sec, at 00-00-00 00:00:00 
 Last 300 seconds input:  0 packets/sec 0 bytes/sec 	-%
 Last 300 seconds output:  0 packets/sec 0 bytes/sec 	-%
 Input (total):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input (normal):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input:  0 input errors, 0 runts, 0 giants, 0 throttles
	 0 CRC, 0 frame, 0 overruns, 0 aborts
	 0 ignored, 0 parity errors
 Output (total): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output (normal): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output: 0 output errors, 0 underruns, 0 buffer failures
	 0 aborts, 0 deferred, 0 collisions, 0 late collisions
	 0 lost carrier, 0 no carrier

 GigabitEthernet1/0/7 current state: DOWN
 IP Packet Frame Type: PKTFMT_ETHNT_2, Hardware Address: 20fd-f124-4815
 Description: GigabitEthernet1/0/7 Interface
 Loopback is not set
 Media type is twisted pair, Port hardware type is 1000_BASE_T
 Unknown-speed mode, unknown-duplex mode
 Link speed type is autonegotiation, link duplex type is autonegotiation
 Flow-control is not enabled
 The Maximum Frame Length is 10240
 Broadcast MAX-ratio: 100%
 Unicast MAX-ratio: 100%
 Multicast MAX-ratio: 100%
 PVID: 1
 Mdi type: auto
 Port link-type: access
  Tagged   VLAN ID : none
  Untagged VLAN ID : 1
 Port priority: 0
 Peak value of input: 0 bytes/sec, at 00-00-00 00:00:00 
 Peak value of output: 0 bytes/sec, at 00-00-00 00:00:00 
 Last 300 seconds input:  0 packets/sec 0 bytes/sec 	-%
 Last 300 seconds output:  0 packets/sec 0 bytes/sec 	-%
 Input (total):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input (normal):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input:  0 input errors, 0 runts, 0 giants, 0 throttles
	 0 CRC, 0 frame, 0 overruns, 0 aborts
	 0 ignored, 0 parity errors
 Output (total): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output (normal): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output: 0 output errors, 0 underruns, 0 buffer failures
	 0 aborts, 0 deferred, 0 collisions, 0 late collisions
	 0 lost carrier, 0 no carrier

 GigabitEthernet1/0/8 current state: DOWN
 IP Packet Frame Type: PKTFMT_ETHNT_2, Hardware Address: 20fd-f124-4816
 Description: GigabitEthernet1/0/8 Interface
 Loopback is not set
 Media type is twisted pair, Port hardware type is 1000_BASE_T
 Unknown-speed mode, unknown-duplex mode
 Link speed type is autonegotiation, link duplex type is autonegotiation
 Flow-control is not enabled
 The Maximum Frame Length is 10240
 Broadcast MAX-ratio: 100%
 Unicast MAX-ratio: 100%
 Multicast MAX-ratio: 100%
 PVID: 1
 Mdi type: auto
 Port link-type: access
  Tagged   VLAN ID : none
  Untagged VLAN ID : 1
 Port priority: 0
 Peak value of input: 0 bytes/sec, at 00-00-00 00:00:00 
 Peak value of output: 0 bytes/sec, at 00-00-00 00:00:00 
 Last 300 seconds input:  0 packets/sec 0 bytes/sec 	-%
 Last 300 seconds output:  0 packets/sec 0 bytes/sec 	-%
 Input (total):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input (normal):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input:  0 input errors, 0 runts, 0 giants, 0 throttles
	 0 CRC, 0 frame, 0 overruns, 0 aborts
	 0 ignored, 0 parity errors
 Output (total): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output (normal): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output: 0 output errors, 0 underruns, 0 buffer failures
	 0 aborts, 0 deferred, 0 collisions, 0 late collisions
	 0 lost carrier, 0 no carrier

 GigabitEthernet1/0/9 current state: DOWN
 IP Packet Frame Type: PKTFMT_ETHNT_2, Hardware Address: 20fd-f124-4817
 Description: GigabitEthernet1/0/9 Interface
 Loopback is not set
 Media type is twisted pair, Port hardware type is 1000_BASE_T
 Unknown-speed mode, unknown-duplex mode
 Link speed type is autonegotiation, link duplex type is autonegotiation
 Flow-control is not enabled
 The Maximum Frame Length is 10240
 Broadcast MAX-ratio: 100%
 Unicast MAX-ratio: 100%
 Multicast MAX-ratio: 100%
 PVID: 1
 Mdi type: auto
 Port link-type: access
  Tagged   VLAN ID : none
  Untagged VLAN ID : 1
 Port priority: 0
 Peak value of input: 0 bytes/sec, at 00-00-00 00:00:00 
 Peak value of output: 0 bytes/sec, at 00-00-00 00:00:00 
 Last 300 seconds input:  0 packets/sec 0 bytes/sec 	-%
 Last 300 seconds output:  0 packets/sec 0 bytes/sec 	-%
 Input (total):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input (normal):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input:  0 input errors, 0 runts, 0 giants, 0 throttles
	 0 CRC, 0 frame, 0 overruns, 0 aborts
	 0 ignored, 0 parity errors
 Output (total): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output (normal): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output: 0 output errors, 0 underruns, 0 buffer failures
	 0 aborts, 0 deferred, 0 collisions, 0 late collisions
	 0 lost carrier, 0 no carrier

 GigabitEthernet1/0/10 current state: DOWN
 IP Packet Frame Type: PKTFMT_ETHNT_2, Hardware Address: 20fd-f124-4818
 Description: GigabitEthernet1/0/10 Interface
 Loopback is not set
 Media type is twisted pair, Port hardware type is 1000_BASE_T
 Unknown-speed mode, unknown-duplex mode
 Link speed type is autonegotiation, link duplex type is autonegotiation
 Flow-control is not enabled
 The Maximum Frame Length is 10240
 Broadcast MAX-ratio: 100%
 Unicast MAX-ratio: 100%
 Multicast MAX-ratio: 100%
 PVID: 1
 Mdi type: auto
 Port link-type: access
  Tagged   VLAN ID : none
  Untagged VLAN ID : 1
 Port priority: 0
 Peak value of input: 0 bytes/sec, at 00-00-00 00:00:00 
 Peak value of output: 0 bytes/sec, at 00-00-00 00:00:00 
 Last 300 seconds input:  0 packets/sec 0 bytes/sec 	-%
 Last 300 seconds output:  0 packets/sec 0 bytes/sec 	-%
 Input (total):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input (normal):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input:  0 input errors, 0 runts, 0 giants, 0 throttles
	 0 CRC, 0 frame, 0 overruns, 0 aborts
	 0 ignored, 0 parity errors
 Output (total): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output (normal): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output: 0 output errors, 0 underruns, 0 buffer failures
	 0 aborts, 0 deferred, 0 collisions, 0 late collisions
	 0 lost carrier, 0 no carrier

 GigabitEthernet1/0/11 current state: DOWN
 IP Packet Frame Type: PKTFMT_ETHNT_2, Hardware Address: 20fd-f124-4819
 Description: GigabitEthernet1/0/11 Interface
 Loopback is not set
 Media type is twisted pair, Port hardware type is 1000_BASE_T
 Unknown-speed mode, unknown-duplex mode
 Link speed type is autonegotiation, link duplex type is autonegotiation
 Flow-control is not enabled
 The Maximum Frame Length is 10240
 Broadcast MAX-ratio: 100%
 Unicast MAX-ratio: 100%
 Multicast MAX-ratio: 100%
 PVID: 1
 Mdi type: auto
 Port link-type: access
  Tagged   VLAN ID : none
  Untagged VLAN ID : 1
 Port priority: 0
 Peak value of input: 0 bytes/sec, at 00-00-00 00:00:00 
 Peak value of output: 0 bytes/sec, at 00-00-00 00:00:00 
 Last 300 seconds input:  0 packets/sec 0 bytes/sec 	-%
 Last 300 seconds output:  0 packets/sec 0 bytes/sec 	-%
 Input (total):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input (normal):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input:  0 input errors, 0 runts, 0 giants, 0 throttles
	 0 CRC, 0 frame, 0 overruns, 0 aborts
	 0 ignored, 0 parity errors
 Output (total): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output (normal): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output: 0 output errors, 0 underruns, 0 buffer failures
	 0 aborts, 0 deferred, 0 collisions, 0 late collisions
	 0 lost carrier, 0 no carrier

 GigabitEthernet1/0/12 current state: DOWN
 IP Packet Frame Type: PKTFMT_ETHNT_2, Hardware Address: 20fd-f124-481a
 Description: GigabitEthernet1/0/12 Interface
 Loopback is not set
 Media type is twisted pair, Port hardware type is 1000_BASE_T
 Unknown-speed mode, unknown-duplex mode
 Link speed type is autonegotiation, link duplex type is autonegotiation
 Flow-control is not enabled
 The Maximum Frame Length is 10240
 Broadcast MAX-ratio: 100%
 Unicast MAX-ratio: 100%
 Multicast MAX-ratio: 100%
 PVID: 1
 Mdi type: auto
 Port link-type: access
  Tagged   VLAN ID : none
  Untagged VLAN ID : 1
 Port priority: 0
 Peak value of input: 0 bytes/sec, at 00-00-00 00:00:00 
 Peak value of output: 0 bytes/sec, at 00-00-00 00:00:00 
 Last 300 seconds input:  0 packets/sec 0 bytes/sec 	-%
 Last 300 seconds output:  0 packets/sec 0 bytes/sec 	-%
 Input (total):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input (normal):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input:  0 input errors, 0 runts, 0 giants, 0 throttles
	 0 CRC, 0 frame, 0 overruns, 0 aborts
	 0 ignored, 0 parity errors
 Output (total): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output (normal): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output: 0 output errors, 0 underruns, 0 buffer failures
	 0 aborts, 0 deferred, 0 collisions, 0 late collisions
	 0 lost carrier, 0 no carrier

 GigabitEthernet1/0/13 current state: DOWN
 IP Packet Frame Type: PKTFMT_ETHNT_2, Hardware Address: 20fd-f124-481b
 Description: GigabitEthernet1/0/13 Interface
 Loopback is not set
 Media type is twisted pair, Port hardware type is 1000_BASE_T
 Unknown-speed mode, unknown-duplex mode
 Link speed type is autonegotiation, link duplex type is autonegotiation
 Flow-control is not enabled
 The Maximum Frame Length is 10240
 Broadcast MAX-ratio: 100%
 Unicast MAX-ratio: 100%
 Multicast MAX-ratio: 100%
 PVID: 1
 Mdi type: auto
 Port link-type: access
  Tagged   VLAN ID : none
  Untagged VLAN ID : 1
 Port priority: 0
 Peak value of input: 0 bytes/sec, at 00-00-00 00:00:00 
 Peak value of output: 0 bytes/sec, at 00-00-00 00:00:00 
 Last 300 seconds input:  0 packets/sec 0 bytes/sec 	-%
 Last 300 seconds output:  0 packets/sec 0 bytes/sec 	-%
 Input (total):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input (normal):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input:  0 input errors, 0 runts, 0 giants, 0 throttles
	 0 CRC, 0 frame, 0 overruns, 0 aborts
	 0 ignored, 0 parity errors
 Output (total): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output (normal): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output: 0 output errors, 0 underruns, 0 buffer failures
	 0 aborts, 0 deferred, 0 collisions, 0 late collisions
	 0 lost carrier, 0 no carrier

 GigabitEthernet1/0/14 current state: DOWN
 IP Packet Frame Type: PKTFMT_ETHNT_2, Hardware Address: 20fd-f124-481c
 Description: GigabitEthernet1/0/14 Interface
 Loopback is not set
 Media type is twisted pair, Port hardware type is 1000_BASE_T
 Unknown-speed mode, unknown-duplex mode
 Link speed type is autonegotiation, link duplex type is autonegotiation
 Flow-control is not enabled
 The Maximum Frame Length is 10240
 Broadcast MAX-ratio: 100%
 Unicast MAX-ratio: 100%
 Multicast MAX-ratio: 100%
 PVID: 1
 Mdi type: auto
 Port link-type: access
  Tagged   VLAN ID : none
  Untagged VLAN ID : 1
 Port priority: 0
 Peak value of input: 0 bytes/sec, at 00-00-00 00:00:00 
 Peak value of output: 0 bytes/sec, at 00-00-00 00:00:00 
 Last 300 seconds input:  0 packets/sec 0 bytes/sec 	-%
 Last 300 seconds output:  0 packets/sec 0 bytes/sec 	-%
 Input (total):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input (normal):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input:  0 input errors, 0 runts, 0 giants, 0 throttles
	 0 CRC, 0 frame, 0 overruns, 0 aborts
	 0 ignored, 0 parity errors
 Output (total): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output (normal): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output: 0 output errors, 0 underruns, 0 buffer failures
	 0 aborts, 0 deferred, 0 collisions, 0 late collisions
	 0 lost carrier, 0 no carrier

 GigabitEthernet1/0/15 current state: DOWN
 IP Packet Frame Type: PKTFMT_ETHNT_2, Hardware Address: 20fd-f124-481d
 Description: GigabitEthernet1/0/15 Interface
 Loopback is not set
 Media type is twisted pair, Port hardware type is 1000_BASE_T
 Unknown-speed mode, unknown-duplex mode
 Link speed type is autonegotiation, link duplex type is autonegotiation
 Flow-control is not enabled
 The Maximum Frame Length is 10240
 Broadcast MAX-ratio: 100%
 Unicast MAX-ratio: 100%
 Multicast MAX-ratio: 100%
 PVID: 1
 Mdi type: auto
 Port link-type: access
  Tagged   VLAN ID : none
  Untagged VLAN ID : 1
 Port priority: 0
 Peak value of input: 0 bytes/sec, at 00-00-00 00:00:00 
 Peak value of output: 0 bytes/sec, at 00-00-00 00:00:00 
 Last 300 seconds input:  0 packets/sec 0 bytes/sec 	-%
 Last 300 seconds output:  0 packets/sec 0 bytes/sec 	-%
 Input (total):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input (normal):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input:  0 input errors, 0 runts, 0 giants, 0 throttles
	 0 CRC, 0 frame, 0 overruns, 0 aborts
	 0 ignored, 0 parity errors
 Output (total): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output (normal): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output: 0 output errors, 0 underruns, 0 buffer failures
	 0 aborts, 0 deferred, 0 collisions, 0 late collisions
	 0 lost carrier, 0 no carrier

 GigabitEthernet1/0/16 current state: DOWN
 IP Packet Frame Type: PKTFMT_ETHNT_2, Hardware Address: 20fd-f124-481e
 Description: GigabitEthernet1/0/16 Interface
 Loopback is not set
 Media type is twisted pair, Port hardware type is 1000_BASE_T
 Unknown-speed mode, unknown-duplex mode
 Link speed type is autonegotiation, link duplex type is autonegotiation
 Flow-control is not enabled
 The Maximum Frame Length is 10240
 Broadcast MAX-ratio: 100%
 Unicast MAX-ratio: 100%
 Multicast MAX-ratio: 100%
 PVID: 1
 Mdi type: auto
 Port link-type: access
  Tagged   VLAN ID : none
  Untagged VLAN ID : 1
 Port priority: 0
 Peak value of input: 0 bytes/sec, at 00-00-00 00:00:00 
 Peak value of output: 0 bytes/sec, at 00-00-00 00:00:00 
 Last 300 seconds input:  0 packets/sec 0 bytes/sec 	-%
 Last 300 seconds output:  0 packets/sec 0 bytes/sec 	-%
 Input (total):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input (normal):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input:  0 input errors, 0 runts, 0 giants, 0 throttles
	 0 CRC, 0 frame, 0 overruns, 0 aborts
	 0 ignored, 0 parity errors
 Output (total): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output (normal): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output: 0 output errors, 0 underruns, 0 buffer failures
	 0 aborts, 0 deferred, 0 collisions, 0 late collisions
	 0 lost carrier, 0 no carrier

 GigabitEthernet1/0/17 current state: DOWN
 IP Packet Frame Type: PKTFMT_ETHNT_2, Hardware Address: 20fd-f124-481f
 Description: GigabitEthernet1/0/17 Interface
 Loopback is not set
 Media type is twisted pair, Port hardware type is 1000_BASE_T
 Unknown-speed mode, unknown-duplex mode
 Link speed type is autonegotiation, link duplex type is autonegotiation
 Flow-control is not enabled
 The Maximum Frame Length is 10240
 Broadcast MAX-ratio: 100%
 Unicast MAX-ratio: 100%
 Multicast MAX-ratio: 100%
 PVID: 1
 Mdi type: auto
 Port link-type: access
  Tagged   VLAN ID : none
  Untagged VLAN ID : 1
 Port priority: 0
 Peak value of input: 0 bytes/sec, at 00-00-00 00:00:00 
 Peak value of output: 0 bytes/sec, at 00-00-00 00:00:00 
 Last 300 seconds input:  0 packets/sec 0 bytes/sec 	-%
 Last 300 seconds output:  0 packets/sec 0 bytes/sec 	-%
 Input (total):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input (normal):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input:  0 input errors, 0 runts, 0 giants, 0 throttles
	 0 CRC, 0 frame, 0 overruns, 0 aborts
	 0 ignored, 0 parity errors
 Output (total): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output (normal): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output: 0 output errors, 0 underruns, 0 buffer failures
	 0 aborts, 0 deferred, 0 collisions, 0 late collisions
	 0 lost carrier, 0 no carrier

 GigabitEthernet1/0/18 current state: DOWN
 IP Packet Frame Type: PKTFMT_ETHNT_2, Hardware Address: 20fd-f124-4820
 Description: GigabitEthernet1/0/18 Interface
 Loopback is not set
 Media type is twisted pair, Port hardware type is 1000_BASE_T
 Unknown-speed mode, unknown-duplex mode
 Link speed type is autonegotiation, link duplex type is autonegotiation
 Flow-control is not enabled
 The Maximum Frame Length is 10240
 Broadcast MAX-ratio: 100%
 Unicast MAX-ratio: 100%
 Multicast MAX-ratio: 100%
 PVID: 1
 Mdi type: auto
 Port link-type: access
  Tagged   VLAN ID : none
  Untagged VLAN ID : 1
 Port priority: 0
 Peak value of input: 0 bytes/sec, at 00-00-00 00:00:00 
 Peak value of output: 0 bytes/sec, at 00-00-00 00:00:00 
 Last 300 seconds input:  0 packets/sec 0 bytes/sec 	-%
 Last 300 seconds output:  0 packets/sec 0 bytes/sec 	-%
 Input (total):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input (normal):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input:  0 input errors, 0 runts, 0 giants, 0 throttles
	 0 CRC, 0 frame, 0 overruns, 0 aborts
	 0 ignored, 0 parity errors
 Output (total): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output (normal): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output: 0 output errors, 0 underruns, 0 buffer failures
	 0 aborts, 0 deferred, 0 collisions, 0 late collisions
	 0 lost carrier, 0 no carrier

 GigabitEthernet1/0/19 current state: DOWN
 IP Packet Frame Type: PKTFMT_ETHNT_2, Hardware Address: 20fd-f124-4821
 Description: GigabitEthernet1/0/19 Interface
 Loopback is not set
 Media type is twisted pair, Port hardware type is 1000_BASE_T
 Unknown-speed mode, unknown-duplex mode
 Link speed type is autonegotiation, link duplex type is autonegotiation
 Flow-control is not enabled
 The Maximum Frame Length is 10240
 Broadcast MAX-ratio: 100%
 Unicast MAX-ratio: 100%
 Multicast MAX-ratio: 100%
 PVID: 1
 Mdi type: auto
 Port link-type: access
  Tagged   VLAN ID : none
  Untagged VLAN ID : 1
 Port priority: 0
 Peak value of input: 0 bytes/sec, at 00-00-00 00:00:00 
 Peak value of output: 0 bytes/sec, at 00-00-00 00:00:00 
 Last 300 seconds input:  0 packets/sec 0 bytes/sec 	-%
 Last 300 seconds output:  0 packets/sec 0 bytes/sec 	-%
 Input (total):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input (normal):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input:  0 input errors, 0 runts, 0 giants, 0 throttles
	 0 CRC, 0 frame, 0 overruns, 0 aborts
	 0 ignored, 0 parity errors
 Output (total): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output (normal): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output: 0 output errors, 0 underruns, 0 buffer failures
	 0 aborts, 0 deferred, 0 collisions, 0 late collisions
	 0 lost carrier, 0 no carrier

 GigabitEthernet1/0/20 current state: DOWN
 IP Packet Frame Type: PKTFMT_ETHNT_2, Hardware Address: 20fd-f124-4822
 Description: GigabitEthernet1/0/20 Interface
 Loopback is not set
 Media type is twisted pair, Port hardware type is 1000_BASE_T
 Unknown-speed mode, unknown-duplex mode
 Link speed type is autonegotiation, link duplex type is autonegotiation
 Flow-control is not enabled
 The Maximum Frame Length is 10240
 Broadcast MAX-ratio: 100%
 Unicast MAX-ratio: 100%
 Multicast MAX-ratio: 100%
 PVID: 1
 Mdi type: auto
 Port link-type: access
  Tagged   VLAN ID : none
  Untagged VLAN ID : 1
 Port priority: 0
 Peak value of input: 0 bytes/sec, at 00-00-00 00:00:00 
 Peak value of output: 0 bytes/sec, at 00-00-00 00:00:00 
 Last 300 seconds input:  0 packets/sec 0 bytes/sec 	-%
 Last 300 seconds output:  0 packets/sec 0 bytes/sec 	-%
 Input (total):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input (normal):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input:  0 input errors, 0 runts, 0 giants, 0 throttles
	 0 CRC, 0 frame, 0 overruns, 0 aborts
	 0 ignored, 0 parity errors
 Output (total): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output (normal): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output: 0 output errors, 0 underruns, 0 buffer failures
	 0 aborts, 0 deferred, 0 collisions, 0 late collisions
	 0 lost carrier, 0 no carrier

 GigabitEthernet1/0/21 current state: DOWN
 IP Packet Frame Type: PKTFMT_ETHNT_2, Hardware Address: 20fd-f124-4823
 Description: GigabitEthernet1/0/21 Interface
 Loopback is not set
 Media type is twisted pair, Port hardware type is 1000_BASE_T
 Unknown-speed mode, unknown-duplex mode
 Link speed type is autonegotiation, link duplex type is autonegotiation
 Flow-control is not enabled
 The Maximum Frame Length is 10240
 Broadcast MAX-ratio: 100%
 Unicast MAX-ratio: 100%
 Multicast MAX-ratio: 100%
 PVID: 1
 Mdi type: auto
 Port link-type: access
  Tagged   VLAN ID : none
  Untagged VLAN ID : 1
 Port priority: 0
 Peak value of input: 0 bytes/sec, at 00-00-00 00:00:00 
 Peak value of output: 0 bytes/sec, at 00-00-00 00:00:00 
 Last 300 seconds input:  0 packets/sec 0 bytes/sec 	-%
 Last 300 seconds output:  0 packets/sec 0 bytes/sec 	-%
 Input (total):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input (normal):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input:  0 input errors, 0 runts, 0 giants, 0 throttles
	 0 CRC, 0 frame, 0 overruns, 0 aborts
	 0 ignored, 0 parity errors
 Output (total): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output (normal): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output: 0 output errors, 0 underruns, 0 buffer failures
	 0 aborts, 0 deferred, 0 collisions, 0 late collisions
	 0 lost carrier, 0 no carrier

 GigabitEthernet1/0/22 current state: DOWN
 IP Packet Frame Type: PKTFMT_ETHNT_2, Hardware Address: 20fd-f124-4824
 Description: GigabitEthernet1/0/22 Interface
 Loopback is not set
 Media type is twisted pair, Port hardware type is 1000_BASE_T
 Unknown-speed mode, unknown-duplex mode
 Link speed type is autonegotiation, link duplex type is autonegotiation
 Flow-control is not enabled
 The Maximum Frame Length is 10240
 Broadcast MAX-ratio: 100%
 Unicast MAX-ratio: 100%
 Multicast MAX-ratio: 100%
 PVID: 1
 Mdi type: auto
 Port link-type: access
  Tagged   VLAN ID : none
  Untagged VLAN ID : 1
 Port priority: 0
 Peak value of input: 0 bytes/sec, at 00-00-00 00:00:00 
 Peak value of output: 0 bytes/sec, at 00-00-00 00:00:00 
 Last 300 seconds input:  0 packets/sec 0 bytes/sec 	-%
 Last 300 seconds output:  0 packets/sec 0 bytes/sec 	-%
 Input (total):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input (normal):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input:  0 input errors, 0 runts, 0 giants, 0 throttles
	 0 CRC, 0 frame, 0 overruns, 0 aborts
	 0 ignored, 0 parity errors
 Output (total): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output (normal): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output: 0 output errors, 0 underruns, 0 buffer failures
	 0 aborts, 0 deferred, 0 collisions, 0 late collisions
	 0 lost carrier, 0 no carrier

 GigabitEthernet1/0/23 current state: DOWN
 IP Packet Frame Type: PKTFMT_ETHNT_2, Hardware Address: 20fd-f124-4825
 Description: GigabitEthernet1/0/23 Interface
 Loopback is not set
 Media type is twisted pair, Port hardware type is 1000_BASE_T
 Unknown-speed mode, unknown-duplex mode
 Link speed type is autonegotiation, link duplex type is autonegotiation
 Flow-control is not enabled
 The Maximum Frame Length is 10240
 Broadcast MAX-ratio: 100%
 Unicast MAX-ratio: 100%
 Multicast MAX-ratio: 100%
 PVID: 1
 Mdi type: auto
 Port link-type: access
  Tagged   VLAN ID : none
  Untagged VLAN ID : 1
 Port priority: 0
 Peak value of input: 0 bytes/sec, at 00-00-00 00:00:00 
 Peak value of output: 0 bytes/sec, at 00-00-00 00:00:00 
 Last 300 seconds input:  0 packets/sec 0 bytes/sec 	-%
 Last 300 seconds output:  0 packets/sec 0 bytes/sec 	-%
 Input (total):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input (normal):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input:  0 input errors, 0 runts, 0 giants, 0 throttles
	 0 CRC, 0 frame, 0 overruns, 0 aborts
	 0 ignored, 0 parity errors
 Output (total): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output (normal): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output: 0 output errors, 0 underruns, 0 buffer failures
	 0 aborts, 0 deferred, 0 collisions, 0 late collisions
	 0 lost carrier, 0 no carrier

 GigabitEthernet1/0/24 current state: DOWN
 IP Packet Frame Type: PKTFMT_ETHNT_2, Hardware Address: 20fd-f124-4826
 Description: GigabitEthernet1/0/24 Interface
 Loopback is not set
 Media type is twisted pair, Port hardware type is 1000_BASE_T
 Unknown-speed mode, unknown-duplex mode
 Link speed type is autonegotiation, link duplex type is autonegotiation
 Flow-control is not enabled
 The Maximum Frame Length is 10240
 Broadcast MAX-ratio: 100%
 Unicast MAX-ratio: 100%
 Multicast MAX-ratio: 100%
 PVID: 1
 Mdi type: auto
 Port link-type: access
  Tagged   VLAN ID : none
  Untagged VLAN ID : 1
 Port priority: 0
 Peak value of input: 0 bytes/sec, at 00-00-00 00:00:00 
 Peak value of output: 0 bytes/sec, at 00-00-00 00:00:00 
 Last 300 seconds input:  0 packets/sec 0 bytes/sec 	-%
 Last 300 seconds output:  0 packets/sec 0 bytes/sec 	-%
 Input (total):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input (normal):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input:  0 input errors, 0 runts, 0 giants, 0 throttles
	 0 CRC, 0 frame, 0 overruns, 0 aborts
	 0 ignored, 0 parity errors
 Output (total): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output (normal): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output: 0 output errors, 0 underruns, 0 buffer failures
	 0 aborts, 0 deferred, 0 collisions, 0 late collisions
	 0 lost carrier, 0 no carrier

 GigabitEthernet1/0/25 current state: DOWN
 IP Packet Frame Type: PKTFMT_ETHNT_2, Hardware Address: 20fd-f124-4827
 Description: GigabitEthernet1/0/25 Interface
 Loopback is not set
 Media type is twisted pair, Port hardware type is 1000_BASE_T
 Unknown-speed mode, unknown-duplex mode
 Link speed type is autonegotiation, link duplex type is autonegotiation
 Flow-control is not enabled
 The Maximum Frame Length is 10240
 Broadcast MAX-ratio: 100%
 Unicast MAX-ratio: 100%
 Multicast MAX-ratio: 100%
 PVID: 1
 Mdi type: auto
 Port link-type: access
  Tagged   VLAN ID : none
  Untagged VLAN ID : 1
 Port priority: 0
 Peak value of input: 0 bytes/sec, at 00-00-00 00:00:00 
 Peak value of output: 0 bytes/sec, at 00-00-00 00:00:00 
 Last 300 seconds input:  0 packets/sec 0 bytes/sec 	-%
 Last 300 seconds output:  0 packets/sec 0 bytes/sec 	-%
 Input (total):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input (normal):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input:  0 input errors, 0 runts, 0 giants, 0 throttles
	 0 CRC, 0 frame, 0 overruns, 0 aborts
	 0 ignored, 0 parity errors
 Output (total): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output (normal): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output: 0 output errors, 0 underruns, 0 buffer failures
	 0 aborts, 0 deferred, 0 collisions, 0 late collisions
	 0 lost carrier, 0 no carrier

 GigabitEthernet1/0/26 current state: DOWN
 IP Packet Frame Type: PKTFMT_ETHNT_2, Hardware Address: 20fd-f124-4828
 Description: GigabitEthernet1/0/26 Interface
 Loopback is not set
 Media type is twisted pair, Port hardware type is 1000_BASE_T
 Unknown-speed mode, unknown-duplex mode
 Link speed type is autonegotiation, link duplex type is autonegotiation
 Flow-control is not enabled
 The Maximum Frame Length is 10240
 Broadcast MAX-ratio: 100%
 Unicast MAX-ratio: 100%
 Multicast MAX-ratio: 100%
 PVID: 1
 Mdi type: auto
 Port link-type: access
  Tagged   VLAN ID : none
  Untagged VLAN ID : 1
 Port priority: 0
 Peak value of input: 0 bytes/sec, at 00-00-00 00:00:00 
 Peak value of output: 0 bytes/sec, at 00-00-00 00:00:00 
 Last 300 seconds input:  0 packets/sec 0 bytes/sec 	-%
 Last 300 seconds output:  0 packets/sec 0 bytes/sec 	-%
 Input (total):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input (normal):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input:  0 input errors, 0 runts, 0 giants, 0 throttles
	 0 CRC, 0 frame, 0 overruns, 0 aborts
	 0 ignored, 0 parity errors
 Output (total): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output (normal): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output: 0 output errors, 0 underruns, 0 buffer failures
	 0 aborts, 0 deferred, 0 collisions, 0 late collisions
	 0 lost carrier, 0 no carrier

 GigabitEthernet1/0/27 current state: DOWN
 IP Packet Frame Type: PKTFMT_ETHNT_2, Hardware Address: 20fd-f124-4829
 Description: GigabitEthernet1/0/27 Interface
 Loopback is not set
 Media type is twisted pair, Port hardware type is 1000_BASE_T
 Unknown-speed mode, unknown-duplex mode
 Link speed type is autonegotiation, link duplex type is autonegotiation
 Flow-control is not enabled
 The Maximum Frame Length is 10240
 Broadcast MAX-ratio: 100%
 Unicast MAX-ratio: 100%
 Multicast MAX-ratio: 100%
 PVID: 1
 Mdi type: auto
 Port link-type: access
  Tagged   VLAN ID : none
  Untagged VLAN ID : 1
 Port priority: 0
 Peak value of input: 0 bytes/sec, at 00-00-00 00:00:00 
 Peak value of output: 0 bytes/sec, at 00-00-00 00:00:00 
 Last 300 seconds input:  0 packets/sec 0 bytes/sec 	-%
 Last 300 seconds output:  0 packets/sec 0 bytes/sec 	-%
 Input (total):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input (normal):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input:  0 input errors, 0 runts, 0 giants, 0 throttles
	 0 CRC, 0 frame, 0 overruns, 0 aborts
	 0 ignored, 0 parity errors
 Output (total): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output (normal): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output: 0 output errors, 0 underruns, 0 buffer failures
	 0 aborts, 0 deferred, 0 collisions, 0 late collisions
	 0 lost carrier, 0 no carrier

 GigabitEthernet1/0/28 current state: DOWN
 IP Packet Frame Type: PKTFMT_ETHNT_2, Hardware Address: 20fd-f124-482a
 Description: GigabitEthernet1/0/28 Interface
 Loopback is not set
 Media type is twisted pair, Port hardware type is 1000_BASE_T
 Unknown-speed mode, unknown-duplex mode
 Link speed type is autonegotiation, link duplex type is autonegotiation
 Flow-control is not enabled
 The Maximum Frame Length is 10240
 Broadcast MAX-ratio: 100%
 Unicast MAX-ratio: 100%
 Multicast MAX-ratio: 100%
 PVID: 1
 Mdi type: auto
 Port link-type: access
  Tagged   VLAN ID : none
  Untagged VLAN ID : 1
 Port priority: 0
 Peak value of input: 0 bytes/sec, at 00-00-00 00:00:00 
 Peak value of output: 0 bytes/sec, at 00-00-00 00:00:00 
 Last 300 seconds input:  0 packets/sec 0 bytes/sec 	-%
 Last 300 seconds output:  0 packets/sec 0 bytes/sec 	-%
 Input (total):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input (normal):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input:  0 input errors, 0 runts, 0 giants, 0 throttles
	 0 CRC, 0 frame, 0 overruns, 0 aborts
	 0 ignored, 0 parity errors
 Output (total): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output (normal): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output: 0 output errors, 0 underruns, 0 buffer failures
	 0 aborts, 0 deferred, 0 collisions, 0 late collisions
	 0 lost carrier, 0 no carrier

 GigabitEthernet1/0/29 current state: DOWN
 IP Packet Frame Type: PKTFMT_ETHNT_2, Hardware Address: 20fd-f124-482b
 Description: GigabitEthernet1/0/29 Interface
 Loopback is not set
 Media type is twisted pair, Port hardware type is 1000_BASE_T
 Unknown-speed mode, unknown-duplex mode
 Link speed type is autonegotiation, link duplex type is autonegotiation
 Flow-control is not enabled
 The Maximum Frame Length is 10240
 Broadcast MAX-ratio: 100%
 Unicast MAX-ratio: 100%
 Multicast MAX-ratio: 100%
 PVID: 1
 Mdi type: auto
 Port link-type: access
  Tagged   VLAN ID : none
  Untagged VLAN ID : 1
 Port priority: 0
 Peak value of input: 0 bytes/sec, at 00-00-00 00:00:00 
 Peak value of output: 0 bytes/sec, at 00-00-00 00:00:00 
 Last 300 seconds input:  0 packets/sec 0 bytes/sec 	-%
 Last 300 seconds output:  0 packets/sec 0 bytes/sec 	-%
 Input (total):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input (normal):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input:  0 input errors, 0 runts, 0 giants, 0 throttles
	 0 CRC, 0 frame, 0 overruns, 0 aborts
	 0 ignored, 0 parity errors
 Output (total): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output (normal): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output: 0 output errors, 0 underruns, 0 buffer failures
	 0 aborts, 0 deferred, 0 collisions, 0 late collisions
	 0 lost carrier, 0 no carrier

 GigabitEthernet1/0/30 current state: DOWN
 IP Packet Frame Type: PKTFMT_ETHNT_2, Hardware Address: 20fd-f124-482c
 Description: GigabitEthernet1/0/30 Interface
 Loopback is not set
 Media type is twisted pair, Port hardware type is 1000_BASE_T
 Unknown-speed mode, unknown-duplex mode
 Link speed type is autonegotiation, link duplex type is autonegotiation
 Flow-control is not enabled
 The Maximum Frame Length is 10240
 Broadcast MAX-ratio: 100%
 Unicast MAX-ratio: 100%
 Multicast MAX-ratio: 100%
 PVID: 1
 Mdi type: auto
 Port link-type: access
  Tagged   VLAN ID : none
  Untagged VLAN ID : 1
 Port priority: 0
 Peak value of input: 0 bytes/sec, at 00-00-00 00:00:00 
 Peak value of output: 0 bytes/sec, at 00-00-00 00:00:00 
 Last 300 seconds input:  0 packets/sec 0 bytes/sec 	-%
 Last 300 seconds output:  0 packets/sec 0 bytes/sec 	-%
 Input (total):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input (normal):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input:  0 input errors, 0 runts, 0 giants, 0 throttles
	 0 CRC, 0 frame, 0 overruns, 0 aborts
	 0 ignored, 0 parity errors
 Output (total): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output (normal): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output: 0 output errors, 0 underruns, 0 buffer failures
	 0 aborts, 0 deferred, 0 collisions, 0 late collisions
	 0 lost carrier, 0 no carrier

 GigabitEthernet1/0/31 current state: DOWN
 IP Packet Frame Type: PKTFMT_ETHNT_2, Hardware Address: 20fd-f124-482d
 Description: GigabitEthernet1/0/31 Interface
 Loopback is not set
 Media type is twisted pair, Port hardware type is 1000_BASE_T
 Unknown-speed mode, unknown-duplex mode
 Link speed type is autonegotiation, link duplex type is autonegotiation
 Flow-control is not enabled
 The Maximum Frame Length is 10240
 Broadcast MAX-ratio: 100%
 Unicast MAX-ratio: 100%
 Multicast MAX-ratio: 100%
 PVID: 1
 Mdi type: auto
 Port link-type: access
  Tagged   VLAN ID : none
  Untagged VLAN ID : 1
 Port priority: 0
 Peak value of input: 0 bytes/sec, at 00-00-00 00:00:00 
 Peak value of output: 0 bytes/sec, at 00-00-00 00:00:00 
 Last 300 seconds input:  0 packets/sec 0 bytes/sec 	-%
 Last 300 seconds output:  0 packets/sec 0 bytes/sec 	-%
 Input (total):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input (normal):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input:  0 input errors, 0 runts, 0 giants, 0 throttles
	 0 CRC, 0 frame, 0 overruns, 0 aborts
	 0 ignored, 0 parity errors
 Output (total): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output (normal): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output: 0 output errors, 0 underruns, 0 buffer failures
	 0 aborts, 0 deferred, 0 collisions, 0 late collisions
	 0 lost carrier, 0 no carrier

 GigabitEthernet1/0/32 current state: DOWN
 IP Packet Frame Type: PKTFMT_ETHNT_2, Hardware Address: 20fd-f124-482e
 Description: GigabitEthernet1/0/32 Interface
 Loopback is not set
 Media type is twisted pair, Port hardware type is 1000_BASE_T
 Unknown-speed mode, unknown-duplex mode
 Link speed type is autonegotiation, link duplex type is autonegotiation
 Flow-control is not enabled
 The Maximum Frame Length is 10240
 Broadcast MAX-ratio: 100%
 Unicast MAX-ratio: 100%
 Multicast MAX-ratio: 100%
 PVID: 1
 Mdi type: auto
 Port link-type: access
  Tagged   VLAN ID : none
  Untagged VLAN ID : 1
 Port priority: 0
 Peak value of input: 0 bytes/sec, at 00-00-00 00:00:00 
 Peak value of output: 0 bytes/sec, at 00-00-00 00:00:00 
 Last 300 seconds input:  0 packets/sec 0 bytes/sec 	-%
 Last 300 seconds output:  0 packets/sec 0 bytes/sec 	-%
 Input (total):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input (normal):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input:  0 input errors, 0 runts, 0 giants, 0 throttles
	 0 CRC, 0 frame, 0 overruns, 0 aborts
	 0 ignored, 0 parity errors
 Output (total): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output (normal): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output: 0 output errors, 0 underruns, 0 buffer failures
	 0 aborts, 0 deferred, 0 collisions, 0 late collisions
	 0 lost carrier, 0 no carrier

 GigabitEthernet1/0/33 current state: DOWN
 IP Packet Frame Type: PKTFMT_ETHNT_2, Hardware Address: 20fd-f124-482f
 Description: GigabitEthernet1/0/33 Interface
 Loopback is not set
 Media type is twisted pair, Port hardware type is 1000_BASE_T
 Unknown-speed mode, unknown-duplex mode
 Link speed type is autonegotiation, link duplex type is autonegotiation
 Flow-control is not enabled
 The Maximum Frame Length is 10240
 Broadcast MAX-ratio: 100%
 Unicast MAX-ratio: 100%
 Multicast MAX-ratio: 100%
 PVID: 1
 Mdi type: auto
 Port link-type: access
  Tagged   VLAN ID : none
  Untagged VLAN ID : 1
 Port priority: 0
 Peak value of input: 0 bytes/sec, at 00-00-00 00:00:00 
 Peak value of output: 0 bytes/sec, at 00-00-00 00:00:00 
 Last 300 seconds input:  0 packets/sec 0 bytes/sec 	-%
 Last 300 seconds output:  0 packets/sec 0 bytes/sec 	-%
 Input (total):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input (normal):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input:  0 input errors, 0 runts, 0 giants, 0 throttles
	 0 CRC, 0 frame, 0 overruns, 0 aborts
	 0 ignored, 0 parity errors
 Output (total): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output (normal): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output: 0 output errors, 0 underruns, 0 buffer failures
	 0 aborts, 0 deferred, 0 collisions, 0 late collisions
	 0 lost carrier, 0 no carrier

 GigabitEthernet1/0/34 current state: DOWN
 IP Packet Frame Type: PKTFMT_ETHNT_2, Hardware Address: 20fd-f124-4830
 Description: GigabitEthernet1/0/34 Interface
 Loopback is not set
 Media type is twisted pair, Port hardware type is 1000_BASE_T
 Unknown-speed mode, unknown-duplex mode
 Link speed type is autonegotiation, link duplex type is autonegotiation
 Flow-control is not enabled
 The Maximum Frame Length is 10240
 Broadcast MAX-ratio: 100%
 Unicast MAX-ratio: 100%
 Multicast MAX-ratio: 100%
 PVID: 1
 Mdi type: auto
 Port link-type: access
  Tagged   VLAN ID : none
  Untagged VLAN ID : 1
 Port priority: 0
 Peak value of input: 0 bytes/sec, at 00-00-00 00:00:00 
 Peak value of output: 0 bytes/sec, at 00-00-00 00:00:00 
 Last 300 seconds input:  0 packets/sec 0 bytes/sec 	-%
 Last 300 seconds output:  0 packets/sec 0 bytes/sec 	-%
 Input (total):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input (normal):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input:  0 input errors, 0 runts, 0 giants, 0 throttles
	 0 CRC, 0 frame, 0 overruns, 0 aborts
	 0 ignored, 0 parity errors
 Output (total): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output (normal): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output: 0 output errors, 0 underruns, 0 buffer failures
	 0 aborts, 0 deferred, 0 collisions, 0 late collisions
	 0 lost carrier, 0 no carrier

 GigabitEthernet1/0/35 current state: DOWN
 IP Packet Frame Type: PKTFMT_ETHNT_2, Hardware Address: 20fd-f124-4831
 Description: GigabitEthernet1/0/35 Interface
 Loopback is not set
 Media type is twisted pair, Port hardware type is 1000_BASE_T
 Unknown-speed mode, unknown-duplex mode
 Link speed type is autonegotiation, link duplex type is autonegotiation
 Flow-control is not enabled
 The Maximum Frame Length is 10240
 Broadcast MAX-ratio: 100%
 Unicast MAX-ratio: 100%
 Multicast MAX-ratio: 100%
 PVID: 1
 Mdi type: auto
 Port link-type: access
  Tagged   VLAN ID : none
  Untagged VLAN ID : 1
 Port priority: 0
 Peak value of input: 0 bytes/sec, at 00-00-00 00:00:00 
 Peak value of output: 0 bytes/sec, at 00-00-00 00:00:00 
 Last 300 seconds input:  0 packets/sec 0 bytes/sec 	-%
 Last 300 seconds output:  0 packets/sec 0 bytes/sec 	-%
 Input (total):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input (normal):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input:  0 input errors, 0 runts, 0 giants, 0 throttles
	 0 CRC, 0 frame, 0 overruns, 0 aborts
	 0 ignored, 0 parity errors
 Output (total): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output (normal): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output: 0 output errors, 0 underruns, 0 buffer failures
	 0 aborts, 0 deferred, 0 collisions, 0 late collisions
	 0 lost carrier, 0 no carrier

 GigabitEthernet1/0/36 current state: DOWN
 IP Packet Frame Type: PKTFMT_ETHNT_2, Hardware Address: 20fd-f124-4832
 Description: GigabitEthernet1/0/36 Interface
 Loopback is not set
 Media type is twisted pair, Port hardware type is 1000_BASE_T
 Unknown-speed mode, unknown-duplex mode
 Link speed type is autonegotiation, link duplex type is autonegotiation
 Flow-control is not enabled
 The Maximum Frame Length is 10240
 Broadcast MAX-ratio: 100%
 Unicast MAX-ratio: 100%
 Multicast MAX-ratio: 100%
 PVID: 1
 Mdi type: auto
 Port link-type: access
  Tagged   VLAN ID : none
  Untagged VLAN ID : 1
 Port priority: 0
 Peak value of input: 0 bytes/sec, at 00-00-00 00:00:00 
 Peak value of output: 0 bytes/sec, at 00-00-00 00:00:00 
 Last 300 seconds input:  0 packets/sec 0 bytes/sec 	-%
 Last 300 seconds output:  0 packets/sec 0 bytes/sec 	-%
 Input (total):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input (normal):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input:  0 input errors, 0 runts, 0 giants, 0 throttles
	 0 CRC, 0 frame, 0 overruns, 0 aborts
	 0 ignored, 0 parity errors
 Output (total): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output (normal): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output: 0 output errors, 0 underruns, 0 buffer failures
	 0 aborts, 0 deferred, 0 collisions, 0 late collisions
	 0 lost carrier, 0 no carrier

 GigabitEthernet1/0/37 current state: DOWN
 IP Packet Frame Type: PKTFMT_ETHNT_2, Hardware Address: 20fd-f124-4833
 Description: GigabitEthernet1/0/37 Interface
 Loopback is not set
 Media type is twisted pair, Port hardware type is 1000_BASE_T
 Unknown-speed mode, unknown-duplex mode
 Link speed type is autonegotiation, link duplex type is autonegotiation
 Flow-control is not enabled
 The Maximum Frame Length is 10240
 Broadcast MAX-ratio: 100%
 Unicast MAX-ratio: 100%
 Multicast MAX-ratio: 100%
 PVID: 1
 Mdi type: auto
 Port link-type: access
  Tagged   VLAN ID : none
  Untagged VLAN ID : 1
 Port priority: 0
 Peak value of input: 0 bytes/sec, at 00-00-00 00:00:00 
 Peak value of output: 0 bytes/sec, at 00-00-00 00:00:00 
 Last 300 seconds input:  0 packets/sec 0 bytes/sec 	-%
 Last 300 seconds output:  0 packets/sec 0 bytes/sec 	-%
 Input (total):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input (normal):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input:  0 input errors, 0 runts, 0 giants, 0 throttles
	 0 CRC, 0 frame, 0 overruns, 0 aborts
	 0 ignored, 0 parity errors
 Output (total): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output (normal): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output: 0 output errors, 0 underruns, 0 buffer failures
	 0 aborts, 0 deferred, 0 collisions, 0 late collisions
	 0 lost carrier, 0 no carrier

 GigabitEthernet1/0/38 current state: DOWN
 IP Packet Frame Type: PKTFMT_ETHNT_2, Hardware Address: 20fd-f124-4834
 Description: GigabitEthernet1/0/38 Interface
 Loopback is not set
 Media type is twisted pair, Port hardware type is 1000_BASE_T
 Unknown-speed mode, unknown-duplex mode
 Link speed type is autonegotiation, link duplex type is autonegotiation
 Flow-control is not enabled
 The Maximum Frame Length is 10240
 Broadcast MAX-ratio: 100%
 Unicast MAX-ratio: 100%
 Multicast MAX-ratio: 100%
 PVID: 1
 Mdi type: auto
 Port link-type: access
  Tagged   VLAN ID : none
  Untagged VLAN ID : 1
 Port priority: 0
 Peak value of input: 0 bytes/sec, at 00-00-00 00:00:00 
 Peak value of output: 0 bytes/sec, at 00-00-00 00:00:00 
 Last 300 seconds input:  0 packets/sec 0 bytes/sec 	-%
 Last 300 seconds output:  0 packets/sec 0 bytes/sec 	-%
 Input (total):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input (normal):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input:  0 input errors, 0 runts, 0 giants, 0 throttles
	 0 CRC, 0 frame, 0 overruns, 0 aborts
	 0 ignored, 0 parity errors
 Output (total): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output (normal): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output: 0 output errors, 0 underruns, 0 buffer failures
	 0 aborts, 0 deferred, 0 collisions, 0 late collisions
	 0 lost carrier, 0 no carrier

 GigabitEthernet1/0/39 current state: DOWN
 IP Packet Frame Type: PKTFMT_ETHNT_2, Hardware Address: 20fd-f124-4835
 Description: GigabitEthernet1/0/39 Interface
 Loopback is not set
 Media type is twisted pair, Port hardware type is 1000_BASE_T
 Unknown-speed mode, unknown-duplex mode
 Link speed type is autonegotiation, link duplex type is autonegotiation
 Flow-control is not enabled
 The Maximum Frame Length is 10240
 Broadcast MAX-ratio: 100%
 Unicast MAX-ratio: 100%
 Multicast MAX-ratio: 100%
 PVID: 1
 Mdi type: auto
 Port link-type: access
  Tagged   VLAN ID : none
  Untagged VLAN ID : 1
 Port priority: 0
 Peak value of input: 0 bytes/sec, at 00-00-00 00:00:00 
 Peak value of output: 0 bytes/sec, at 00-00-00 00:00:00 
 Last 300 seconds input:  0 packets/sec 0 bytes/sec 	-%
 Last 300 seconds output:  0 packets/sec 0 bytes/sec 	-%
 Input (total):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input (normal):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input:  0 input errors, 0 runts, 0 giants, 0 throttles
	 0 CRC, 0 frame, 0 overruns, 0 aborts
	 0 ignored, 0 parity errors
 Output (total): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output (normal): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output: 0 output errors, 0 underruns, 0 buffer failures
	 0 aborts, 0 deferred, 0 collisions, 0 late collisions
	 0 lost carrier, 0 no carrier

 GigabitEthernet1/0/40 current state: DOWN
 IP Packet Frame Type: PKTFMT_ETHNT_2, Hardware Address: 20fd-f124-4836
 Description: GigabitEthernet1/0/40 Interface
 Loopback is not set
 Media type is twisted pair, Port hardware type is 1000_BASE_T
 Unknown-speed mode, unknown-duplex mode
 Link speed type is autonegotiation, link duplex type is autonegotiation
 Flow-control is not enabled
 The Maximum Frame Length is 10240
 Broadcast MAX-ratio: 100%
 Unicast MAX-ratio: 100%
 Multicast MAX-ratio: 100%
 PVID: 1
 Mdi type: auto
 Port link-type: access
  Tagged   VLAN ID : none
  Untagged VLAN ID : 1
 Port priority: 0
 Peak value of input: 0 bytes/sec, at 00-00-00 00:00:00 
 Peak value of output: 0 bytes/sec, at 00-00-00 00:00:00 
 Last 300 seconds input:  0 packets/sec 0 bytes/sec 	-%
 Last 300 seconds output:  0 packets/sec 0 bytes/sec 	-%
 Input (total):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input (normal):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input:  0 input errors, 0 runts, 0 giants, 0 throttles
	 0 CRC, 0 frame, 0 overruns, 0 aborts
	 0 ignored, 0 parity errors
 Output (total): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output (normal): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output: 0 output errors, 0 underruns, 0 buffer failures
	 0 aborts, 0 deferred, 0 collisions, 0 late collisions
	 0 lost carrier, 0 no carrier

 GigabitEthernet1/0/41 current state: DOWN
 IP Packet Frame Type: PKTFMT_ETHNT_2, Hardware Address: 20fd-f124-4837
 Description: GigabitEthernet1/0/41 Interface
 Loopback is not set
 Media type is twisted pair, Port hardware type is 1000_BASE_T
 Unknown-speed mode, unknown-duplex mode
 Link speed type is autonegotiation, link duplex type is autonegotiation
 Flow-control is not enabled
 The Maximum Frame Length is 10240
 Broadcast MAX-ratio: 100%
 Unicast MAX-ratio: 100%
 Multicast MAX-ratio: 100%
 PVID: 1
 Mdi type: auto
 Port link-type: access
  Tagged   VLAN ID : none
  Untagged VLAN ID : 1
 Port priority: 0
 Peak value of input: 0 bytes/sec, at 00-00-00 00:00:00 
 Peak value of output: 0 bytes/sec, at 00-00-00 00:00:00 
 Last 300 seconds input:  0 packets/sec 0 bytes/sec 	-%
 Last 300 seconds output:  0 packets/sec 0 bytes/sec 	-%
 Input (total):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input (normal):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input:  0 input errors, 0 runts, 0 giants, 0 throttles
	 0 CRC, 0 frame, 0 overruns, 0 aborts
	 0 ignored, 0 parity errors
 Output (total): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output (normal): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output: 0 output errors, 0 underruns, 0 buffer failures
	 0 aborts, 0 deferred, 0 collisions, 0 late collisions
	 0 lost carrier, 0 no carrier

 GigabitEthernet1/0/42 current state: DOWN
 IP Packet Frame Type: PKTFMT_ETHNT_2, Hardware Address: 20fd-f124-4838
 Description: GigabitEthernet1/0/42 Interface
 Loopback is not set
 Media type is twisted pair, Port hardware type is 1000_BASE_T
 Unknown-speed mode, unknown-duplex mode
 Link speed type is autonegotiation, link duplex type is autonegotiation
 Flow-control is not enabled
 The Maximum Frame Length is 10240
 Broadcast MAX-ratio: 100%
 Unicast MAX-ratio: 100%
 Multicast MAX-ratio: 100%
 PVID: 1
 Mdi type: auto
 Port link-type: access
  Tagged   VLAN ID : none
  Untagged VLAN ID : 1
 Port priority: 0
 Peak value of input: 0 bytes/sec, at 00-00-00 00:00:00 
 Peak value of output: 0 bytes/sec, at 00-00-00 00:00:00 
 Last 300 seconds input:  0 packets/sec 0 bytes/sec 	-%
 Last 300 seconds output:  0 packets/sec 0 bytes/sec 	-%
 Input (total):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input (normal):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input:  0 input errors, 0 runts, 0 giants, 0 throttles
	 0 CRC, 0 frame, 0 overruns, 0 aborts
	 0 ignored, 0 parity errors
 Output (total): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output (normal): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output: 0 output errors, 0 underruns, 0 buffer failures
	 0 aborts, 0 deferred, 0 collisions, 0 late collisions
	 0 lost carrier, 0 no carrier

 GigabitEthernet1/0/43 current state: DOWN
 IP Packet Frame Type: PKTFMT_ETHNT_2, Hardware Address: 20fd-f124-4839
 Description: GigabitEthernet1/0/43 Interface
 Loopback is not set
 Media type is twisted pair, Port hardware type is 1000_BASE_T
 Unknown-speed mode, unknown-duplex mode
 Link speed type is autonegotiation, link duplex type is autonegotiation
 Flow-control is not enabled
 The Maximum Frame Length is 10240
 Broadcast MAX-ratio: 100%
 Unicast MAX-ratio: 100%
 Multicast MAX-ratio: 100%
 PVID: 1
 Mdi type: auto
 Port link-type: access
  Tagged   VLAN ID : none
  Untagged VLAN ID : 1
 Port priority: 0
 Peak value of input: 0 bytes/sec, at 00-00-00 00:00:00 
 Peak value of output: 0 bytes/sec, at 00-00-00 00:00:00 
 Last 300 seconds input:  0 packets/sec 0 bytes/sec 	-%
 Last 300 seconds output:  0 packets/sec 0 bytes/sec 	-%
 Input (total):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input (normal):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input:  0 input errors, 0 runts, 0 giants, 0 throttles
	 0 CRC, 0 frame, 0 overruns, 0 aborts
	 0 ignored, 0 parity errors
 Output (total): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output (normal): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output: 0 output errors, 0 underruns, 0 buffer failures
	 0 aborts, 0 deferred, 0 collisions, 0 late collisions
	 0 lost carrier, 0 no carrier

 GigabitEthernet1/0/44 current state: DOWN
 IP Packet Frame Type: PKTFMT_ETHNT_2, Hardware Address: 20fd-f124-483a
 Description: GigabitEthernet1/0/44 Interface
 Loopback is not set
 Media type is twisted pair, Port hardware type is 1000_BASE_T
 Unknown-speed mode, unknown-duplex mode
 Link speed type is autonegotiation, link duplex type is autonegotiation
 Flow-control is not enabled
 The Maximum Frame Length is 10240
 Broadcast MAX-ratio: 100%
 Unicast MAX-ratio: 100%
 Multicast MAX-ratio: 100%
 PVID: 1
 Mdi type: auto
 Port link-type: access
  Tagged   VLAN ID : none
  Untagged VLAN ID : 1
 Port priority: 0
 Peak value of input: 0 bytes/sec, at 00-00-00 00:00:00 
 Peak value of output: 0 bytes/sec, at 00-00-00 00:00:00 
 Last 300 seconds input:  0 packets/sec 0 bytes/sec 	-%
 Last 300 seconds output:  0 packets/sec 0 bytes/sec 	-%
 Input (total):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input (normal):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input:  0 input errors, 0 runts, 0 giants, 0 throttles
	 0 CRC, 0 frame, 0 overruns, 0 aborts
	 0 ignored, 0 parity errors
 Output (total): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output (normal): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output: 0 output errors, 0 underruns, 0 buffer failures
	 0 aborts, 0 deferred, 0 collisions, 0 late collisions
	 0 lost carrier, 0 no carrier

 GigabitEthernet1/0/45 current state: DOWN
 IP Packet Frame Type: PKTFMT_ETHNT_2, Hardware Address: 20fd-f124-483b
 Description: GigabitEthernet1/0/45 Interface
 Loopback is not set
 Media type is twisted pair, Port hardware type is 1000_BASE_T
 Unknown-speed mode, unknown-duplex mode
 Link speed type is autonegotiation, link duplex type is autonegotiation
 Flow-control is not enabled
 The Maximum Frame Length is 10240
 Broadcast MAX-ratio: 100%
 Unicast MAX-ratio: 100%
 Multicast MAX-ratio: 100%
 PVID: 1
 Mdi type: auto
 Port link-type: access
  Tagged   VLAN ID : none
  Untagged VLAN ID : 1
 Port priority: 0
 Peak value of input: 0 bytes/sec, at 00-00-00 00:00:00 
 Peak value of output: 0 bytes/sec, at 00-00-00 00:00:00 
 Last 300 seconds input:  0 packets/sec 0 bytes/sec 	-%
 Last 300 seconds output:  0 packets/sec 0 bytes/sec 	-%
 Input (total):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input (normal):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input:  0 input errors, 0 runts, 0 giants, 0 throttles
	 0 CRC, 0 frame, 0 overruns, 0 aborts
	 0 ignored, 0 parity errors
 Output (total): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output (normal): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output: 0 output errors, 0 underruns, 0 buffer failures
	 0 aborts, 0 deferred, 0 collisions, 0 late collisions
	 0 lost carrier, 0 no carrier

 GigabitEthernet1/0/46 current state: DOWN
 IP Packet Frame Type: PKTFMT_ETHNT_2, Hardware Address: 20fd-f124-483c
 Description: GigabitEthernet1/0/46 Interface
 Loopback is not set
 Media type is twisted pair, Port hardware type is 1000_BASE_T
 Unknown-speed mode, unknown-duplex mode
 Link speed type is autonegotiation, link duplex type is autonegotiation
 Flow-control is not enabled
 The Maximum Frame Length is 10240
 Broadcast MAX-ratio: 100%
 Unicast MAX-ratio: 100%
 Multicast MAX-ratio: 100%
 PVID: 1
 Mdi type: auto
 Port link-type: access
  Tagged   VLAN ID : none
  Untagged VLAN ID : 1
 Port priority: 0
 Peak value of input: 0 bytes/sec, at 00-00-00 00:00:00 
 Peak value of output: 0 bytes/sec, at 00-00-00 00:00:00 
 Last 300 seconds input:  0 packets/sec 0 bytes/sec 	-%
 Last 300 seconds output:  0 packets/sec 0 bytes/sec 	-%
 Input (total):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input (normal):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input:  0 input errors, 0 runts, 0 giants, 0 throttles
	 0 CRC, 0 frame, 0 overruns, 0 aborts
	 0 ignored, 0 parity errors
 Output (total): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output (normal): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output: 0 output errors, 0 underruns, 0 buffer failures
	 0 aborts, 0 deferred, 0 collisions, 0 late collisions
	 0 lost carrier, 0 no carrier

 GigabitEthernet1/0/47 current state: DOWN
 IP Packet Frame Type: PKTFMT_ETHNT_2, Hardware Address: 20fd-f124-483d
 Description: GigabitEthernet1/0/47 Interface
 Loopback is not set
 Media type is twisted pair, Port hardware type is 1000_BASE_T
 Unknown-speed mode, unknown-duplex mode
 Link speed type is autonegotiation, link duplex type is autonegotiation
 Flow-control is not enabled
 The Maximum Frame Length is 10240
 Broadcast MAX-ratio: 100%
 Unicast MAX-ratio: 100%
 Multicast MAX-ratio: 100%
 PVID: 1
 Mdi type: auto
 Port link-type: access
  Tagged   VLAN ID : none
  Untagged VLAN ID : 1
 Port priority: 0
 Peak value of input: 0 bytes/sec, at 00-00-00 00:00:00 
 Peak value of output: 0 bytes/sec, at 00-00-00 00:00:00 
 Last 300 seconds input:  0 packets/sec 0 bytes/sec 	-%
 Last 300 seconds output:  0 packets/sec 0 bytes/sec 	-%
 Input (total):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input (normal):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input:  0 input errors, 0 runts, 0 giants, 0 throttles
	 0 CRC, 0 frame, 0 overruns, 0 aborts
	 0 ignored, 0 parity errors
 Output (total): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output (normal): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output: 0 output errors, 0 underruns, 0 buffer failures
	 0 aborts, 0 deferred, 0 collisions, 0 late collisions
	 0 lost carrier, 0 no carrier

 GigabitEthernet1/0/48 current state: DOWN
 IP Packet Frame Type: PKTFMT_ETHNT_2, Hardware Address: 20fd-f124-483e
 Description: GigabitEthernet1/0/48 Interface
 Loopback is not set
 Media type is twisted pair, Port hardware type is 1000_BASE_T
 Unknown-speed mode, unknown-duplex mode
 Link speed type is autonegotiation, link duplex type is autonegotiation
 Flow-control is not enabled
 The Maximum Frame Length is 10240
 Broadcast MAX-ratio: 100%
 Unicast MAX-ratio: 100%
 Multicast MAX-ratio: 100%
 PVID: 1
 Mdi type: auto
 Port link-type: access
  Tagged   VLAN ID : none
  Untagged VLAN ID : 1
 Port priority: 0
 Peak value of input: 0 bytes/sec, at 00-00-00 00:00:00 
 Peak value of output: 0 bytes/sec, at 00-00-00 00:00:00 
 Last 300 seconds input:  0 packets/sec 0 bytes/sec 	-%
 Last 300 seconds output:  0 packets/sec 0 bytes/sec 	-%
 Input (total):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input (normal):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input:  0 input errors, 0 runts, 0 giants, 0 throttles
	 0 CRC, 0 frame, 0 overruns, 0 aborts
	 0 ignored, 0 parity errors
 Output (total): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output (normal): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output: 0 output errors, 0 underruns, 0 buffer failures
	 0 aborts, 0 deferred, 0 collisions, 0 late collisions
	 0 lost carrier, 0 no carrier

 GigabitEthernet1/0/49 current state: DOWN
 IP Packet Frame Type: PKTFMT_ETHNT_2, Hardware Address: 20fd-f124-483f
 Description: GigabitEthernet1/0/49 Interface
 Loopback is not set
 Media type is not sure, Port hardware type is No connector
 Unknown-speed mode, unknown-duplex mode
 Link speed type is autonegotiation, link duplex type is autonegotiation
 Flow-control is not enabled
 The Maximum Frame Length is 10240
 Broadcast MAX-ratio: 100%
 Unicast MAX-ratio: 100%
 Multicast MAX-ratio: 100%
 PVID: 1
 Port link-type: access
  Tagged   VLAN ID : none
  Untagged VLAN ID : 1
 Port priority: 0
 Peak value of input: 0 bytes/sec, at 00-00-00 00:00:00 
 Peak value of output: 0 bytes/sec, at 00-00-00 00:00:00 
 Last 300 seconds input:  0 packets/sec 0 bytes/sec 	-%
 Last 300 seconds output:  0 packets/sec 0 bytes/sec 	-%
 Input (total):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input (normal):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input:  0 input errors, 0 runts, 0 giants, 0 throttles
	 0 CRC, 0 frame, 0 overruns, 0 aborts
	 0 ignored, 0 parity errors
 Output (total): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output (normal): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output: 0 output errors, 0 underruns, 0 buffer failures
	 0 aborts, 0 deferred, 0 collisions, 0 late collisions
	 0 lost carrier, 0 no carrier

 GigabitEthernet1/0/50 current state: DOWN
 IP Packet Frame Type: PKTFMT_ETHNT_2, Hardware Address: 20fd-f124-4840
 Description: GigabitEthernet1/0/50 Interface
 Loopback is not set
 Media type is not sure, Port hardware type is No connector
 Unknown-speed mode, unknown-duplex mode
 Link speed type is autonegotiation, link duplex type is autonegotiation
 Flow-control is not enabled
 The Maximum Frame Length is 10240
 Broadcast MAX-ratio: 100%
 Unicast MAX-ratio: 100%
 Multicast MAX-ratio: 100%
 PVID: 1
 Port link-type: access
  Tagged   VLAN ID : none
  Untagged VLAN ID : 1
 Port priority: 0
 Peak value of input: 0 bytes/sec, at 00-00-00 00:00:00 
 Peak value of output: 0 bytes/sec, at 00-00-00 00:00:00 
 Last 300 seconds input:  0 packets/sec 0 bytes/sec 	-%
 Last 300 seconds output:  0 packets/sec 0 bytes/sec 	-%
 Input (total):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input (normal):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input:  0 input errors, 0 runts, 0 giants, 0 throttles
	 0 CRC, 0 frame, 0 overruns, 0 aborts
	 0 ignored, 0 parity errors
 Output (total): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output (normal): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output: 0 output errors, 0 underruns, 0 buffer failures
	 0 aborts, 0 deferred, 0 collisions, 0 late collisions
	 0 lost carrier, 0 no carrier

 GigabitEthernet1/0/51 current state: DOWN
 IP Packet Frame Type: PKTFMT_ETHNT_2, Hardware Address: 20fd-f124-4841
 Description: GigabitEthernet1/0/51 Interface
 Loopback is not set
 Media type is not sure, Port hardware type is No connector
 Unknown-speed mode, unknown-duplex mode
 Link speed type is autonegotiation, link duplex type is autonegotiation
 Flow-control is not enabled
 The Maximum Frame Length is 10240
 Broadcast MAX-ratio: 100%
 Unicast MAX-ratio: 100%
 Multicast MAX-ratio: 100%
 PVID: 1
 Port link-type: access
  Tagged   VLAN ID : none
  Untagged VLAN ID : 1
 Port priority: 0
 Peak value of input: 0 bytes/sec, at 00-00-00 00:00:00 
 Peak value of output: 0 bytes/sec, at 00-00-00 00:00:00 
 Last 300 seconds input:  0 packets/sec 0 bytes/sec 	-%
 Last 300 seconds output:  0 packets/sec 0 bytes/sec 	-%
 Input (total):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input (normal):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input:  0 input errors, 0 runts, 0 giants, 0 throttles
	 0 CRC, 0 frame, 0 overruns, 0 aborts
	 0 ignored, 0 parity errors
 Output (total): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output (normal): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output: 0 output errors, 0 underruns, 0 buffer failures
	 0 aborts, 0 deferred, 0 collisions, 0 late collisions
	 0 lost carrier, 0 no carrier

 GigabitEthernet1/0/52 current state: DOWN
 IP Packet Frame Type: PKTFMT_ETHNT_2, Hardware Address: 20fd-f124-4842
 Description: GigabitEthernet1/0/52 Interface
 Loopback is not set
 Media type is not sure, Port hardware type is No connector
 Unknown-speed mode, unknown-duplex mode
 Link speed type is autonegotiation, link duplex type is autonegotiation
 Flow-control is not enabled
 The Maximum Frame Length is 10240
 Broadcast MAX-ratio: 100%
 Unicast MAX-ratio: 100%
 Multicast MAX-ratio: 100%
 PVID: 1
 Port link-type: access
  Tagged   VLAN ID : none
  Untagged VLAN ID : 1
 Port priority: 0
 Peak value of input: 0 bytes/sec, at 00-00-00 00:00:00 
 Peak value of output: 0 bytes/sec, at 00-00-00 00:00:00 
 Last 300 seconds input:  0 packets/sec 0 bytes/sec 	-%
 Last 300 seconds output:  0 packets/sec 0 bytes/sec 	-%
 Input (total):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input (normal):  0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts
 Input:  0 input errors, 0 runts, 0 giants, 0 throttles
	 0 CRC, 0 frame, 0 overruns, 0 aborts
	 0 ignored, 0 parity errors
 Output (total): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output (normal): 0 packets, 0 bytes
	 0 unicasts, 0 broadcasts, 0 multicasts, 0 pauses
 Output: 0 output errors, 0 underruns, 0 buffer failures
	 0 aborts, 0 deferred, 0 collisions, 0 late collisions
	 0 lost carrier, 0 no carrier

NULL0 current state: UP  
Line protocol current state: UP (spoofing)
Description: NULL0 Interface
The Maximum Transmit Unit is 1500
Internet protocol processing : disabled
Physical is NULL DEV
Last clearing of counters:  13:46:10 Thu 04/27/2000 
    Last 300 seconds input rate: 0 bytes/sec, 0 bits/sec, 0 packets/sec
    Last 300 seconds output rate: 0 bytes/sec, 0 bits/sec, 0 packets/sec
    0 packets input, 0 bytes, 0 drops
    0 packets output, 0 bytes, 0 drops

Vlan-interface1 current state: UP  
Line protocol current state: UP
Description: Vlan-interface1 Interface
The Maximum Transmit Unit is 1500
Internet Address is 192.168.250.10/24 Primary
IP Packet Frame Type: PKTFMT_ETHNT_2,  Hardware Address: 20fd-f124-480e
Last clearing of counters:  13:46:10 Thu 04/27/2000 
    Last 300 seconds input rate: 0 bytes/sec, 0 bits/sec, 0 packets/sec
    Last 300 seconds output rate: 0 bytes/sec, 0 bits/sec, 0 packets/sec
    0 packets input, 0 bytes, 0 drops
    0 packets output, 0 bytes, 0 drops

==================================================
  ===============display memory===============
==================================================
System Total Memory(bytes): 82243280
Total Used Memory(bytes): 34193196
Used Rate: 41%
============================================================
  ===============running task information===============
============================================================
name      Tid Vid TSize Mod priority    Status       Total/Max/Last(Millsecs)
================================================================================
MacS  243ba00   1   40   N   100      eventblock        547/         6/        3
MacF  243be00   2   40   N   100      eventblock          0/         0/        0
VIDL  243b800   3   16   P     1    preemptready   91985291/         9/        9
TICK  243b600   4   16   P   250    preemptready     871953/         0/        0
STMR  243b400   5   40   N   150      eventblock      18669/         1/        0
SYSM  243b200   6   40   N   100      eventblock      10338/       361/        0
 LED  243b000   7   40   N   180      eventblock     187893/         2/        0
LED3  2438e00   8   40   N   180      eventblock      44843/         0/        0
intS  2438c00   9   44   N   100        semblock       5858/        59/        0
RxMi  2438a00  10   40   N   100        semblock     209307/     21391/        0
TxMi  2438800  11   40   N   100        semblock          0/         0/        0
mTrA  2438600  12   10   N   250        semblock          0/         0/        0
macT  2438400  13    8   N   246        semblock          0/         0/        0
LPDT  2438200  14    8   N   100           sleep       1321/         0/        0
AtkT  2438000  15   40   N   100           sleep        829/         0/        0
VMON  2437e00  16   40   N   100      eventblock          0/         0/        0
MGRP  2437c00  17   40   N   100      eventblock          7/         1/        0
IPCM  2437a00  18   40   N   100      eventblock       8553/         0/        0
 CFM  2437800  19   40   N   100        queblock       3460/      1105/     1105
INFO  2437600  20   40   N   100      eventblock       1884/       100/        1
LGFT  2437400  21   40   N   100      eventblock        106/       100/        5
EXCP  2437200  22   40   N   100         suspend          0/         0/        0
 DEV  2437000  23   40   N   140      eventblock      33507/         0/        0
WORK  2436e00  24   40   N   100      eventblock          0/         0/        0
STND  2436c00  25    4   N   100      eventblock      36407/         0/        0
SOCK  2436a00  26   40   N   100      eventblock       9450/         8/        0
ADJ4  2436800  27   40   N   100      eventblock       8720/         0/        0
 ACL  2436600  28   40   N   100      eventblock       8326/         0/        0
VLAN  2436400  29   40   N   100      eventblock        462/         5/        0
 mac  2436200  30   40   N   100      eventblock          4/         1/        0
LAGG  2436000  31   40   N   140      eventblock      30026/         7/        0
MSTP  2435e00  32   40   N   100      eventblock      62358/         6/        1
CLST  2435c00  33   40   N   100      eventblock      21438/         0/        0
 NDP  2435a00  34   40   N   100      eventblock      12689/         1/        0
NTDP  2435800  35   40   N   100      eventblock       9581/         0/        0
HABP  2435600  36   40   N   100      eventblock       7930/         0/        0
LLDP  2435400  37   40   N   100      eventblock       8584/         2/        0
 qos  2435200  38   40   N   100      eventblock          2/         0/        0
 ARP  2435000  39   40   N   100      eventblock      33348/         3/        0
  IP  2434e00  40   40   N   100      eventblock      68083/         3/        0
FSLH  2434c00  41   40   N   100      eventblock       7905/         0/        0
FSLR  2434a00  42   40   N   100      eventblock      83396/         0/        0
HTTP  2434800  43   20   N   100      eventblock       1710/        14/        0
NTPT  2434600  44   40   N   100      eventblock       8812/         0/        0
VTYD  2434400  45   40   N   100      eventblock     103758/         1/        0
DHCC  2434200  46   40   N   100      eventblock        154/         1/        0
DHCP  2434000  47   40   N   100      eventblock          0/         0/        0
DHSE  2433e00  48   40   N   100      eventblock         47/         0/        0
 FIB  2433c00  49   40   N   100      eventblock         38/         2/        1
AGNT  2433a00  50   40   N   100      eventblock          2/         1/        0
TRAP  2433800  51   40   N   100      eventblock         71/         0/        0
DT1X  2433600  52   40   N   100      eventblock       9478/         1/        0
 ACM  2433400  53   40   N   100      eventblock      52127/         0/        0
  LS  2433200  54   40   N   100           sleep      77609/         2/        0
RDSO  2433000  55   40   N   100      eventblock      24722/         0/        0
 RDS  2432e00  56   40   N   100      eventblock       2632/        10/        0
  SC  2432c00  57   40   N   100      eventblock      25546/         0/        0
 NAT  2432a00  58   40   N   100      eventblock          0/         0/        0
 PKI  2432800  59   40   N   100      eventblock         14/         0/        0
IPGD  2432600  60   40   N   100           sleep      65439/         0/        0
PKEY  2432400  61   40   N   100      eventblock          0/         0/        0
PSEC  2432200  62   40   N   100      eventblock       8562/         0/        0
IGSP  2432000  63   40   N   100      eventblock         56/         1/        0
ROUT  2431e00  64   40   N   100      eventblock    1005794/         1/        0
IFNT  2431c00  65   40   N   100      eventblock      12165/        24/        0
WEBS  2431a00  66   40   N   100      eventblock       3288/         3/        0
HDQ0  2430e00  67   20   N   100         running        829/       177/        0
PrdT  2431600  68   40   N   100      eventblock     153635/         9/        9
DrvT  2431400  69   40   N   100      eventblock      57520/         1/        0
=====================================================
  ===============display logbuffer===============
=====================================================
Logging buffer configuration and contents:enabled
Allowed max buffer size : 1024
Actual buffer size : 512
Channel number : 4 , Channel name : logbuffer
Dropped messages : 0
Overwritten messages : 682
Current messages : 512

%Apr 26 17:27:49:558 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/4 of aggregation group BAGG2 becomes ACTIVE!
%Apr 26 17:27:49:566 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation2: link status is UP
%Apr 26 17:27:49:576 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Vlan-interface1: link status is UP
%Apr 26 17:27:49:576 2000 3Com Baseline Switch IFNET/4/UPDOWN:
 Line protocol on the interface Vlan-interface1 is UP
%Apr 26 17:27:50:222 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/2 of aggregation group BAGG1 becomes ACTIVE!
%Apr 26 17:27:50:228 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation1: link status is UP
%Apr 26 17:27:51:235 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/1 of aggregation group BAGG1 becomes ACTIVE!
%Apr 26 17:28:19:439 2000 3Com Baseline Switch MSTP/2/PFWD:Instance 0's Bridge-Aggregation1 has been set to forwarding state!
%Apr 26 17:28:19:440 2000 3Com Baseline Switch MSTP/2/PFWD:Instance 0's Bridge-Aggregation2 has been set to forwarding state!
%Apr 26 17:47:54:76 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/1: link status is DOWN
%Apr 26 17:47:54:77 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/1 of aggregation group BAGG1 becomes INACTIVE, because the port's configuration is improper for aggregation.
%Apr 26 17:47:55:178 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/2: link status is DOWN
%Apr 26 17:47:55:179 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/2 of aggregation group BAGG1 becomes INACTIVE, because the port's configuration is improper for aggregation.
%Apr 26 17:47:55:196 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation1: link status is DOWN
%Apr 26 17:47:57:36 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/18: link status is UP
%Apr 26 17:47:57:37 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/18 of aggregation group BAGG3 becomes ACTIVE!
%Apr 26 17:47:57:45 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation3: link status is UP
%Apr 26 17:48:00:775 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/17: link status is UP
%Apr 26 17:48:00:776 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/17 of aggregation group BAGG3 becomes ACTIVE!
%Apr 26 17:48:02:73 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/3: link status is DOWN
%Apr 26 17:48:02:73 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/3 of aggregation group BAGG2 becomes INACTIVE, because the port's configuration is improper for aggregation.
%Apr 26 17:48:03:750 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/4: link status is DOWN
%Apr 26 17:48:03:751 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/4 of aggregation group BAGG2 becomes INACTIVE, because the port's configuration is improper for aggregation.
%Apr 26 17:48:03:766 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation2: link status is DOWN
%Apr 26 17:48:05:606 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/20: link status is UP
%Apr 26 17:48:05:606 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/20 of aggregation group BAGG4 becomes ACTIVE!
%Apr 26 17:48:05:614 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation4: link status is UP
%Apr 26 17:48:09:896 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/19: link status is UP
%Apr 26 17:48:09:897 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/19 of aggregation group BAGG4 becomes ACTIVE!
%Apr 26 17:48:26:457 2000 3Com Baseline Switch MSTP/2/PFWD:Instance 0's Bridge-Aggregation3 has been set to forwarding state!
%Apr 26 17:48:35:458 2000 3Com Baseline Switch MSTP/2/PFWD:Instance 0's Bridge-Aggregation4 has been set to forwarding state!
%Apr 26 17:50:06:988 2000 3Com Baseline Switch MSTP/2/PFWD:Instance 0's GigabitEthernet1/0/18 has been set to forwarding state!
%Apr 26 17:50:18:333 2000 3Com Baseline Switch HWCM/4/TRAPLOG:
	 1.3.6.1.4.1.43.45.1.6.10.2.1<h3cCfgManEventlog> configure changed:
	 EventIndex=0,CommandSource=2,ConfigSource=4,ConfigDestination=2
%Apr 26 17:50:58:49 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/18 of aggregation group BAGG3 becomes ACTIVE!
%Apr 26 17:52:19:818 2000 3Com Baseline Switch MSTP/2/PFWD:Instance 0's GigabitEthernet1/0/19 has been set to forwarding state!
%Apr 26 17:52:19:837 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation4: link status is DOWN
%Apr 26 17:52:19:847 2000 3Com Baseline Switch MSTP/2/PFWD:Instance 0's GigabitEthernet1/0/20 has been set to forwarding state!
%Apr 26 17:52:41:739 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/19 of aggregation group BAGG4 becomes ACTIVE!
%Apr 26 17:52:41:753 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation4: link status is UP
%Apr 26 17:52:41:766 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/20 of aggregation group BAGG4 becomes ACTIVE!
%Apr 26 17:53:11:591 2000 3Com Baseline Switch MSTP/2/PFWD:Instance 0's Bridge-Aggregation4 has been set to forwarding state!
%Apr 26 17:57:39:287 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/19 of aggregation group BAGG4 becomes INACTIVE, because the port's configuration is improper for aggregation.
%Apr 26 17:57:39:288 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/20 of aggregation group BAGG4 becomes INACTIVE, because the port's configuration is improper for aggregation.
%Apr 26 17:57:39:316 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation4: link status is DOWN
%Apr 26 17:57:39:346 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/19: link status is DOWN
%Apr 26 17:57:39:346 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/20: link status is DOWN
%Apr 26 17:57:41:924 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/20: link status is UP
%Apr 26 17:57:41:930 2000 3Com Baseline Switch MSTP/2/PFWD:Instance 0's GigabitEthernet1/0/20 has been set to forwarding state!
%Apr 26 17:57:41:952 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/19: link status is UP
%Apr 26 17:57:41:958 2000 3Com Baseline Switch MSTP/2/PFWD:Instance 0's GigabitEthernet1/0/19 has been set to forwarding state!
%Apr 26 17:57:53:687 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/17 of aggregation group BAGG3 becomes INACTIVE, because the port's configuration is improper for aggregation.
%Apr 26 17:57:53:688 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/18 of aggregation group BAGG3 becomes INACTIVE, because the port's configuration is improper for aggregation.
%Apr 26 17:57:53:716 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation3: link status is DOWN
%Apr 26 17:57:53:746 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/17: link status is DOWN
%Apr 26 17:57:53:746 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/18: link status is DOWN
%Apr 26 17:57:56:283 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/17: link status is UP
%Apr 26 17:57:56:289 2000 3Com Baseline Switch MSTP/2/PFWD:Instance 0's GigabitEthernet1/0/17 has been set to forwarding state!
%Apr 26 17:57:56:321 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/18: link status is UP
%Apr 26 17:57:56:328 2000 3Com Baseline Switch MSTP/2/PFWD:Instance 0's GigabitEthernet1/0/18 has been set to forwarding state!
%Apr 26 18:00:18:223 2000 3Com Baseline Switch HWCM/4/TRAPLOG:
	 1.3.6.1.4.1.43.45.1.6.10.2.1<h3cCfgManEventlog> configure changed:
	 EventIndex=0,CommandSource=2,ConfigSource=4,ConfigDestination=2
%Apr 26 18:04:21:27 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/18: link status is DOWN
%Apr 26 18:04:22:33 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/17: link status is DOWN
%Apr 26 18:04:23:930 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/1: link status is UP
%Apr 26 18:04:25:303 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/2: link status is UP
%Apr 26 18:04:26:60 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/1 of aggregation group BAGG1 becomes ACTIVE!
%Apr 26 18:04:26:66 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation1: link status is UP
%Apr 26 18:04:26:452 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/19: link status is DOWN
%Apr 26 18:04:27:318 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/20: link status is DOWN
%Apr 26 18:04:27:355 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/2 of aggregation group BAGG1 becomes ACTIVE!
%Apr 26 18:04:29:126 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/4: link status is UP
%Apr 26 18:04:31:285 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/3: link status is UP
%Apr 26 18:04:36:593 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/3 of aggregation group BAGG2 becomes ACTIVE!
%Apr 26 18:04:36:596 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation2: link status is UP
%Apr 26 18:04:44:586 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/3 of aggregation group BAGG2 becomes INACTIVE, because the port's partner is improper for aggregation.
%Apr 26 18:04:44:587 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/4 of aggregation group BAGG2 becomes ACTIVE!
%Apr 26 18:04:44:604 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/3 of aggregation group BAGG2 becomes ACTIVE!
%Apr 26 18:04:55:588 2000 3Com Baseline Switch MSTP/2/PFWD:Instance 0's Bridge-Aggregation1 has been set to forwarding state!
%Apr 26 18:05:06:589 2000 3Com Baseline Switch MSTP/2/PFWD:Instance 0's Bridge-Aggregation2 has been set to forwarding state!
%Apr 26 18:09:18:19 2000 3Com Baseline Switch MSTP/2/PFWD:Instance 0's GigabitEthernet1/0/1 has been set to forwarding state!
%Apr 26 18:09:18:48 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation1: link status is DOWN
%Apr 26 18:09:18:57 2000 3Com Baseline Switch MSTP/2/PFWD:Instance 0's GigabitEthernet1/0/2 has been set to forwarding state!
%Apr 26 18:10:18:214 2000 3Com Baseline Switch HWCM/4/TRAPLOG:
	 1.3.6.1.4.1.43.45.1.6.10.2.1<h3cCfgManEventlog> configure changed:
	 EventIndex=0,CommandSource=2,ConfigSource=4,ConfigDestination=2
%Apr 26 18:10:21:139 2000 3Com Baseline Switch MSTP/2/PFWD:Instance 0's GigabitEthernet1/0/3 has been set to forwarding state!
%Apr 26 18:10:21:168 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation2: link status is DOWN
%Apr 26 18:10:21:178 2000 3Com Baseline Switch MSTP/2/PFWD:Instance 0's GigabitEthernet1/0/4 has been set to forwarding state!
%Apr 26 18:13:07:828 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/1 of aggregation group BAGG1 becomes ACTIVE!
%Apr 26 18:13:07:838 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation1: link status is UP
%Apr 26 18:13:37:629 2000 3Com Baseline Switch MSTP/2/PFWD:Instance 0's Bridge-Aggregation1 has been set to forwarding state!
%Apr 26 18:15:06:367 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/3 of aggregation group BAGG2 becomes ACTIVE!
%Apr 26 18:15:06:372 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation2: link status is UP
%Apr 26 18:15:23:244 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/4 of aggregation group BAGG2 becomes ACTIVE!
%Apr 26 18:15:35:631 2000 3Com Baseline Switch MSTP/2/PFWD:Instance 0's Bridge-Aggregation2 has been set to forwarding state!
%Apr 26 18:15:54:549 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/2: link status is DOWN
%Apr 26 18:16:00:482 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/2: link status is UP
%Apr 26 18:20:18:224 2000 3Com Baseline Switch HWCM/4/TRAPLOG:
	 1.3.6.1.4.1.43.45.1.6.10.2.1<h3cCfgManEventlog> configure changed:
	 EventIndex=0,CommandSource=2,ConfigSource=4,ConfigDestination=2
%Apr 26 18:26:27:898 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/4: link status is DOWN
%Apr 26 18:26:27:898 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/4 of aggregation group BAGG2 becomes INACTIVE, because the port's configuration is improper for aggregation.
%Apr 26 18:26:29:854 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/3: link status is DOWN
%Apr 26 18:26:29:854 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/3 of aggregation group BAGG2 becomes INACTIVE, because the port's configuration is improper for aggregation.
%Apr 26 18:26:29:867 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation2: link status is DOWN
%Apr 26 18:26:30:660 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/4: link status is UP
%Apr 26 18:26:32:883 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/3: link status is UP
%Apr 26 18:26:33:271 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/4 of aggregation group BAGG2 becomes ACTIVE!
%Apr 26 18:26:33:277 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation2: link status is UP
%Apr 26 18:26:35:252 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/3 of aggregation group BAGG2 becomes ACTIVE!
%Apr 26 18:27:02:639 2000 3Com Baseline Switch MSTP/2/PFWD:Instance 0's Bridge-Aggregation2 has been set to forwarding state!
%Apr 26 18:36:28:25 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/2 of aggregation group BAGG1 becomes ACTIVE!
%Apr 27 11:10:44:968 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/4: link status is DOWN
%Apr 27 11:10:44:969 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/4 of aggregation group BAGG2 becomes INACTIVE, because the port's configuration is improper for aggregation.
%Apr 27 11:10:47:350 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/4: link status is UP
%Apr 27 11:10:48:306 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/4: link status is DOWN
%Apr 27 11:10:50:910 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/4: link status is UP
%Apr 27 11:10:51:632 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/3: link status is DOWN
%Apr 27 11:10:51:632 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/3 of aggregation group BAGG2 becomes INACTIVE, because the port's configuration is improper for aggregation.
%Apr 27 11:10:51:647 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation2: link status is DOWN
%Apr 27 11:10:52:872 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/4 of aggregation group BAGG2 becomes ACTIVE!
%Apr 27 11:10:52:879 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation2: link status is UP
%Apr 27 11:10:53:887 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/3: link status is UP
%Apr 27 11:10:54:985 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/3: link status is DOWN
%Apr 27 11:10:57:255 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/3: link status is UP
%Apr 27 11:11:00:674 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/3 of aggregation group BAGG2 becomes ACTIVE!
%Apr 27 11:11:03:937 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/4: link status is DOWN
%Apr 27 11:11:03:938 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/4 of aggregation group BAGG2 becomes INACTIVE, because the port's configuration is improper for aggregation.
%Apr 27 11:11:06:60 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/3: link status is DOWN
%Apr 27 11:11:06:61 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/3 of aggregation group BAGG2 becomes INACTIVE, because the port's configuration is improper for aggregation.
%Apr 27 11:11:06:76 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation2: link status is DOWN
%Apr 27 11:11:07:887 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/4: link status is UP
%Apr 27 11:11:08:362 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/3: link status is UP
%Apr 27 11:11:09:201 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/3: link status is DOWN
%Apr 27 11:11:11:673 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/4 of aggregation group BAGG2 becomes ACTIVE!
%Apr 27 11:11:11:677 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation2: link status is UP
%Apr 27 11:11:11:803 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/3: link status is UP
%Apr 27 11:11:11:803 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/4 of aggregation group BAGG2 becomes INACTIVE, because the port's partner is improper for aggregation.
%Apr 27 11:11:11:816 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation2: link status is DOWN
%Apr 27 11:11:16:676 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/3 of aggregation group BAGG2 becomes ACTIVE!
%Apr 27 11:11:16:677 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/4 of aggregation group BAGG2 becomes ACTIVE!
%Apr 27 11:11:16:680 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation2: link status is UP
%Apr 27 11:11:46:670 2000 3Com Baseline Switch MSTP/2/PFWD:Instance 0's Bridge-Aggregation2 has been set to forwarding state!
%Apr 27 11:11:59:742 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/4: link status is DOWN
%Apr 27 11:11:59:743 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/4 of aggregation group BAGG2 becomes INACTIVE, because the port's configuration is improper for aggregation.
%Apr 27 11:12:00:83 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/3: link status is DOWN
%Apr 27 11:12:00:84 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/3 of aggregation group BAGG2 becomes INACTIVE, because the port's configuration is improper for aggregation.
%Apr 27 11:12:00:97 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation2: link status is DOWN
%Apr 27 11:12:02:186 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/4: link status is UP
%Apr 27 11:12:03:601 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/3: link status is UP
%Apr 27 11:12:08:673 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/3 of aggregation group BAGG2 becomes ACTIVE!
%Apr 27 11:12:08:676 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation2: link status is UP
%Apr 27 11:12:38:669 2000 3Com Baseline Switch MSTP/2/PFWD:Instance 0's Bridge-Aggregation2 has been set to forwarding state!
%Apr 27 11:13:01:857 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/4: link status is DOWN
%Apr 27 11:13:06:98 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/4: link status is UP
%Apr 27 11:13:07:682 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/4: link status is DOWN
%Apr 27 11:13:30:790 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/4: link status is UP
%Apr 27 11:15:50:142 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/4: link status is DOWN
%Apr 27 11:15:50:249 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/3: link status is DOWN
%Apr 27 11:15:50:249 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/3 of aggregation group BAGG2 becomes INACTIVE, because the port's configuration is improper for aggregation.
%Apr 27 11:15:50:267 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation2: link status is DOWN
%Apr 27 11:15:52:758 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/4: link status is UP
%Apr 27 11:15:52:759 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/4 of aggregation group BAGG2 becomes ACTIVE!
%Apr 27 11:15:52:767 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation2: link status is UP
%Apr 27 11:15:52:842 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/3: link status is UP
%Apr 27 11:15:52:842 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/3 of aggregation group BAGG2 becomes ACTIVE!
%Apr 27 11:15:52:843 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/4 of aggregation group BAGG2 becomes INACTIVE, because the port's partner is improper for aggregation.
%Apr 27 11:15:55:129 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/4 of aggregation group BAGG2 becomes ACTIVE!
%Apr 27 11:16:22:670 2000 3Com Baseline Switch MSTP/2/PFWD:Instance 0's Bridge-Aggregation2 has been set to forwarding state!
%Apr 27 11:16:39:328 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/4: link status is DOWN
%Apr 27 11:16:39:328 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/4 of aggregation group BAGG2 becomes INACTIVE, because the port's configuration is improper for aggregation.
%Apr 27 11:16:41:706 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/4: link status is UP
%Apr 27 11:16:44:65 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/4 of aggregation group BAGG2 becomes ACTIVE!
%Apr 27 11:22:53:966 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/2: link status is DOWN
%Apr 27 11:22:53:966 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/2 of aggregation group BAGG1 becomes INACTIVE, because the port's configuration is improper for aggregation.
%Apr 27 11:22:54:297 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/1: link status is DOWN
%Apr 27 11:22:54:297 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/1 of aggregation group BAGG1 becomes INACTIVE, because the port's configuration is improper for aggregation.
%Apr 27 11:22:54:317 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation1: link status is DOWN
%Apr 27 11:22:56:892 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/1: link status is UP
%Apr 27 11:22:58:151 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/2: link status is UP
%Apr 27 11:23:03:673 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/1 of aggregation group BAGG1 becomes ACTIVE!
%Apr 27 11:23:03:676 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation1: link status is UP
%Apr 27 11:23:33:670 2000 3Com Baseline Switch MSTP/2/PFWD:Instance 0's Bridge-Aggregation1 has been set to forwarding state!
%Apr 27 11:25:28:475 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/1: link status is DOWN
%Apr 27 11:25:28:475 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/1 of aggregation group BAGG1 becomes INACTIVE, because the port's configuration is improper for aggregation.
%Apr 27 11:25:28:476 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/2 of aggregation group BAGG1 becomes ACTIVE!
%Apr 27 11:25:31:07 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/1: link status is UP
%Apr 27 11:25:31:07 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/1 of aggregation group BAGG1 becomes ACTIVE!
%Apr 27 11:25:31:07 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/2 of aggregation group BAGG1 becomes INACTIVE, because the port's partner is improper for aggregation.
%Apr 27 11:25:32:680 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/2: link status is DOWN
%Apr 27 11:25:36:934 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/2: link status is UP
%Apr 27 11:32:40:312 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/2: link status is DOWN
%Apr 27 11:32:40:426 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/1: link status is DOWN
%Apr 27 11:32:40:426 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/1 of aggregation group BAGG1 becomes INACTIVE, because the port's configuration is improper for aggregation.
%Apr 27 11:32:40:438 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation1: link status is DOWN
%Apr 27 11:32:42:618 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/2: link status is UP
%Apr 27 11:32:42:619 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/2 of aggregation group BAGG1 becomes ACTIVE!
%Apr 27 11:32:42:627 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation1: link status is UP
%Apr 27 11:32:43:279 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/1: link status is UP
%Apr 27 11:32:43:280 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/1 of aggregation group BAGG1 becomes ACTIVE!
%Apr 27 11:32:43:280 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/2 of aggregation group BAGG1 becomes INACTIVE, because the port's partner is improper for aggregation.
%Apr 27 11:32:44:959 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/1 of aggregation group BAGG1 becomes INACTIVE, because the port's partner is improper for aggregation.
%Apr 27 11:32:44:959 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/2 of aggregation group BAGG1 becomes ACTIVE!
%Apr 27 11:32:45:706 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/1 of aggregation group BAGG1 becomes ACTIVE!
%Apr 27 11:33:11:670 2000 3Com Baseline Switch MSTP/2/PFWD:Instance 0's Bridge-Aggregation1 has been set to forwarding state!
%Apr 27 11:34:31:662 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/1: link status is DOWN
%Apr 27 11:34:31:662 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/2: link status is DOWN
%Apr 27 11:34:31:663 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/1 of aggregation group BAGG1 becomes INACTIVE, because the port's configuration is improper for aggregation.
%Apr 27 11:34:31:681 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/2 of aggregation group BAGG1 becomes INACTIVE, because the port's configuration is improper for aggregation.
%Apr 27 11:34:31:698 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation1: link status is DOWN
%Apr 27 11:34:33:944 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/2: link status is UP
%Apr 27 11:34:34:08 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/1: link status is UP
%Apr 27 11:34:35:985 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/1: link status is DOWN
%Apr 27 11:34:35:986 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/2: link status is DOWN
%Apr 27 11:34:38:321 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/2: link status is UP
%Apr 27 11:34:38:321 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/1: link status is UP
%Apr 27 11:34:43:674 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/1 of aggregation group BAGG1 becomes ACTIVE!
%Apr 27 11:34:43:677 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation1: link status is UP
%Apr 27 11:35:02:246 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/1: link status is DOWN
%Apr 27 11:35:02:246 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/2: link status is DOWN
%Apr 27 11:35:02:247 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/1 of aggregation group BAGG1 becomes INACTIVE, because the port's configuration is improper for aggregation.
%Apr 27 11:35:02:247 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/2 of aggregation group BAGG1 becomes ACTIVE!
%Apr 27 11:35:02:262 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/2 of aggregation group BAGG1 becomes INACTIVE, because the port's configuration is improper for aggregation.
%Apr 27 11:35:02:276 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation1: link status is DOWN
%Apr 27 11:35:04:617 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/2: link status is UP
%Apr 27 11:35:04:618 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/1: link status is UP
%Apr 27 11:35:04:618 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/1 of aggregation group BAGG1 becomes ACTIVE!
%Apr 27 11:35:04:628 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation1: link status is UP
%Apr 27 11:35:33:670 2000 3Com Baseline Switch MSTP/2/PFWD:Instance 0's Bridge-Aggregation1 has been set to forwarding state!
%Apr 27 11:35:53:108 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/1: link status is DOWN
%Apr 27 11:35:53:109 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/1 of aggregation group BAGG1 becomes INACTIVE, because the port's configuration is improper for aggregation.
%Apr 27 11:35:53:109 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/2 of aggregation group BAGG1 becomes ACTIVE!
%Apr 27 11:35:53:311 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/2: link status is DOWN
%Apr 27 11:35:53:311 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/2 of aggregation group BAGG1 becomes INACTIVE, because the port's configuration is improper for aggregation.
%Apr 27 11:35:53:327 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation1: link status is DOWN
%Apr 27 11:35:55:453 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/1: link status is UP
%Apr 27 11:35:55:454 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/1 of aggregation group BAGG1 becomes ACTIVE!
%Apr 27 11:35:55:462 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation1: link status is UP
%Apr 27 11:35:55:889 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/2: link status is UP
%Apr 27 11:35:55:889 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/1 of aggregation group BAGG1 becomes INACTIVE, because the port's partner is improper for aggregation.
%Apr 27 11:35:55:907 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation1: link status is DOWN
%Apr 27 11:35:58:23 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/1 of aggregation group BAGG1 becomes ACTIVE!
%Apr 27 11:35:58:30 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation1: link status is UP
%Apr 27 11:35:58:398 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/2 of aggregation group BAGG1 becomes ACTIVE!
%Apr 27 11:36:27:670 2000 3Com Baseline Switch MSTP/2/PFWD:Instance 0's Bridge-Aggregation1 has been set to forwarding state!
%Apr 27 11:37:27:956 2000 3Com Baseline Switch WEB/4/WEBOPT_LOGOUT:admin logged out from 192.168.250.1
%Apr 27 11:37:27:965 2000 3Com Baseline Switch WEB/4/WEBOPT_LOGOUT:admin logged out from 192.168.250.1
%Apr 27 11:37:27:975 2000 3Com Baseline Switch WEB/4/WEBOPT_LOGOUT:admin logged out from 192.168.250.1
%Apr 27 11:37:33:501 2000 3Com Baseline Switch WEB/4/WEBOPT_LOGIN_SUC:admin logged in from 192.168.250.1
%Apr 27 12:00:14:545 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/1: link status is DOWN
%Apr 27 12:00:14:545 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/1 of aggregation group BAGG1 becomes INACTIVE, because the port's configuration is improper for aggregation.
%Apr 27 12:00:15:940 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/2: link status is DOWN
%Apr 27 12:00:15:940 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/2 of aggregation group BAGG1 becomes INACTIVE, because the port's configuration is improper for aggregation.
%Apr 27 12:00:15:958 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation1: link status is DOWN
%Apr 27 12:00:18:296 2000 3Com Baseline Switch HWCM/4/TRAPLOG:
	 1.3.6.1.4.1.43.45.1.6.10.2.1<h3cCfgManEventlog> configure changed:
	 EventIndex=0,CommandSource=2,ConfigSource=4,ConfigDestination=2
%Apr 27 12:00:19:461 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/18: link status is UP
%Apr 27 12:00:19:461 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/18 of aggregation group BAGG3 becomes ACTIVE!
%Apr 27 12:00:19:469 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation3: link status is UP
%Apr 27 12:00:26:197 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/17: link status is UP
%Apr 27 12:00:26:198 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/17 of aggregation group BAGG3 becomes ACTIVE!
%Apr 27 12:00:26:886 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/3: link status is DOWN
%Apr 27 12:00:26:886 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/3 of aggregation group BAGG2 becomes INACTIVE, because the port's configuration is improper for aggregation.
%Apr 27 12:00:27:851 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/4: link status is DOWN
%Apr 27 12:00:27:852 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/4 of aggregation group BAGG2 becomes INACTIVE, because the port's configuration is improper for aggregation.
%Apr 27 12:00:27:868 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation2: link status is DOWN
%Apr 27 12:00:29:727 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/20: link status is UP
%Apr 27 12:00:29:727 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/20 of aggregation group BAGG4 becomes ACTIVE!
%Apr 27 12:00:29:735 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation4: link status is UP
%Apr 27 12:00:32:566 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/19: link status is UP
%Apr 27 12:00:32:567 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/19 of aggregation group BAGG4 becomes ACTIVE!
%Apr 27 12:00:48:791 2000 3Com Baseline Switch MSTP/2/PFWD:Instance 0's Bridge-Aggregation3 has been set to forwarding state!
%Apr 27 12:00:58:793 2000 3Com Baseline Switch MSTP/2/PFWD:Instance 0's Bridge-Aggregation4 has been set to forwarding state!
%Apr 27 12:06:11:824 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/18: link status is DOWN
%Apr 27 12:06:11:824 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/18 of aggregation group BAGG3 becomes INACTIVE, because the port's configuration is improper for aggregation.
%Apr 27 12:06:11:913 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/17: link status is DOWN
%Apr 27 12:06:11:913 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/17 of aggregation group BAGG3 becomes INACTIVE, because the port's configuration is improper for aggregation.
%Apr 27 12:06:11:929 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation3: link status is DOWN
%Apr 27 12:06:15:34 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/18: link status is UP
%Apr 27 12:06:15:35 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/18 of aggregation group BAGG3 becomes ACTIVE!
%Apr 27 12:06:15:43 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation3: link status is UP
%Apr 27 12:06:15:284 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/17: link status is UP
%Apr 27 12:06:15:284 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/17 of aggregation group BAGG3 becomes ACTIVE!
%Apr 27 12:06:21:40 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/18: link status is DOWN
%Apr 27 12:06:21:41 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/18 of aggregation group BAGG3 becomes INACTIVE, because the port's configuration is improper for aggregation.
%Apr 27 12:06:21:150 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/17: link status is DOWN
%Apr 27 12:06:21:150 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/17 of aggregation group BAGG3 becomes INACTIVE, because the port's configuration is improper for aggregation.
%Apr 27 12:06:21:168 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation3: link status is DOWN
%Apr 27 12:06:23:458 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/18: link status is UP
%Apr 27 12:06:23:458 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/18 of aggregation group BAGG3 becomes ACTIVE!
%Apr 27 12:06:23:467 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation3: link status is UP
%Apr 27 12:06:23:620 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/17: link status is UP
%Apr 27 12:06:23:621 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/17 of aggregation group BAGG3 becomes ACTIVE!
%Apr 27 12:06:52:793 2000 3Com Baseline Switch MSTP/2/PFWD:Instance 0's Bridge-Aggregation3 has been set to forwarding state!
%Apr 27 12:21:26:39 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/20: link status is DOWN
%Apr 27 12:21:26:40 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/20 of aggregation group BAGG4 becomes INACTIVE, because the port's configuration is improper for aggregation.
%Apr 27 12:21:27:967 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/22: link status is UP
%Apr 27 12:21:27:973 2000 3Com Baseline Switch MSTP/2/PFWD:Instance 0's GigabitEthernet1/0/22 has been set to forwarding state!
%Apr 27 12:21:28:965 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/19: link status is DOWN
%Apr 27 12:21:28:966 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/19 of aggregation group BAGG4 becomes INACTIVE, because the port's configuration is improper for aggregation.
%Apr 27 12:21:28:979 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation4: link status is DOWN
%Apr 27 12:21:30:933 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/21: link status is UP
%Apr 27 12:21:30:939 2000 3Com Baseline Switch MSTP/2/PFWD:Instance 0's GigabitEthernet1/0/21 has been set to forwarding state!
%Apr 27 12:21:31:718 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/18: link status is DOWN
%Apr 27 12:21:31:718 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/18 of aggregation group BAGG3 becomes INACTIVE, because the port's configuration is improper for aggregation.
%Apr 27 12:21:34:125 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/24: link status is UP
%Apr 27 12:21:34:131 2000 3Com Baseline Switch MSTP/2/PFWD:Instance 0's GigabitEthernet1/0/24 has been set to forwarding state!
%Apr 27 12:21:35:960 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/17: link status is DOWN
%Apr 27 12:21:35:960 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/17 of aggregation group BAGG3 becomes INACTIVE, because the port's configuration is improper for aggregation.
%Apr 27 12:21:35:979 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation3: link status is DOWN
%Apr 27 12:21:37:800 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/23: link status is UP
%Apr 27 12:21:37:806 2000 3Com Baseline Switch MSTP/2/PFWD:Instance 0's GigabitEthernet1/0/23 has been set to forwarding state!
%Apr 27 12:22:31:994 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/23: link status is DOWN
%Apr 27 12:22:35:56 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/21: link status is DOWN
%Apr 27 12:22:50:578 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/23: link status is UP
%Apr 27 12:22:50:584 2000 3Com Baseline Switch MSTP/2/PFWD:Instance 0's GigabitEthernet1/0/23 has been set to forwarding state!
%Apr 27 12:22:57:395 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/21: link status is UP
%Apr 27 12:22:57:401 2000 3Com Baseline Switch MSTP/2/PFWD:Instance 0's GigabitEthernet1/0/21 has been set to forwarding state!
%Apr 27 12:23:46:590 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/21: link status is DOWN
%Apr 27 12:23:48:10 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/22: link status is DOWN
%Apr 27 12:23:49:795 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/18: link status is UP
%Apr 27 12:23:49:796 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/18 of aggregation group BAGG3 becomes ACTIVE!
%Apr 27 12:23:49:804 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation3: link status is UP
%Apr 27 12:23:51:480 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/17: link status is UP
%Apr 27 12:23:51:481 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/17 of aggregation group BAGG3 becomes ACTIVE!
%Apr 27 12:23:52:881 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/23: link status is DOWN
%Apr 27 12:23:54:248 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/24: link status is DOWN
%Apr 27 12:23:57:936 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/20: link status is UP
%Apr 27 12:23:57:937 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/20 of aggregation group BAGG4 becomes ACTIVE!
%Apr 27 12:23:57:945 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation4: link status is UP
%Apr 27 12:24:00:483 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/19: link status is UP
%Apr 27 12:24:00:483 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/19 of aggregation group BAGG4 becomes ACTIVE!
%Apr 27 12:24:18:852 2000 3Com Baseline Switch MSTP/2/PFWD:Instance 0's Bridge-Aggregation3 has been set to forwarding state!
%Apr 27 12:24:27:853 2000 3Com Baseline Switch MSTP/2/PFWD:Instance 0's Bridge-Aggregation4 has been set to forwarding state!
%Apr 27 12:25:03:869 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/18: link status is DOWN
%Apr 27 12:25:03:870 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/18 of aggregation group BAGG3 becomes INACTIVE, because the port's configuration is improper for aggregation.
%Apr 27 12:25:03:995 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/17: link status is DOWN
%Apr 27 12:25:03:996 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/17 of aggregation group BAGG3 becomes INACTIVE, because the port's configuration is improper for aggregation.
%Apr 27 12:25:04:09 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation3: link status is DOWN
%Apr 27 12:25:06:339 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/18: link status is UP
%Apr 27 12:25:06:339 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/18 of aggregation group BAGG3 becomes ACTIVE!
%Apr 27 12:25:06:349 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation3: link status is UP
%Apr 27 12:25:06:393 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/17: link status is UP
%Apr 27 12:25:06:394 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/17 of aggregation group BAGG3 becomes ACTIVE!
%Apr 27 12:25:35:853 2000 3Com Baseline Switch MSTP/2/PFWD:Instance 0's Bridge-Aggregation3 has been set to forwarding state!
%Apr 27 12:25:46:353 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/17: link status is DOWN
%Apr 27 12:25:46:354 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/17 of aggregation group BAGG3 becomes INACTIVE, because the port's configuration is improper for aggregation.
%Apr 27 12:25:47:443 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/18: link status is DOWN
%Apr 27 12:25:47:443 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/18 of aggregation group BAGG3 becomes INACTIVE, because the port's configuration is improper for aggregation.
%Apr 27 12:25:47:459 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation3: link status is DOWN
%Apr 27 12:25:52:711 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/2: link status is UP
%Apr 27 12:25:56:05 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/1: link status is UP
%Apr 27 12:25:56:78 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/19: link status is DOWN
%Apr 27 12:25:56:78 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/19 of aggregation group BAGG4 becomes INACTIVE, because the port's configuration is improper for aggregation.
%Apr 27 12:25:56:812 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/20: link status is DOWN
%Apr 27 12:25:56:813 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/20 of aggregation group BAGG4 becomes INACTIVE, because the port's configuration is improper for aggregation.
%Apr 27 12:25:56:829 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation4: link status is DOWN
%Apr 27 12:25:56:839 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Vlan-interface1: link status is DOWN
%Apr 27 12:25:56:840 2000 3Com Baseline Switch IFNET/4/UPDOWN:
 Line protocol on the interface Vlan-interface1 is DOWN
%Apr 27 12:25:58:606 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/4: link status is UP
%Apr 27 12:25:59:843 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/3: link status is UP
%Apr 27 12:26:01:857 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/1 of aggregation group BAGG1 becomes ACTIVE!
%Apr 27 12:26:01:860 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation1: link status is UP
%Apr 27 12:26:01:870 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Vlan-interface1: link status is UP
%Apr 27 12:26:01:870 2000 3Com Baseline Switch IFNET/4/UPDOWN:
 Line protocol on the interface Vlan-interface1 is UP
%Apr 27 12:26:04:856 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/3 of aggregation group BAGG2 becomes ACTIVE!
%Apr 27 12:26:04:859 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation2: link status is UP
%Apr 27 12:26:31:852 2000 3Com Baseline Switch MSTP/2/PFWD:Instance 0's Bridge-Aggregation1 has been set to forwarding state!
%Apr 27 12:26:34:853 2000 3Com Baseline Switch MSTP/2/PFWD:Instance 0's Bridge-Aggregation2 has been set to forwarding state!
%Apr 27 12:27:03:540 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/4: link status is DOWN
%Apr 27 12:27:03:638 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/3: link status is DOWN
%Apr 27 12:27:03:638 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/3 of aggregation group BAGG2 becomes INACTIVE, because the port's configuration is improper for aggregation.
%Apr 27 12:27:03:649 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation2: link status is DOWN
%Apr 27 12:27:05:887 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/4: link status is UP
%Apr 27 12:27:05:887 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/4 of aggregation group BAGG2 becomes ACTIVE!
%Apr 27 12:27:05:895 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation2: link status is UP
%Apr 27 12:27:05:935 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/3: link status is UP
%Apr 27 12:27:05:936 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/3 of aggregation group BAGG2 becomes ACTIVE!
%Apr 27 12:27:05:936 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/4 of aggregation group BAGG2 becomes INACTIVE, because the port's partner is improper for aggregation.
%Apr 27 12:27:07:730 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/4: link status is DOWN
%Apr 27 12:27:07:941 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/3: link status is DOWN
%Apr 27 12:27:07:942 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/3 of aggregation group BAGG2 becomes INACTIVE, because the port's configuration is improper for aggregation.
%Apr 27 12:27:07:958 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation2: link status is DOWN
%Apr 27 12:27:10:38 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/4: link status is UP
%Apr 27 12:27:10:38 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/4 of aggregation group BAGG2 becomes ACTIVE!
%Apr 27 12:27:10:47 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation2: link status is UP
%Apr 27 12:27:10:449 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/3: link status is UP
%Apr 27 12:27:10:449 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/3 of aggregation group BAGG2 becomes ACTIVE!
%Apr 27 12:27:10:450 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/4 of aggregation group BAGG2 becomes INACTIVE, because the port's partner is improper for aggregation.
%Apr 27 12:27:35:894 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/4: link status is DOWN
%Apr 27 12:27:36:07 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/3: link status is DOWN
%Apr 27 12:27:36:07 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/3 of aggregation group BAGG2 becomes INACTIVE, because the port's configuration is improper for aggregation.
%Apr 27 12:27:36:19 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation2: link status is DOWN
%Apr 27 12:27:38:363 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/3: link status is UP
%Apr 27 12:27:38:363 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/3 of aggregation group BAGG2 becomes ACTIVE!
%Apr 27 12:27:38:372 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation2: link status is UP
%Apr 27 12:27:38:560 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/4: link status is UP
%Apr 27 12:28:07:852 2000 3Com Baseline Switch MSTP/2/PFWD:Instance 0's Bridge-Aggregation2 has been set to forwarding state!
%Apr 27 12:32:24:623 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/2: link status is DOWN
%Apr 27 12:32:24:720 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/1: link status is DOWN
%Apr 27 12:32:24:720 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/1 of aggregation group BAGG1 becomes INACTIVE, because the port's configuration is improper for aggregation.
%Apr 27 12:32:24:740 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation1: link status is DOWN
%Apr 27 12:32:27:81 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/1: link status is UP
%Apr 27 12:32:27:81 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/1 of aggregation group BAGG1 becomes ACTIVE!
%Apr 27 12:32:27:90 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation1: link status is UP
%Apr 27 12:32:27:116 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/2: link status is UP
%Apr 27 12:32:54:686 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/4: link status is DOWN
%Apr 27 12:32:54:777 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/3: link status is DOWN
%Apr 27 12:32:54:778 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/3 of aggregation group BAGG2 becomes INACTIVE, because the port's configuration is improper for aggregation.
%Apr 27 12:32:54:789 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation2: link status is DOWN
%Apr 27 12:32:56:851 2000 3Com Baseline Switch MSTP/2/PFWD:Instance 0's Bridge-Aggregation1 has been set to forwarding state!
%Apr 27 12:32:57:301 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/4: link status is UP
%Apr 27 12:32:57:301 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/4 of aggregation group BAGG2 becomes ACTIVE!
%Apr 27 12:32:57:310 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation2: link status is UP
%Apr 27 12:32:57:546 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/3: link status is UP
%Apr 27 12:32:57:547 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/3 of aggregation group BAGG2 becomes ACTIVE!
%Apr 27 12:32:57:547 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/4 of aggregation group BAGG2 becomes INACTIVE, because the port's partner is improper for aggregation.
%Apr 27 12:33:26:852 2000 3Com Baseline Switch MSTP/2/PFWD:Instance 0's Bridge-Aggregation2 has been set to forwarding state!
%Apr 27 12:34:25:775 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/3: link status is DOWN
%Apr 27 12:34:25:775 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/3 of aggregation group BAGG2 becomes INACTIVE, because the port's configuration is improper for aggregation.
%Apr 27 12:34:25:776 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/4 of aggregation group BAGG2 becomes ACTIVE!
%Apr 27 12:34:27:130 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/4: link status is DOWN
%Apr 27 12:34:27:130 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/4 of aggregation group BAGG2 becomes INACTIVE, because the port's configuration is improper for aggregation.
%Apr 27 12:34:27:150 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation2: link status is DOWN
%Apr 27 12:34:30:470 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/3: link status is UP
%Apr 27 12:34:30:470 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/3 of aggregation group BAGG2 becomes ACTIVE!
%Apr 27 12:34:30:478 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation2: link status is UP
%Apr 27 12:34:31:251 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/3: link status is DOWN
%Apr 27 12:34:31:251 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/3 of aggregation group BAGG2 becomes INACTIVE, because the port's configuration is improper for aggregation.
%Apr 27 12:34:31:268 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation2: link status is DOWN
%Apr 27 12:34:31:622 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/4: link status is UP
%Apr 27 12:34:31:622 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/4 of aggregation group BAGG2 becomes ACTIVE!
%Apr 27 12:34:31:631 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation2: link status is UP
%Apr 27 12:34:32:593 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/4: link status is DOWN
%Apr 27 12:34:32:593 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/4 of aggregation group BAGG2 becomes INACTIVE, because the port's configuration is improper for aggregation.
%Apr 27 12:34:32:608 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation2: link status is DOWN
%Apr 27 12:34:35:723 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/3: link status is UP
%Apr 27 12:34:35:723 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/3 of aggregation group BAGG2 becomes ACTIVE!
%Apr 27 12:34:35:732 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation2: link status is UP
%Apr 27 12:34:36:724 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/3: link status is DOWN
%Apr 27 12:34:36:725 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/3 of aggregation group BAGG2 becomes INACTIVE, because the port's configuration is improper for aggregation.
%Apr 27 12:34:36:738 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation2: link status is DOWN
%Apr 27 12:34:39:162 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/3: link status is UP
%Apr 27 12:34:39:162 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/3 of aggregation group BAGG2 becomes ACTIVE!
%Apr 27 12:34:39:171 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation2: link status is UP
%Apr 27 12:34:39:676 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/4: link status is UP
%Apr 27 12:34:41:838 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/3 of aggregation group BAGG2 becomes INACTIVE, because the port's partner is improper for aggregation.
%Apr 27 12:34:41:839 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/4 of aggregation group BAGG2 becomes ACTIVE!
%Apr 27 12:34:50:857 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/3 of aggregation group BAGG2 becomes ACTIVE!
%Apr 27 12:35:08:852 2000 3Com Baseline Switch MSTP/2/PFWD:Instance 0's Bridge-Aggregation2 has been set to forwarding state!
%Apr 27 12:38:57:464 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/2: link status is DOWN
%Apr 27 12:38:58:825 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/1: link status is DOWN
%Apr 27 12:38:58:825 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/1 of aggregation group BAGG1 becomes INACTIVE, because the port's configuration is improper for aggregation.
%Apr 27 12:38:58:841 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation1: link status is DOWN
%Apr 27 12:39:01:998 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/2: link status is UP
%Apr 27 12:39:01:998 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/2 of aggregation group BAGG1 becomes ACTIVE!
%Apr 27 12:39:02:06 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation1: link status is UP
%Apr 27 12:39:02:914 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/2: link status is DOWN
%Apr 27 12:39:02:914 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/2 of aggregation group BAGG1 becomes INACTIVE, because the port's configuration is improper for aggregation.
%Apr 27 12:39:02:929 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation1: link status is DOWN
%Apr 27 12:39:03:207 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/1: link status is UP
%Apr 27 12:39:03:207 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/1 of aggregation group BAGG1 becomes ACTIVE!
%Apr 27 12:39:03:215 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation1: link status is UP
%Apr 27 12:39:04:288 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/1: link status is DOWN
%Apr 27 12:39:04:288 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/1 of aggregation group BAGG1 becomes INACTIVE, because the port's configuration is improper for aggregation.
%Apr 27 12:39:04:298 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation1: link status is DOWN
%Apr 27 12:39:07:483 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/2: link status is UP
%Apr 27 12:39:07:483 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/2 of aggregation group BAGG1 becomes ACTIVE!
%Apr 27 12:39:07:492 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation1: link status is UP
%Apr 27 12:39:08:719 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/1: link status is UP
%Apr 27 12:39:08:720 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/1 of aggregation group BAGG1 becomes ACTIVE!
%Apr 27 12:39:08:720 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/2 of aggregation group BAGG1 becomes INACTIVE, because the port's partner is improper for aggregation.
%Apr 27 12:39:19:856 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/2 of aggregation group BAGG1 becomes ACTIVE!
%Apr 27 12:39:36:853 2000 3Com Baseline Switch MSTP/2/PFWD:Instance 0's Bridge-Aggregation1 has been set to forwarding state!
%Apr 27 13:00:18:257 2000 3Com Baseline Switch HWCM/4/TRAPLOG:
	 1.3.6.1.4.1.43.45.1.6.10.2.1<h3cCfgManEventlog> configure changed:
	 EventIndex=0,CommandSource=2,ConfigSource=4,ConfigDestination=2
%Apr 27 14:16:55:613 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/3: link status is DOWN
%Apr 27 14:16:55:613 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/4: link status is DOWN
%Apr 27 14:16:55:614 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/3 of aggregation group BAGG2 becomes INACTIVE, because the port's configuration is improper for aggregation.
%Apr 27 14:16:55:635 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/4 of aggregation group BAGG2 becomes INACTIVE, because the port's configuration is improper for aggregation.
%Apr 27 14:16:55:653 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation2: link status is DOWN
%Apr 27 14:16:58:67 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/3: link status is UP
%Apr 27 14:16:58:115 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/4: link status is UP
%Apr 27 14:17:00:50 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/3: link status is DOWN
%Apr 27 14:17:00:51 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/4: link status is DOWN
%Apr 27 14:17:02:483 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/3: link status is UP
%Apr 27 14:17:02:499 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/4: link status is UP
%Apr 27 14:17:08:78 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/3 of aggregation group BAGG2 becomes ACTIVE!
%Apr 27 14:17:08:82 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation2: link status is UP
%Apr 27 14:17:26:353 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/3: link status is DOWN
%Apr 27 14:17:26:353 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/4: link status is DOWN
%Apr 27 14:17:26:354 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/3 of aggregation group BAGG2 becomes INACTIVE, because the port's configuration is improper for aggregation.
%Apr 27 14:17:26:354 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/4 of aggregation group BAGG2 becomes ACTIVE!
%Apr 27 14:17:26:377 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/4 of aggregation group BAGG2 becomes INACTIVE, because the port's configuration is improper for aggregation.
%Apr 27 14:17:26:391 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation2: link status is DOWN
%Apr 27 14:17:28:818 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/4: link status is UP
%Apr 27 14:17:28:818 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/4 of aggregation group BAGG2 becomes ACTIVE!
%Apr 27 14:17:28:826 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation2: link status is UP
%Apr 27 14:17:28:973 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/3: link status is UP
%Apr 27 14:17:28:973 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/3 of aggregation group BAGG2 becomes ACTIVE!
%Apr 27 14:17:28:974 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/4 of aggregation group BAGG2 becomes INACTIVE, because the port's partner is improper for aggregation.
%Apr 27 14:17:58:76 2000 3Com Baseline Switch MSTP/2/PFWD:Instance 0's Bridge-Aggregation2 has been set to forwarding state!
%Apr 27 14:19:29:230 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/3: link status is DOWN
%Apr 27 14:19:29:231 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/3 of aggregation group BAGG2 becomes INACTIVE, because the port's configuration is improper for aggregation.
%Apr 27 14:19:29:231 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/4 of aggregation group BAGG2 becomes ACTIVE!
%Apr 27 14:19:29:432 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/4: link status is DOWN
%Apr 27 14:19:29:433 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/4 of aggregation group BAGG2 becomes INACTIVE, because the port's configuration is improper for aggregation.
%Apr 27 14:19:29:441 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation2: link status is DOWN
%Apr 27 14:19:31:658 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/3: link status is UP
%Apr 27 14:19:31:658 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/3 of aggregation group BAGG2 becomes ACTIVE!
%Apr 27 14:19:31:666 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation2: link status is UP
%Apr 27 14:19:31:827 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 GigabitEthernet1/0/4: link status is UP
%Apr 27 14:19:32:79 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/3 of aggregation group BAGG2 becomes INACTIVE, because the port's partner is improper for aggregation.
%Apr 27 14:19:32:84 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation2: link status is DOWN
%Apr 27 14:19:33:87 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/3 of aggregation group BAGG2 becomes ACTIVE!
%Apr 27 14:19:33:93 2000 3Com Baseline Switch IFNET/4/LINK UPDOWN:
 Bridge-Aggregation2: link status is UP
%Apr 27 14:20:03:77 2000 3Com Baseline Switch MSTP/2/PFWD:Instance 0's Bridge-Aggregation2 has been set to forwarding state!
%Apr 27 14:20:06:79 2000 3Com Baseline Switch LAGG/2/LAGG_LOG:
 Port member GigabitEthernet1/0/4 of aggregation group BAGG2 becomes ACTIVE!
%Apr 27 14:36:31:400 2000 3Com Baseline Switch WEB/4/WEBOPT_LOGIN_SUC:admin logged in from 192.168.250.1
====================================================
  ===============display vlan all===============
====================================================
 VLAN ID: 1
 VLAN Type: static
 Route Interface: configured
 IP Address: 192.168.250.10
 Subnet Mask: 255.255.255.0
 Description: VLAN 0001
 Name: VLAN 0001
 Tagged   Ports: none
 Untagged Ports: 
    Bridge-Aggregation1      Bridge-Aggregation2      
    GigabitEthernet1/0/1     GigabitEthernet1/0/2     GigabitEthernet1/0/3     
    GigabitEthernet1/0/4     GigabitEthernet1/0/5     GigabitEthernet1/0/6     
    GigabitEthernet1/0/7     GigabitEthernet1/0/8     GigabitEthernet1/0/9     
    GigabitEthernet1/0/10    GigabitEthernet1/0/11    GigabitEthernet1/0/12    
    GigabitEthernet1/0/13    GigabitEthernet1/0/14    GigabitEthernet1/0/15    
    GigabitEthernet1/0/16    GigabitEthernet1/0/17    GigabitEthernet1/0/18    
    GigabitEthernet1/0/19    GigabitEthernet1/0/20    GigabitEthernet1/0/21    
    GigabitEthernet1/0/22    GigabitEthernet1/0/23    GigabitEthernet1/0/24    
    GigabitEthernet1/0/25    GigabitEthernet1/0/26    GigabitEthernet1/0/27    
    GigabitEthernet1/0/28    GigabitEthernet1/0/29    GigabitEthernet1/0/30    
    GigabitEthernet1/0/31    GigabitEthernet1/0/32    GigabitEthernet1/0/33    
    GigabitEthernet1/0/34    GigabitEthernet1/0/35    GigabitEthernet1/0/36    
    GigabitEthernet1/0/37    GigabitEthernet1/0/38    GigabitEthernet1/0/39    
    GigabitEthernet1/0/40    GigabitEthernet1/0/41    GigabitEthernet1/0/42    
    GigabitEthernet1/0/43    GigabitEthernet1/0/44    GigabitEthernet1/0/45    
    GigabitEthernet1/0/46    GigabitEthernet1/0/47    GigabitEthernet1/0/48    
    GigabitEthernet1/0/49    GigabitEthernet1/0/50    GigabitEthernet1/0/51    
    GigabitEthernet1/0/52    

=======================================================
  ===============all history command===============
=======================================================
=====================================================
  ===============display stp brief===============
=====================================================
 MSTID      Port                         Role  STP State     Protection
   0        Bridge-Aggregation1          DESI  FORWARDING    NONE
   0        Bridge-Aggregation2          DESI  FORWARDING    NONE
===================================================
  ===============display arp all===============
===================================================
                Type: S-Static    D-Dynamic
IP Address       MAC Address     VLAN ID  Interface              Aging Type
192.168.250.1    d485-6444-19f0  1        BAGG1                  20    D
========================================================
  ===============display ip interface===============
========================================================
Vlan-interface1 current state :UP 
Line protocol current state :UP
Internet Address is 192.168.250.10/24 Primary
Broadcast address : 192.168.250.255
The Maximum Transmit Unit : 1500 bytes
input packets : 38702, bytes : 3816715, multicasts : 0
output packets : 39084, bytes : 17190033, multicasts : 0
ARP packet input number:        2108
  Request packet:               2011
  Reply packet:                   97
  Unknown packet:                  0
TTL invalid packet number:         0
ICMP packet input number:      12375
  Echo reply:                      0
  Unreachable:                     0
  Source quench:                   0
  Routing redirect:                0
  Echo request:                12375
  Router advert:                   0
  Router solicit:                  0
  Time exceed:                     0
  IP header bad:                   0
  Timestamp request:               0
  Timestamp reply:                 0
  Information request:             0
  Information reply:               0
  Netmask request:                 0
  Netmask reply:                   0
  Unknown type:                    0

=========================================================
  ===============display ip statistics===============
=========================================================
  Input:   sum            38702            local             38700     
           bad protocol   0                bad format        0         
           bad checksum   0                bad options       0         
  Output:  forwarding     0                local             39516     
           dropped        0                no route          434       
           compress fails 0         
  Fragment:input          0                output            0         
           dropped        0         
           fragmented     0                couldn't fragment 0         
  Reassembling:sum        0                timeouts          0         
===============================================
  ===============display fib===============
===============================================
Destination count: 4    FIB entry count: 4

Flag:
  U:Useable   G:Gateway   H:Host   B:Blackhole   D:Dynamic   S:Static
  R:Relay

Destination/Mask   Nexthop         Flag    OutInterface   InnerLabel Token
192.168.250.0/24   0.0.0.0         U       Vlan1               Null  Invalid   
192.168.250.10/32  127.0.0.1       UH      InLoop0             Null  Invalid   
127.0.0.1/32       127.0.0.1       UH      InLoop0             Null  Invalid   
127.0.0.0/8        127.0.0.1       U       InLoop0             Null  Invalid   
====================================================
  ===============_display version===============
====================================================
3Com Corporation
3Com OS Software Version COMWAREV500R002B66D212
3Com Baseline Switch 2952-SFP Plus Software Version V100R002B03D007SP01
Copyright (c) 2004-2010 3Com Corp. and its licensors. All rights reserved.
Compiled Jun 28 2010 14:07:33, RELEASE SOFTWARE
3Com Baseline Switch 2952-SFP Plus uptime is 0 week, 1 day, 2 hours, 36 minutes

3Com Baseline Switch 2952-SFP Plus
128M    bytes DRAM
128M    bytes Nand Flash Memory
Config Register points to Nand Flash

Hardware Version is REV.B
CPLD Version is 002
Bootrom Version is 119
[SubSlot 0] 48GE+4SFP Hardware Version is REV.B

=================================================================
  ===============_display drv ni interrupt all===============
=================================================================
 Dev: 0 Display all Interrupt information.
 Interrupt 42 XCAT_EB_AUQ_PENDING total num 7
 Interrupt 321 XCAT_LINK_STATUS_CHANGED_PORT2 total num 8
 Interrupt 322 XCAT_AN_COMPLETED_PORT2 total num 4
 Interrupt 353 XCAT_LINK_STATUS_CHANGED_PORT3 total num 8
 Interrupt 354 XCAT_AN_COMPLETED_PORT3 total num 4
 Dev: 1 Display all Interrupt information.
===============================================================
  ===============_clear drv ni interrupt all===============
===============================================================
 Reset Dev: 0 Interrupt success!
 Reset Dev: 1 Interrupt success!
==================================================================
  ===============_display drv 1000m_cablelength===============
==================================================================
 1000M Powersaving len:90, Class-A len:90, Power-saving:0,LinkDelay:10S 
P 0 l: 17,  0m.L:1,S:1000 CReg:0040 NoPSv:1 PSSt:0,Post:1 PSReg:a004 ClassA:0 
P 1 l: 18,  5m.L:1,S:1000 CReg:0040 NoPSv:1 PSSt:0,Post:1 PSReg:a004 ClassA:0 
P 2 l: 17,  0m.L:1,S:1000 CReg:0040 NoPSv:1 PSSt:0,Post:1 PSReg:a004 ClassA:0 
P 3 l: 16,  0m.L:1,S:1000 CReg:0040 NoPSv:1 PSSt:0,Post:1 PSReg:a004 ClassA:0 
P 4 l:  0,  0m.L:0,S:1000 CReg:9040 NoPSv:1 PSSt:0,Post:1 PSReg:a004 ClassA:0 
P 5 l:  0,  0m.L:0,S:1000 CReg:9040 NoPSv:1 PSSt:0,Post:1 PSReg:a004 ClassA:0 
P 6 l:  0,  0m.L:0,S:1000 CReg:9040 NoPSv:1 PSSt:0,Post:1 PSReg:a004 ClassA:0 
P 7 l:  0,  0m.L:0,S:1000 CReg:9040 NoPSv:1 PSSt:0,Post:1 PSReg:a004 ClassA:0 
P 8 l:  0,  0m.L:0,S:1000 CReg:9040 NoPSv:1 PSSt:0,Post:1 PSReg:a004 ClassA:0 
P 9 l:  0,  0m.L:0,S:1000 CReg:9040 NoPSv:1 PSSt:0,Post:1 PSReg:a004 ClassA:0 
P10 l:  0,  0m.L:0,S:1000 CReg:9040 NoPSv:1 PSSt:0,Post:1 PSReg:a004 ClassA:0 
P11 l:  0,  0m.L:0,S:1000 CReg:9040 NoPSv:1 PSSt:0,Post:1 PSReg:a004 ClassA:0 
P12 l:  0,  0m.L:0,S:1000 CReg:9040 NoPSv:1 PSSt:0,Post:1 PSReg:a004 ClassA:0 
P13 l:  0,  0m.L:0,S:1000 CReg:9040 NoPSv:1 PSSt:0,Post:1 PSReg:a004 ClassA:0 
P14 l:  0,  0m.L:0,S:1000 CReg:9040 NoPSv:1 PSSt:0,Post:1 PSReg:a004 ClassA:0 
P15 l:  0,  0m.L:0,S:1000 CReg:9040 NoPSv:1 PSSt:0,Post:1 PSReg:a004 ClassA:0 
P16 l:  0,  0m.L:0,S:1000 CReg:9040 NoPSv:1 PSSt:0,Post:1 PSReg:a004 ClassA:0 
P17 l:  0,  0m.L:0,S:1000 CReg:9040 NoPSv:1 PSSt:0,Post:1 PSReg:a004 ClassA:0 
P18 l:  0,  0m.L:0,S:1000 CReg:9040 NoPSv:1 PSSt:0,Post:1 PSReg:a004 ClassA:0 
P19 l:  0,  0m.L:0,S:1000 CReg:9040 NoPSv:1 PSSt:0,Post:1 PSReg:a004 ClassA:0 
P20 l:  0,  0m.L:0,S:1000 CReg:9040 NoPSv:1 PSSt:0,Post:1 PSReg:a004 ClassA:0 
P21 l:  0,  0m.L:0,S:1000 CReg:9040 NoPSv:1 PSSt:0,Post:1 PSReg:a004 ClassA:0 
P22 l:  0,  0m.L:0,S:1000 CReg:9040 NoPSv:1 PSSt:0,Post:1 PSReg:a004 ClassA:0 
P23 l:  0,  0m.L:0,S:1000 CReg:9040 NoPSv:1 PSSt:0,Post:1 PSReg:a004 ClassA:0 
P24 l:  0,  0m.L:0,S:1000 CReg:9040 NoPSv:1 PSSt:0,Post:1 PSReg:a004 ClassA:0 
P25 l:  0,  0m.L:0,S:1000 CReg:9040 NoPSv:1 PSSt:0,Post:1 PSReg:a004 ClassA:0 
P26 l:  0,  0m.L:0,S:1000 CReg:9040 NoPSv:1 PSSt:0,Post:1 PSReg:a004 ClassA:0 
P27 l:  0,  0m.L:0,S:1000 CReg:9040 NoPSv:1 PSSt:0,Post:1 PSReg:a004 ClassA:0 
P28 l:  0,  0m.L:0,S:1000 CReg:9040 NoPSv:1 PSSt:0,Post:1 PSReg:a004 ClassA:0 
P29 l:  0,  0m.L:0,S:1000 CReg:9040 NoPSv:1 PSSt:0,Post:1 PSReg:a004 ClassA:0 
P30 l:  0,  0m.L:0,S:1000 CReg:9040 NoPSv:1 PSSt:0,Post:1 PSReg:a004 ClassA:0 
P31 l:  0,  0m.L:0,S:1000 CReg:9040 NoPSv:1 PSSt:0,Post:1 PSReg:a004 ClassA:0 
P32 l:  0,  0m.L:0,S:1000 CReg:9040 NoPSv:1 PSSt:0,Post:1 PSReg:a004 ClassA:0 
P33 l:  0,  0m.L:0,S:1000 CReg:9040 NoPSv:1 PSSt:0,Post:1 PSReg:a004 ClassA:0 
P34 l:  0,  0m.L:0,S:1000 CReg:9040 NoPSv:1 PSSt:0,Post:1 PSReg:a004 ClassA:0 
P35 l:  0,  0m.L:0,S:1000 CReg:9040 NoPSv:1 PSSt:0,Post:1 PSReg:a004 ClassA:0 
P36 l:  0,  0m.L:0,S:1000 CReg:9040 NoPSv:1 PSSt:0,Post:1 PSReg:a004 ClassA:0 
P37 l:  0,  0m.L:0,S:1000 CReg:9040 NoPSv:1 PSSt:0,Post:1 PSReg:a004 ClassA:0 
P38 l:  0,  0m.L:0,S:1000 CReg:9040 NoPSv:1 PSSt:0,Post:1 PSReg:a004 ClassA:0 
P39 l:  0,  0m.L:0,S:1000 CReg:9040 NoPSv:1 PSSt:0,Post:1 PSReg:a004 ClassA:0 
P40 l:  0,  0m.L:0,S:1000 CReg:9040 NoPSv:1 PSSt:0,Post:1 PSReg:a004 ClassA:0 
P41 l:  0,  0m.L:0,S:1000 CReg:9040 NoPSv:1 PSSt:0,Post:1 PSReg:a004 ClassA:0 
P42 l:  0,  0m.L:0,S:1000 CReg:9040 NoPSv:1 PSSt:0,Post:1 PSReg:a004 ClassA:0 
P43 l:  0,  0m.L:0,S:1000 CReg:9040 NoPSv:1 PSSt:0,Post:1 PSReg:a004 ClassA:0 
P44 l:  0,  0m.L:0,S:1000 CReg:9040 NoPSv:1 PSSt:0,Post:1 PSReg:a004 ClassA:0 
P45 l:  0,  0m.L:0,S:1000 CReg:9040 NoPSv:1 PSSt:0,Post:1 PSReg:a004 ClassA:0 
P46 l:  0,  0m.L:0,S:1000 CReg:9040 NoPSv:1 PSSt:0,Post:1 PSReg:a004 ClassA:0 
P47 l:  0,  0m.L:0,S:1000 CReg:9040 NoPSv:1 PSSt:0,Post:1 PSReg:a004 ClassA:0 
===============================================================
  ===============_display drv phy-esd-status===============
===============================================================
  g_ulESDTestEnableSwitch=1,g_drvESDResetPhyMode=0,PortNumPerScan=1 
 g_drvESDTest_PhyRcvErrRecoverCount[]: 
        0        0    35326        0        0        0        0        0
        0        0        0        0        0        0        0        0
        0        0        0        0        0        0        0        0
        0        0        0        0        0        0        0        0
        0        0        0        0        0        0        0        0
        0        0        0        0        0        0        0        0
        0        0        0        0
 g_drvESDTest_PhyRcvErrReset[]: 
        0        0        1        0        0        0        0        0
        0        0        0        0        0        0        0        0
        0        0        0        0        0        0        0        0
        0        0        0        0        0        0        0        0
        0        0        0        0        0        0        0        0
        0        0        0        0        0        0        0        0
        0        0        0        0
 g_drvESDTest_PhyMdixErrCount[]: 
        0        0        0        0        0        0        0        0
        0        0        0        0        0        0        0        0
        0        0        0        0        0        0        0        0
        0        0        0        0        0        0        0        0
        0        0        0        0        0        0        0        0
        0        0        0        0        0        0        0        0
        0        0        0        0
 g_drvESDTest_PhyPowerdownErrCount[]: 
        0        0        0        0        0        0        0        0
        0        0        0        0        0        0        0        0
        0        0        0        0        0        0        0        0
        0        0        0        0        0        0        0        0
        0        0        0        0        0        0        0        0
        0        0        0        0        0        0        0        0
        0        0        0        0
 g_drvESDTest_PhyRcvErrHwReset[]: 
        0        0        0        0        0        0        0        0
        0        0        0        0        0        0        0        0
        0        0        0        0        0        0        0        0
        0        0        0        0        0        0        0        0
        0        0        0        0        0        0        0        0
        0        0        0        0        0        0        0        0
        0        0        0        0
 g_ulLinkdownPortAutoShutUndoshut:0, g_ulShutUndoShutPortCount[]: 
        0        0        0        0        0        0        0        0
        0        0        0        0        0        0        0        0
        0        0        0        0        0        0        0        0
        0        0        0        0        0        0        0        0
        0        0        0        0        0        0        0        0
        0        0        0        0        0        0        0        0
        0        0        0        0
 g_ulPortLinkHistory[]: 
       45       43       43       40        2        0        0        0
        0        0        0        0        0        0        0        0
        7        7        4        4        2        1        2        1
        0        0        0        0        0        0        0        0
        0        0        0        0        0        0        0        0
        0        0        0        0        0        0       10        0
        0        0        0        0
 PHY chip: g_ulRevNum[]: 
      dc0      dc0      dc0      dc0      dc0      dc0      dc0      dc0
      dc0      dc0      dc0      dc0      dc0      dc0      dc0      dc0
      dc0      dc0      dc0      dc0      dc0      dc0      dc0      dc0
      dc0      dc0      dc0      dc0      dc0      dc0      dc0      dc0
      dc0      dc0      dc0      dc0      dc0      dc0      dc0      dc0
      dc0      dc0      dc0      dc0      dc0      dc0      dc0      dc0
        0        0        0        0
============================================================
  ===============_display drv arp counter===============
============================================================
 ALL ARP entries: 1 
   ARP ONLY entries: 0 
   MAC ARP entries: 1 
=============================================================
  ===============_display drv arp software===============
=============================================================
0  d485644419f0,VLAN0001,DEV0,TRUNK66,ROUTE0,DACMD0,SACMD0,IDX03368,STATUS:MACARP
==========================================================================
  ===============_display drv arp hardware all chipid 0===============
==========================================================================
0 MACd485644419f0,hardindex1,softindex3368
==========================================================================
  ===============_display drv arp hardware all chipid 1===============
==========================================================================
0 MACd485644419f0,hardindex1,softindex3368
==============================================================
  ===============_display drv packet bufcnt===============
==============================================================
Number of buffer allocated ingress
 port01~08: 0003 0003 0003 0003 0003 0003 0003 0003
 port09~16: 0003 0003 0003 0003 0003 0003 0003 0003
 port17~24: 0003 0003 0003 0003 0003 0003 0003 0003
 port25~32: 0003 0003 0003 0003 0003 0003 0003 0003
 port33~40: 0003 0003 0003 0003 0003 0003 0003 0003
 port41~48: 0003 0003 0003 0003 0003 0003 0003 0003
 port49~52: 0003 0003 0003 0003
 ucDev:0 CPU Port buffer allocated  3
 ucDev:1 CPU Port buffer allocated  3
Number of buffer total allocated egress
 ucDev:0 egress buffer total allocated  87
 ucDev:1 egress buffer total allocated  87
The current number of enqueued buffer allocated 
 port01~08: 0000 0000 0000 0000 0000 0000 0000 0000
 port09~16: 0000 0000 0000 0000 0000 0000 0000 0000
 port17~24: 0000 0000 0000 0000 0000 0000 0000 0000
 port25~32: 0000 0000 0000 0000 0000 0000 0000 0000
 port33~40: 0000 0000 0000 0000 0000 0000 0000 0000
 port41~48: 0000 0000 0000 0000 0000 0000 0000 0000
 port49~52: 0000 0000 0000 0000
 ucDev:0 CPU Port enqueued buffer allocated  0
 ucDev:1 CPU Port enqueued buffer allocated  0
 ucDev:0 enqueued buffer total allocated 0
 ucDev:0 total shared buffers 0
 ucDev:1 enqueued buffer total allocated 0
 ucDev:1 total shared buffers 0
ports' queue buffers used
 port01(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port02(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port03(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port04(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port05(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port06(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port07(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port08(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port09(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port10(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port11(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port12(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port13(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port14(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port15(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port16(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port17(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port18(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port19(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port20(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port21(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port22(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port23(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port24(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port25(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port26(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port27(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port28(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port29(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port30(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port31(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port32(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port33(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port34(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port35(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port36(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port37(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port38(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port39(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port40(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port41(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port42(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port43(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port44(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port45(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port46(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port47(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port48(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port49(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port50(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port51(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port52(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
=========================================================================
  ===============_display drv packet descriptor global===============
=========================================================================
ports' descriptors used
 port01~08: 0000 0000 0000 0000 0000 0000 0000 0000
 port09~16: 0000 0000 0000 0000 0000 0000 0000 0000
 port17~24: 0000 0000 0000 0000 0000 0000 0000 0000
 port25~32: 0000 0000 0000 0000 0000 0000 0000 0000
 port33~40: 0000 0000 0000 0000 0000 0000 0000 0000
 port41~48: 0000 0000 0000 0000 0000 0000 0000 0000
 port49~52: 0000 0000 0000 0000
 dev 0 cpu port: 0000
 dev 1 cpu port: 0000
 ucDev:0 descriptors total allocated in the TxQ 0
 ucDev:0 total shared descriptors 0
 ucDev:0 multicast descriptors total allocated 0
 ucDev:0 sniffer descriptors (rx:27-14 tx:13-0 ) 0
 ucDev:1 descriptors total allocated in the TxQ 0
 ucDev:1 total shared descriptors 0
 ucDev:1 multicast descriptors total allocated 0
 ucDev:1 sniffer descriptors (rx:27-14 tx:13-0 ) 0
========================================================================
  ===============_display drv packet descriptor queue===============
========================================================================
ports' queue descriptors used
 port01(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port02(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port03(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port04(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port05(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port06(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port07(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port08(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port09(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port10(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port11(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port12(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port13(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port14(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port15(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port16(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port17(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port18(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port19(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port20(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port21(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port22(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port23(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port24(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port25(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port26(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port27(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port28(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port29(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port30(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port31(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port32(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port33(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port34(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port35(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port36(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port37(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port38(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port39(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port40(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port41(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port42(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port43(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port44(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port45(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port46(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port47(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port48(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port49(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port50(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port51(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 port52(Queue 0~7): 0000 0000 0000 0000 0000 0000 0000 0000
 dev 0 cpu port(Queue 0~7):  0000 0000 0000 0000 0000 0000 0000 0000
 dev 1 cpu port(Queue 0~7):  0000 0000 0000 0000 0000 0000 0000 0000
============================================================
  ===============_display drv ip variable===============
============================================================
<IPv4 Unicast RM Module>
 g_ulDrvIPv4DefaultNextHopId=1
 g_ulDrvIPv4DropNextHopId=2
 g_ulDrvIPv4TrapNextHopId=3
 g_ulDrvIPv4Route2CPUNextHopId=4
 g_ulDrvIPv4UCOutOfPPMem=0
 g_enDrvIPv4SysDefaultRTMode=0, [0-drop, 1-route2cpu, 2-trap]
 g_enDrvIPv4SysRejectRTMode=1, [0-drop, 1-route2cpu]
 g_aulDrvIPv4UCDstCnt[1]=3
<IP NextHop Module>
 g_ulDrvNextHopCnt[0]=5
 g_ulDrvNextHopCnt[1]=5
===================================================================
  ===============_display drv ipv4mc drop_mc_num===============
===================================================================
 Display Current Drop MAC Num :
       g_ulDropMCMacLimit=4000!g_ulDropUnknowMCNum=0!!
==============================================================
  ===============_display drv ipv6 variable===============
==============================================================
 g_ulDrvIPv6DefaultNextHopId=0
 g_ulDrvIPv6DropNextHopId=0
 g_ulDrvIPv6TrapNextHopId=0
 g_ulDrvIPv6Route2CPUNextHopId=0
 g_ulDrvIPv6NDRouteCnt=0
 g_enDrvIPv6SysDefaultRTMode=1 [0-drop,1-route2cpu,2-trap]
 g_aulDrvIPv6UCDstCnt[0]=0
 g_aulDrvIPv6UCDstCnt[1]=0
 g_aulDrvIPv6UCDstCnt[2]=0
 g_aulDrvIPv6UCDstCnt[3]=0
 g_aulDrvIPv6UCDstCnt[4]=0
 g_aulDrvIPv6UCDstCnt[5]=0
 g_aulDrvIPv6UCDstCnt[6]=0
 g_aulDrvIPv6UCDstCnt[7]=0
 g_aulDrvIPv6UCDstCnt[8]=0
 g_aulDrvIPv6UCDstCnt[9]=0
 g_aulDrvIPv6UCDstCnt[10]=0
 g_aulDrvIPv6UCDstCnt[11]=0
 g_aulDrvIPv6UCDstCnt[12]=0
 g_aulDrvIPv6UCDstCnt[13]=0
 g_aulDrvIPv6UCDstCnt[14]=0
 g_aulDrvIPv6UCDstCnt[15]=0
====================================================================
  ===============_display drv l2ingresscfg chip 0===============
====================================================================
====================================================================
  ===============_display drv l2ingresscfg chip 1===============
====================================================================
==========================================================
  ===============_display drv l2mc vidx===============
==========================================================
VIDX Used by: L3      L2      DROP
              0       0       0
=============================================================
  ===============_display drv mac software===============
=============================================================
0  d485645bf6ca,VLAN0001,DEV0,TRUNK68,ROUTE0,DACMD0,SACMD0,IDX02472,STATUS:MAC
1  1cc1de7b226c,VLAN0001,DEV0,TRUNK66,ROUTE0,DACMD0,SACMD0,IDX02928,STATUS:MAC
2  d485644419f0,VLAN0001,DEV0,TRUNK66,ROUTE0,DACMD0,SACMD0,IDX03368,STATUS:MACARP
3  20fdf124480e,VLAN0001,DEV0,CPUPORT,ROUTE1,DACMD0,SACMD0,IDX04552,STATUS:MAC
==========================================================================
  ===============_display drv mac hardware all chipid 0===============
==========================================================================
+++++++++++++++++++++++++++++++++++++++++++++++++++++++

Skip: Skip this entry is used to delete an entry in a hash chain.
        0 = Don't skip this entry.
        1 = Skip this entry.
Route:If the packet's Destination Address matches this entry.
        0 = Disable routing on this packet.
        1 = Enable routing on this packet.
Aging: This bit is used for the two-step Aging process.
        0 = Cleared by the CPU or Aging process.
        1 = When automatically learned, the bit is set to 1
DACMD:Controls the action taken when a packet. Destination Address matches this entry.
        0 = Forward (default for Learned entries)
        1 = Mirror (Mirror to CPU)
        2 = Trap  -(Trap to CPU)
        3 = HardDrop
        4 = SoftDrop
SACMD:Controls the action taken when a packet.Source Address matches this entry.
        0 = Forward (default for Learned entries)
        1 = Mirror (Mirror to CPU)
        2 = Trap  -(Trap to CPU)
        3 = HardDrop
        4 = SoftDrop
+++++++++++++++++++++++++++++++++++++++++++++++++++++++

0 MACd485645bf6ca,VLAN0001,DEV0,TRUNK68,AGE1,SKIP0,ROUTE0,DACMD0,SACMD0,IDX02472
1 MAC1cc1de7b226c,VLAN0001,DEV0,TRUNK66,AGE1,SKIP0,ROUTE0,DACMD0,SACMD0,IDX02928
2 MACd485644419f0,VLAN0001,DEV0,TRUNK66,AGE1,SKIP0,ROUTE0,DACMD0,SACMD0,IDX03368
3 MAC20fdf124480e,VLAN0001,DEV0,CPUPORT,AGE1,SKIP0,ROUTE1,DACMD0,SACMD0,IDX04552
==========================================================================
  ===============_display drv mac hardware all chipid 1===============
==========================================================================
+++++++++++++++++++++++++++++++++++++++++++++++++++++++

Skip: Skip this entry is used to delete an entry in a hash chain.
        0 = Don't skip this entry.
        1 = Skip this entry.
Route:If the packet's Destination Address matches this entry.
        0 = Disable routing on this packet.
        1 = Enable routing on this packet.
Aging: This bit is used for the two-step Aging process.
        0 = Cleared by the CPU or Aging process.
        1 = When automatically learned, the bit is set to 1
DACMD:Controls the action taken when a packet. Destination Address matches this entry.
        0 = Forward (default for Learned entries)
        1 = Mirror (Mirror to CPU)
        2 = Trap  -(Trap to CPU)
        3 = HardDrop
        4 = SoftDrop
SACMD:Controls the action taken when a packet.Source Address matches this entry.
        0 = Forward (default for Learned entries)
        1 = Mirror (Mirror to CPU)
        2 = Trap  -(Trap to CPU)
        3 = HardDrop
        4 = SoftDrop
+++++++++++++++++++++++++++++++++++++++++++++++++++++++

0 MACd485645bf6ca,VLAN0001,DEV1,TRUNK68,AGE1,SKIP0,ROUTE0,DACMD0,SACMD0,IDX02472
1 MAC1cc1de7b226c,VLAN0001,DEV1,TRUNK66,AGE1,SKIP0,ROUTE0,DACMD0,SACMD0,IDX02928
2 MACd485644419f0,VLAN0001,DEV1,TRUNK66,AGE1,SKIP0,ROUTE0,DACMD0,SACMD0,IDX03368
3 MAC20fdf124480e,VLAN0001,DEV0,CPUPORT,AGE1,SKIP0,ROUTE1,DACMD0,SACMD0,IDX04552
================================================================
  ===============_display drv mac_learn_state===============
================================================================
-----------------------------------------------------
Mac learning state in all Ports
 H(Hardware automatic learning) S(Software learning) 
-----------------------------------------------------
  1 S  2 S  3 S  4 S  5 S  6 S  7 S  8 S  9 S 10 S
 11 S 12 S 13 S 14 S 15 S 16 S 17 S 18 S 19 S 20 S
 21 S 22 S 23 S 24 S 25 S 26 S 27 S 28 S 29 S 30 S
 31 S 32 S 33 S 34 S 35 S 36 S 37 S 38 S 39 S 40 S
 41 S 42 S 43 S 44 S 45 S 46 S 47 S 48 S 49 S 50 S
 51 S 52 S
================================================================
  ===============_display drv macrange-filter===============
================================================================
This device do not support mac range filter!
===========================================================
  ===============_display drv mc_mac all===============
===========================================================


  No MAC address found.
=============================================================================
  ===============_display drv mirror-entry chip 0 hardware===============
=============================================================================
=============================================================================
  ===============_display drv mirror-entry chip 0 software===============
=============================================================================

  Inboud Mirror Port: 

  Outboud Mirror Port: 

  Inboud Monitor Port:     NULL      Outboud Monitor Port:     NULL  
=============================================================================
  ===============_display drv mirror-entry chip 1 hardware===============
=============================================================================
=============================================================================
  ===============_display drv mirror-entry chip 1 software===============
=============================================================================

  Inboud Mirror Port: 

  Outboud Mirror Port: 

  Inboud Monitor Port:     NULL      Outboud Monitor Port:     NULL  
=============================================================
  ===============_display drv port-isolate===============
=============================================================
*** software info ***

*** hardware info ***
============================================================
  ===============_display drv reboot-type===============
============================================================
 The rebooting type this time is: Cold reboot 
=======================================================
  ===============display reboot-type===============
=======================================================
  The rebooting type this time is: Cold
=================================================================
  ===============_display drv register cpld 24===============
=================================================================
 CPLD register Informaition
g_stProductInfo: Addr 0226ba8c
: szDefaultHostName 3Com Baseline Switch
: szDefaultCfgFile startup.cfg
: szFactoryDefaultCfgFile startup.cfg
: szProductVersion Release 1101P10
: szProductInternalVersion V100R002B03D007SP01
: szCorporation 3com
: szReleaseVersion ##1##
: szProductVersionForMib 5.20 Release 1101P10
: szSoftwareVersionForMib 5.20 Release 1101P10
: szLswReleaseVersion Release 1101P10
: szCopyrightTime 1998-2009
: szVersionProduct Switch 2900 Plus
: szPhysicalModelName 3CRBSG5293
: szWebPrefix s3v
: szWebFile ##2##
: szProductName 2952-SFP Plus
: szHGMPProductName 
: usDeviceOID 73
: usObjectID: 1.3.6.1.4.1.43.1.8.0.0.
: ucOidLen 10
: ucPwrNum 1
: ucFanNum 1
: ucDevicePortNum 52
: ucMACChipNum 2
: enOEMCorpID 1
: szDevicePortsString 48GE+4SFP
: enProductType 2
: enBoardType 2
: szBoardType LS51LTSS
: ulIsPoE 0
 g_ulCpldPhaseFlag: 1 
 g_ucSysmBootData: 0x04 
 g_ucWatchDogDefaultData: 0x07 
 g_ulIsNotComboTypeDevice: 0x01 
 g_mac_revision_A0A1: 0x2 
 g_ucPoeVendorId: 0x1 
 g_ulTopMemStartAddr: 0x7c00000 
 g_ulProductInit_Flag: 0x1 
Port 0 02400002 02400002 02400002 02400002 02400000 02400000 02400000 02400000 
Port 8 02400000 02400000 02400000 02400000 02400000 02400000 02400000 02400000 
Port16 02400002 02400002 02400002 02400002 02400000 02400000 02400000 02400000 
Port24 02400000 02400000 02400000 02400000 02400000 02400000 02400000 02400000 
Port32 02400000 02400000 02400000 02400000 02400000 02400000 02400000 02400000 
Port40 02400000 02400000 02400000 02400000 02400000 02400000 02400000 02400000 
Port48 00000000 00000000 00000000 00000000 
 g_szCurrentMainBootFile: flash:/S2900-CMW520-R1101P10.bin 
 g_ucSysmDeviceType: 2 
 g_ucBoardType: 2 
 g_stDeviceConfig:usArpNum 256 
 g_stDeviceConfig:usNextHopNum 256 
 g_stDeviceConfig:usIpv4MCNum 0 
 g_stDeviceConfig:usIpv4PrefixNum 50 
 g_stDeviceConfig:usIpv6PrefixNum 0 
 g_stDeviceConfig:usNumOfMLL 0 
 g_stDeviceConfig:usTunnelEntries 0 
 g_stDeviceConfig:usIpv4TunnelTerms 0 
 g_stDeviceConfig:usTcEntries 256 
 g_stDeviceConfig:usPclActions 256 
 g_stDeviceConfig:usPclSize 256 
 g_stDeviceConfig:usPces 256 
 g_stDeviceConfig:usAclNum 256 
 g_stDeviceConfig:usCarNum 256 
 g_stDeviceConfig:usVlanNum 256 
 g_stDeviceConfig:usVRFNum 0 
 g_stDeviceConfig:eInlifType 1 
 g_stDeviceConfig:usValid 1 
 g_stDeviceConfig:usNarrowSram 1 
 g_ulCPLDModeTest 1 
 Stacking Ports ReConf Num: 0 
 g_ulPseRecoverTims: 0 
=================================================================
  ===============_display drv register cpld 25===============
=================================================================
 CPLD register Informaition
 DRV_REC_FLAG_S stFlashFlag Len:180 
0x0000:1d 4d 00 00 00 00 00 00 07 00 00 00 ff ff ff ff  .M..............
0x0010:01 00 00 00 00 00 00 00 00 00 00 00 59 00 00 00  ............Y...
0x0020:59 00 00 00 59 00 00 00 59 00 00 00 00 00 00 00  Y...Y...Y.......
0x0030:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x0040:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x0050:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x0060:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x0070:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x0080:00 00 00 00 00 00 00 00 00 00 00 00 13 00 01 00  ................
0x0090:13 00 01 00 59 00 00 00 59 00 00 00 ff 00 00 00  ....Y...Y.......
0x00a0:ff 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x00b0:00 00 00 00   ....
 DRV_REC_DIMG_S stFlashDimg Len:924 
0x0000:c6 31 00 00 66 6c 61 73 68 3a 2f 53 32 39 30 30  .1..flash:/S2900
0x0010:2d 43 4d 57 35 32 30 2d 52 31 31 30 31 50 31 30  -CMW520-R1101P10
0x0020:2e 62 69 6e 00 6e 00 00 00 00 00 00 00 00 00 00  .bin.n..........
0x0030:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x0040:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x0050:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x0060:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x0070:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x0080:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x0090:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x00a0:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x00b0:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x00c0:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x00d0:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x00e0:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x00f0:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x0100:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x0110:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x0120:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x0130:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x0140:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x0150:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x0160:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x0170:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x0180:00 00 00 00 66 6c 61 73 68 3a 2f 73 74 61 72 74  ....flash:/start
0x0190:75 70 2e 63 66 67 00 00 00 00 00 00 00 00 00 00  up.cfg..........
0x01a0:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x01b0:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x01c0:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x01d0:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x01e0:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x01f0:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x0200:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x0210:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x0220:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x0230:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x0240:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x0250:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x0260:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x0270:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x0280:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x0290:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x02a0:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x02b0:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x02c0:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x02d0:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x02e0:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x02f0:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x0300:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x0310:00 00 00 00 00 00 00 00 00 00 00 00 ff ff ff ff  ................
0x0320:ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff  ................
0x0330:ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff  ................
0x0340:ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff  ................
0x0350:ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff  ................
0x0360:ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff  ................
0x0370:ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff  ................
0x0380:ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff  ................
0x0390:ff ff ff ff ff ff ff ff ff ff ff ff   ............
 DRV_REC_DATA_S stFlashData Len:340 
0x0000:33 59 00 00 00 e0 fc 00 36 20 00 00 00 00 00 00  3Y......6 ......
0x0010:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x0020:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x0030:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x0040:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x0050:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x0060:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x0070:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x0080:00 00 00 00 80 25 00 00 00 00 00 00 00 00 00 00  .....%..........
0x0090:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x00a0:00 00 00 00 02 00 00 00 00 00 00 00 00 00 00 00  ................
0x00b0:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x00c0:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x00d0:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x00e0:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x00f0:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x0100:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x0110:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x0120:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x0130:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x0140:00 00 00 00 01 5a 00 5a 0a 5a 00 00 00 00 00 00  .....Z.Z.Z......
0x0150:00 00 00 00   ....
 DRV_REC_MANU_S stFlashManu Len:964 
0x0000:4a cf 00 00 37 f0 48 a5 33 43 52 42 53 47 35 32  J...7.H.3CRBSG52
0x0010:39 33 00 00 00 00 00 00 00 00 00 00 00 00 00 00  93..............
0x0020:00 00 00 00 00 00 00 00 39 32 37 46 44 43 53 32  ........927FDCS2
0x0030:34 34 38 30 44 00 00 00 00 00 00 00 00 00 00 00  4480D...........
0x0040:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x0050:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x0060:00 00 00 00 00 00 00 00 20 fd f1 24 48 0d 32 34  ........ ..$H.24
0x0070:34 38 30 44 00 00 00 00 00 00 00 00 00 00 00 00  480D............
0x0080:00 00 00 00 00 00 00 00 32 30 31 30 2d 31 31 2d  ........2010-11-
0x0090:31 35 00 00 00 00 00 00 00 00 00 00 00 00 00 00  15..............
0x00a0:00 00 00 00 00 00 00 00 33 43 4f 4d 00 00 00 00  ........3COM....
0x00b0:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x00c0:00 00 00 00 00 00 00 00 39 32 37 46 44 43 53 32  ........927FDCS2
0x00d0:34 34 38 30 44 00 00 00 00 00 00 00 00 00 00 00  4480D...........
0x00e0:00 00 00 00 00 00 00 00 4e 4f 4e 45 00 00 00 00  ........NONE....
0x00f0:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x0100:00 00 00 00 00 00 00 00 30 30 2e 30 30 2e 30 30  ........00.00.00
0x0110:01 00 00 00 3a 00 00 00 30 32 33 35 41 34 31 56  ....:...0235A41V
0x0120:00 00 00 00 00 00 00 00 39 32 37 46 44 43 53 32  ........927FDCS2
0x0130:34 34 38 30 44 00 00 00 00 00 00 00 00 00 00 00  4480D...........
0x0140:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x0150:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x0160:00 00 00 00 00 00 00 00 99 00 00 00 00 00 00 00  ................
0x0170:31 30 39 20 30 31 3a 31 30 39 20 30 32 00 00 00  109 01:109 02...
0x0180:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x0190:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x01a0:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x01b0:02 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x01c0:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x01d0:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x01e0:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x01f0:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x0200:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x0210:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x0220:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x0230:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x0240:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x0250:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x0260:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x0270:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x0280:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x0290:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x02a0:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x02b0:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x02c0:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x02d0:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x02e0:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x02f0:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x0300:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x0310:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x0320:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x0330:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x0340:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x0350:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x0360:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x0370:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x0380:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x0390:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x03a0:00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  ................
0x03b0:00 00 00 00 00 00 00 00 35 41 35 41 35 41 35 41  ........5A5A5A5A
0x03c0:01 00 00 00   ....
=================================================================
  ===============_display drv register cpld 26===============
=================================================================
 CPLD register Informaition
 Port  3 temperature:  55 0x1910 ulRet: 0 
 Port  7 temperature:  35 0x190c ulRet: 0 
 Port 11 temperature:  40 0x190d ulRet: 0 
 Port 15 temperature:  40 0x190d ulRet: 0 
 Port 19 temperature:  35 0x190c ulRet: 0 
 Port 23 temperature:  45 0x190e ulRet: 0 
 Port 27 temperature:  40 0x190d ulRet: 0 
 Port 31 temperature:  40 0x190d ulRet: 0 
 Port 35 temperature:  35 0x190c ulRet: 0 
 Port 39 temperature:  35 0x190c ulRet: 0 
 Port 43 temperature:  35 0x190c ulRet: 0 
 Port 47 temperature:  30 0x190b ulRet: 0 
=================================================================
  ===============_display drv register cpld 34===============
=================================================================
 CPLD register Informaition
 drv_NandFlashBlockScan : 
   Nand ID = 0x20 
   0: 0  3 ff ff ff ff ff ff  1  2  4  5 ff ff ff ff 
  16:ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff 
  32:ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff 
  48:ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff 
  64:ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff 
  80:ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff 
  96:ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff 
 112:ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff 
 128:ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff 
 144:ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff 
 160:ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff 
 176:ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff 
 192:ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff 
 208:ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff 
 224:ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff 
 240:ff ff ff ff ff ff ff ff ff  X ff ff ff ff ff ff 
===========================================================
  ===============_display drv revisionid===============
===========================================================
              chip 0  chip 1 
===============================================
Revision         A2    A2 
=====================================================
  ===============_display drv rrpp===============
=====================================================
 GigabitEthernet1/0/1      RRPP enable status is Disable
 GigabitEthernet1/0/2      RRPP enable status is Disable
 GigabitEthernet1/0/3      RRPP enable status is Disable
 GigabitEthernet1/0/4      RRPP enable status is Disable
 GigabitEthernet1/0/5      RRPP enable status is Disable
 GigabitEthernet1/0/6      RRPP enable status is Disable
 GigabitEthernet1/0/7      RRPP enable status is Disable
 GigabitEthernet1/0/8      RRPP enable status is Disable
 GigabitEthernet1/0/9      RRPP enable status is Disable
 GigabitEthernet1/0/10     RRPP enable status is Disable
 GigabitEthernet1/0/11     RRPP enable status is Disable
 GigabitEthernet1/0/12     RRPP enable status is Disable
 GigabitEthernet1/0/13     RRPP enable status is Disable
 GigabitEthernet1/0/14     RRPP enable status is Disable
 GigabitEthernet1/0/15     RRPP enable status is Disable
 GigabitEthernet1/0/16     RRPP enable status is Disable
 GigabitEthernet1/0/17     RRPP enable status is Disable
 GigabitEthernet1/0/18     RRPP enable status is Disable
 GigabitEthernet1/0/19     RRPP enable status is Disable
 GigabitEthernet1/0/20     RRPP enable status is Disable
 GigabitEthernet1/0/21     RRPP enable status is Disable
 GigabitEthernet1/0/22     RRPP enable status is Disable
 GigabitEthernet1/0/23     RRPP enable status is Disable
 GigabitEthernet1/0/24     RRPP enable status is Disable
 GigabitEthernet1/0/25     RRPP enable status is Disable
 GigabitEthernet1/0/26     RRPP enable status is Disable
 GigabitEthernet1/0/27     RRPP enable status is Disable
 GigabitEthernet1/0/28     RRPP enable status is Disable
 GigabitEthernet1/0/29     RRPP enable status is Disable
 GigabitEthernet1/0/30     RRPP enable status is Disable
 GigabitEthernet1/0/31     RRPP enable status is Disable
 GigabitEthernet1/0/32     RRPP enable status is Disable
 GigabitEthernet1/0/33     RRPP enable status is Disable
 GigabitEthernet1/0/34     RRPP enable status is Disable
 GigabitEthernet1/0/35     RRPP enable status is Disable
 GigabitEthernet1/0/36     RRPP enable status is Disable
 GigabitEthernet1/0/37     RRPP enable status is Disable
 GigabitEthernet1/0/38     RRPP enable status is Disable
 GigabitEthernet1/0/39     RRPP enable status is Disable
 GigabitEthernet1/0/40     RRPP enable status is Disable
 GigabitEthernet1/0/41     RRPP enable status is Disable
 GigabitEthernet1/0/42     RRPP enable status is Disable
 GigabitEthernet1/0/43     RRPP enable status is Disable
 GigabitEthernet1/0/44     RRPP enable status is Disable
 GigabitEthernet1/0/45     RRPP enable status is Disable
 GigabitEthernet1/0/46     RRPP enable status is Disable
 GigabitEthernet1/0/47     RRPP enable status is Disable
 GigabitEthernet1/0/48     RRPP enable status is Disable
 GigabitEthernet1/0/49     RRPP enable status is Disable
 GigabitEthernet1/0/50     RRPP enable status is Disable
 GigabitEthernet1/0/51     RRPP enable status is Disable
 GigabitEthernet1/0/52     RRPP enable status is Disable
===============================================================
  ===============_display drv stp instance 0===============
===============================================================
In STP instance 0 All Ports' state
 D(Disable) B(Block) L(Learn) F(Forward)
-----------------------------------------------------
  1 B  2 B  3 B  4 B  5 B  6 B  7 B  8 B  9 B 10 B
 11 B 12 B 13 B 14 B 15 B 16 B 17 B 18 B 19 B 20 B
 21 B 22 B 23 B 24 B 25 B 26 B 27 B 28 B 29 B 30 B
 31 B 32 B 33 B 34 B 35 B 36 B 37 B 38 B 39 B 40 B
 41 B 42 B 43 B 44 B 45 B 46 B 47 B 48 B 49 B 50 B
 51 B 52 B
===============================================================
  ===============_display drv stp instance 1===============
===============================================================
In STP instance 1 All Ports' state
 D(Disable) B(Block) L(Learn) F(Forward)
-----------------------------------------------------
  1 F  2 F  3 F  4 F  5 B  6 B  7 B  8 B  9 B 10 B
 11 B 12 B 13 B 14 B 15 B 16 B 17 B 18 B 19 B 20 B
 21 B 22 B 23 B 24 B 25 B 26 B 27 B 28 B 29 B 30 B
 31 B 32 B 33 B 34 B 35 B 36 B 37 B 38 B 39 B 40 B
 41 B 42 B 43 B 44 B 45 B 46 B 47 B 48 B 49 B 50 B
 51 B 52 B
===============================================================
  ===============_display drv stp instance 2===============
===============================================================
In STP instance 2 All Ports' state
 D(Disable) B(Block) L(Learn) F(Forward)
-----------------------------------------------------
  1 B  2 B  3 B  4 B  5 B  6 B  7 B  8 B  9 B 10 B
 11 B 12 B 13 B 14 B 15 B 16 B 17 B 18 B 19 B 20 B
 21 B 22 B 23 B 24 B 25 B 26 B 27 B 28 B 29 B 30 B
 31 B 32 B 33 B 34 B 35 B 36 B 37 B 38 B 39 B 40 B
 41 B 42 B 43 B 44 B 45 B 46 B 47 B 48 B 49 B 50 B
 51 B 52 B
===============================================================
  ===============_display drv stp instance 3===============
===============================================================
In STP instance 3 All Ports' state
 D(Disable) B(Block) L(Learn) F(Forward)
-----------------------------------------------------
  1 B  2 B  3 B  4 B  5 B  6 B  7 B  8 B  9 B 10 B
 11 B 12 B 13 B 14 B 15 B 16 B 17 B 18 B 19 B 20 B
 21 B 22 B 23 B 24 B 25 B 26 B 27 B 28 B 29 B 30 B
 31 B 32 B 33 B 34 B 35 B 36 B 37 B 38 B 39 B 40 B
 41 B 42 B 43 B 44 B 45 B 46 B 47 B 48 B 49 B 50 B
 51 B 52 B
===============================================================
  ===============_display drv stp instance 4===============
===============================================================
In STP instance 4 All Ports' state
 D(Disable) B(Block) L(Learn) F(Forward)
-----------------------------------------------------
  1 B  2 B  3 B  4 B  5 B  6 B  7 B  8 B  9 B 10 B
 11 B 12 B 13 B 14 B 15 B 16 B 17 B 18 B 19 B 20 B
 21 B 22 B 23 B 24 B 25 B 26 B 27 B 28 B 29 B 30 B
 31 B 32 B 33 B 34 B 35 B 36 B 37 B 38 B 39 B 40 B
 41 B 42 B 43 B 44 B 45 B 46 B 47 B 48 B 49 B 50 B
 51 B 52 B
===============================================================
  ===============_display drv stp instance 5===============
===============================================================
In STP instance 5 All Ports' state
 D(Disable) B(Block) L(Learn) F(Forward)
-----------------------------------------------------
  1 F  2 F  3 F  4 F  5 F  6 D  7 D  8 D  9 D 10 D
 11 D 12 D 13 D 14 D 15 D 16 D 17 B 18 B 19 B 20 B
 21 F 22 F 23 F 24 F 25 D 26 D 27 D 28 D 29 D 30 D
 31 D 32 D 33 D 34 D 35 D 36 D 37 D 38 D 39 D 40 D
 41 D 42 D 43 D 44 D 45 D 46 D 47 F 48 D 49 D 50 D
 51 D 52 D
=======================================================
  ===============display stp history===============
=======================================================
===============================================
  ===============display stp===============
===============================================
-------[CIST Global Info][Mode RSTP]-------
CIST Bridge         :32768.20fd-f124-480d
Bridge Times        :Hello 2s MaxAge 20s FwDly 15s MaxHop 20
CIST Root/ERPC      :32768.20fd-f124-480d / 0
CIST RegRoot/IRPC   :32768.20fd-f124-480d / 0
CIST RootPortId     :0.0
BPDU-Protection     :disabled
Bridge Config-             
Digest-Snooping     :disabled
TC or TCN received  :0
Time since last TC  :0 days 0h:16m:50s

----[Port53(Bridge-Aggregation1)][FORWARDING]----
 Port Protocol       :enabled
 Port Role           :CIST Designated Port
 Port Priority       :128
 Port Cost(Legacy)   :Config=auto / Active=18
 Desg. Bridge/Port   :32768.20fd-f124-480d / 128.53
 Port Edged          :Config=disabled / Active=disabled
 Point-to-point      :Config=auto / Active=true
 Transmit Limit      :10 packets/hello-time
 Protection Type     :None
 MST BPDU Format     :Config=auto / Active=legacy
 Port Config-             
 Digest-Snooping     :disabled
 Rapid transition    :false
 Num of Vlans Mapped :1 
 PortTimes           :Hello 2s MaxAge 20s FwDly 15s MsgAge 0s RemHop 20
 BPDU Sent           :3534             
          TCN: 0, Config: 0, RST: 3534, MST: 0
 BPDU Received       :0             
          TCN: 0, Config: 0, RST: 0, MST: 0

----[Port54(Bridge-Aggregation2)][FORWARDING]----
 Port Protocol       :enabled
 Port Role           :CIST Designated Port
 Port Priority       :128
 Port Cost(Legacy)   :Config=auto / Active=18
 Desg. Bridge/Port   :32768.20fd-f124-480d / 128.54
 Port Edged          :Config=disabled / Active=disabled
 Point-to-point      :Config=auto / Active=true
 Transmit Limit      :10 packets/hello-time
 Protection Type     :None
 MST BPDU Format     :Config=auto / Active=legacy
 Port Config-             
 Digest-Snooping     :disabled
 Rapid transition    :false
 Num of Vlans Mapped :1 
 PortTimes           :Hello 2s MaxAge 20s FwDly 15s MsgAge 0s RemHop 20
 BPDU Sent           :521             
          TCN: 0, Config: 0, RST: 521, MST: 0
 BPDU Received       :0             
          TCN: 0, Config: 0, RST: 0, MST: 0

----[Port1(GigabitEthernet1/0/1)][DOWN]----
 Port Protocol       :enabled
 Port Role           :CIST Disabled Port
 Port Priority       :128
 Port Cost(Legacy)   :Config=auto / Active=200000
 Desg. Bridge/Port   :32768.20fd-f124-480d / 128.1
 Port Edged          :Config=enabled / Active=enabled
 Point-to-point      :Config=auto / Active=false
 Transmit Limit      :10 packets/hello-time
 Protection Type     :None
 MST BPDU Format     :Config=auto / Active=legacy
 Port Config-             
 Digest-Snooping     :disabled
 Rapid transition    :true
 Num of Vlans Mapped :1 
 PortTimes           :Hello 2s MaxAge 20s FwDly 15s MsgAge 0s RemHop 20
 BPDU Sent           :116             
          TCN: 0, Config: 0, RST: 116, MST: 0
 BPDU Received       :0             
          TCN: 0, Config: 0, RST: 0, MST: 0

----[Port2(GigabitEthernet1/0/2)][DOWN]----
 Port Protocol       :enabled
 Port Role           :CIST Disabled Port
 Port Priority       :128
 Port Cost(Legacy)   :Config=auto / Active=200000
 Desg. Bridge/Port   :32768.20fd-f124-480d / 128.2
 Port Edged          :Config=enabled / Active=enabled
 Point-to-point      :Config=auto / Active=false
 Transmit Limit      :10 packets/hello-time
 Protection Type     :None
 MST BPDU Format     :Config=auto / Active=legacy
 Port Config-             
 Digest-Snooping     :disabled
 Rapid transition    :true
 Num of Vlans Mapped :1 
 PortTimes           :Hello 2s MaxAge 20s FwDly 15s MsgAge 0s RemHop 20
 BPDU Sent           :116             
          TCN: 0, Config: 0, RST: 116, MST: 0
 BPDU Received       :0             
          TCN: 0, Config: 0, RST: 0, MST: 0

----[Port3(GigabitEthernet1/0/3)][DOWN]----
 Port Protocol       :enabled
 Port Role           :CIST Disabled Port
 Port Priority       :128
 Port Cost(Legacy)   :Config=auto / Active=200000
 Desg. Bridge/Port   :32768.20fd-f124-480d / 128.3
 Port Edged          :Config=enabled / Active=enabled
 Point-to-point      :Config=auto / Active=false
 Transmit Limit      :10 packets/hello-time
 Protection Type     :None
 MST BPDU Format     :Config=auto / Active=legacy
 Port Config-             
 Digest-Snooping     :disabled
 Rapid transition    :true
 Num of Vlans Mapped :1 
 PortTimes           :Hello 2s MaxAge 20s FwDly 15s MsgAge 0s RemHop 20
 BPDU Sent           :143             
          TCN: 0, Config: 0, RST: 143, MST: 0
 BPDU Received       :0             
          TCN: 0, Config: 0, RST: 0, MST: 0

----[Port4(GigabitEthernet1/0/4)][DOWN]----
 Port Protocol       :enabled
 Port Role           :CIST Disabled Port
 Port Priority       :128
 Port Cost(Legacy)   :Config=auto / Active=200000
 Desg. Bridge/Port   :32768.20fd-f124-480d / 128.4
 Port Edged          :Config=enabled / Active=enabled
 Point-to-point      :Config=auto / Active=false
 Transmit Limit      :10 packets/hello-time
 Protection Type     :None
 MST BPDU Format     :Config=auto / Active=legacy
 Port Config-             
 Digest-Snooping     :disabled
 Rapid transition    :true
 Num of Vlans Mapped :1 
 PortTimes           :Hello 2s MaxAge 20s FwDly 15s MsgAge 0s RemHop 20
 BPDU Sent           :143             
          TCN: 0, Config: 0, RST: 143, MST: 0
 BPDU Received       :0             
          TCN: 0, Config: 0, RST: 0, MST: 0

----[Port5(GigabitEthernet1/0/5)][DOWN]----
 Port Protocol       :enabled
 Port Role           :CIST Disabled Port
 Port Priority       :128
 Port Cost(Legacy)   :Config=auto / Active=200000
 Desg. Bridge/Port   :32768.20fd-f124-480d / 128.5
 Port Edged          :Config=enabled / Active=enabled
 Point-to-point      :Config=auto / Active=false
 Transmit Limit      :10 packets/hello-time
 Protection Type     :None
 MST BPDU Format     :Config=auto / Active=legacy
 Port Config-             
 Digest-Snooping     :disabled
 Rapid transition    :true
 Num of Vlans Mapped :1 
 PortTimes           :Hello 2s MaxAge 20s FwDly 15s MsgAge 0s RemHop 20
 BPDU Sent           :37             
          TCN: 0, Config: 0, RST: 37, MST: 0
 BPDU Received       :0             
          TCN: 0, Config: 0, RST: 0, MST: 0

----[Port6(GigabitEthernet1/0/6)][DOWN]----
 Port Protocol       :enabled
 Port Role           :CIST Disabled Port
 Port Priority       :128
 Port Cost(Legacy)   :Config=auto / Active=200000
 Desg. Bridge/Port   :32768.20fd-f124-480d / 128.6
 Port Edged          :Config=enabled / Active=enabled
 Point-to-point      :Config=auto / Active=false
 Transmit Limit      :10 packets/hello-time
 Protection Type     :None
 MST BPDU Format     :Config=auto / Active=legacy
 Port Config-             
 Digest-Snooping     :disabled
 Num of Vlans Mapped :1 
 PortTimes           :Hello 2s MaxAge 20s FwDly 15s MsgAge 0s RemHop 20
 BPDU Sent           :0             
          TCN: 0, Config: 0, RST: 0, MST: 0
 BPDU Received       :0             
          TCN: 0, Config: 0, RST: 0, MST: 0

----[Port7(GigabitEthernet1/0/7)][DOWN]----
 Port Protocol       :enabled
 Port Role           :CIST Disabled Port
 Port Priority       :128
 Port Cost(Legacy)   :Config=auto / Active=200000
 Desg. Bridge/Port   :32768.20fd-f124-480d / 128.7
 Port Edged          :Config=enabled / Active=enabled
 Point-to-point      :Config=auto / Active=false
 Transmit Limit      :10 packets/hello-time
 Protection Type     :None
 MST BPDU Format     :Config=auto / Active=legacy
 Port Config-             
 Digest-Snooping     :disabled
 Num of Vlans Mapped :1 
 PortTimes           :Hello 2s MaxAge 20s FwDly 15s MsgAge 0s RemHop 20
 BPDU Sent           :0             
          TCN: 0, Config: 0, RST: 0, MST: 0
 BPDU Received       :0             
          TCN: 0, Config: 0, RST: 0, MST: 0

----[Port8(GigabitEthernet1/0/8)][DOWN]----
 Port Protocol       :enabled
 Port Role           :CIST Disabled Port
 Port Priority       :128
 Port Cost(Legacy)   :Config=auto / Active=200000
 Desg. Bridge/Port   :32768.20fd-f124-480d / 128.8
 Port Edged          :Config=enabled / Active=enabled
 Point-to-point      :Config=auto / Active=false
 Transmit Limit      :10 packets/hello-time
 Protection Type     :None
 MST BPDU Format     :Config=auto / Active=legacy
 Port Config-             
 Digest-Snooping     :disabled
 Num of Vlans Mapped :1 
 PortTimes           :Hello 2s MaxAge 20s FwDly 15s MsgAge 0s RemHop 20
 BPDU Sent           :0             
          TCN: 0, Config: 0, RST: 0, MST: 0
 BPDU Received       :0             
          TCN: 0, Config: 0, RST: 0, MST: 0

----[Port9(GigabitEthernet1/0/9)][DOWN]----
 Port Protocol       :enabled
 Port Role           :CIST Disabled Port
 Port Priority       :128
 Port Cost(Legacy)   :Config=auto / Active=200000
 Desg. Bridge/Port   :32768.20fd-f124-480d / 128.9
 Port Edged          :Config=enabled / Active=enabled
 Point-to-point      :Config=auto / Active=false
 Transmit Limit      :10 packets/hello-time
 Protection Type     :None
 MST BPDU Format     :Config=auto / Active=legacy
 Port Config-             
 Digest-Snooping     :disabled
 Num of Vlans Mapped :1 
 PortTimes           :Hello 2s MaxAge 20s FwDly 15s MsgAge 0s RemHop 20
 BPDU Sent           :0             
          TCN: 0, Config: 0, RST: 0, MST: 0
 BPDU Received       :0             
          TCN: 0, Config: 0, RST: 0, MST: 0

----[Port10(GigabitEthernet1/0/10)][DOWN]----
 Port Protocol       :enabled
 Port Role           :CIST Disabled Port
 Port Priority       :128
 Port Cost(Legacy)   :Config=auto / Active=200000
 Desg. Bridge/Port   :32768.20fd-f124-480d / 128.10
 Port Edged          :Config=enabled / Active=enabled
 Point-to-point      :Config=auto / Active=false
 Transmit Limit      :10 packets/hello-time
 Protection Type     :None
 MST BPDU Format     :Config=auto / Active=legacy
 Port Config-             
 Digest-Snooping     :disabled
 Num of Vlans Mapped :1 
 PortTimes           :Hello 2s MaxAge 20s FwDly 15s MsgAge 0s RemHop 20
 BPDU Sent           :0             
          TCN: 0, Config: 0, RST: 0, MST: 0
 BPDU Received       :0             
          TCN: 0, Config: 0, RST: 0, MST: 0

----[Port11(GigabitEthernet1/0/11)][DOWN]----
 Port Protocol       :enabled
 Port Role           :CIST Disabled Port
 Port Priority       :128
 Port Cost(Legacy)   :Config=auto / Active=200000
 Desg. Bridge/Port   :32768.20fd-f124-480d / 128.11
 Port Edged          :Config=enabled / Active=enabled
 Point-to-point      :Config=auto / Active=false
 Transmit Limit      :10 packets/hello-time
 Protection Type     :None
 MST BPDU Format     :Config=auto / Active=legacy
 Port Config-             
 Digest-Snooping     :disabled
 Num of Vlans Mapped :1 
 PortTimes           :Hello 2s MaxAge 20s FwDly 15s MsgAge 0s RemHop 20
 BPDU Sent           :0             
          TCN: 0, Config: 0, RST: 0, MST: 0
 BPDU Received       :0             
          TCN: 0, Config: 0, RST: 0, MST: 0

----[Port12(GigabitEthernet1/0/12)][DOWN]----
 Port Protocol       :enabled
 Port Role           :CIST Disabled Port
 Port Priority       :128
 Port Cost(Legacy)   :Config=auto / Active=200000
 Desg. Bridge/Port   :32768.20fd-f124-480d / 128.12
 Port Edged          :Config=enabled / Active=enabled
 Point-to-point      :Config=auto / Active=false
 Transmit Limit      :10 packets/hello-time
 Protection Type     :None
 MST BPDU Format     :Config=auto / Active=legacy
 Port Config-             
 Digest-Snooping     :disabled
 Num of Vlans Mapped :1 
 PortTimes           :Hello 2s MaxAge 20s FwDly 15s MsgAge 0s RemHop 20
 BPDU Sent           :0             
          TCN: 0, Config: 0, RST: 0, MST: 0
 BPDU Received       :0             
          TCN: 0, Config: 0, RST: 0, MST: 0

----[Port13(GigabitEthernet1/0/13)][DOWN]----
 Port Protocol       :enabled
 Port Role           :CIST Disabled Port
 Port Priority       :128
 Port Cost(Legacy)   :Config=auto / Active=200000
 Desg. Bridge/Port   :32768.20fd-f124-480d / 128.13
 Port Edged          :Config=enabled / Active=enabled
 Point-to-point      :Config=auto / Active=false
 Transmit Limit      :10 packets/hello-time
 Protection Type     :None
 MST BPDU Format     :Config=auto / Active=legacy
 Port Config-             
 Digest-Snooping     :disabled
 Num of Vlans Mapped :1 
 PortTimes           :Hello 2s MaxAge 20s FwDly 15s MsgAge 0s RemHop 20
 BPDU Sent           :0             
          TCN: 0, Config: 0, RST: 0, MST: 0
 BPDU Received       :0             
          TCN: 0, Config: 0, RST: 0, MST: 0

----[Port14(GigabitEthernet1/0/14)][DOWN]----
 Port Protocol       :enabled
 Port Role           :CIST Disabled Port
 Port Priority       :128
 Port Cost(Legacy)   :Config=auto / Active=200000
 Desg. Bridge/Port   :32768.20fd-f124-480d / 128.14
 Port Edged          :Config=enabled / Active=enabled
 Point-to-point      :Config=auto / Active=false
 Transmit Limit      :10 packets/hello-time
 Protection Type     :None
 MST BPDU Format     :Config=auto / Active=legacy
 Port Config-             
 Digest-Snooping     :disabled
 Num of Vlans Mapped :1 
 PortTimes           :Hello 2s MaxAge 20s FwDly 15s MsgAge 0s RemHop 20
 BPDU Sent           :0             
          TCN: 0, Config: 0, RST: 0, MST: 0
 BPDU Received       :0             
          TCN: 0, Config: 0, RST: 0, MST: 0

----[Port15(GigabitEthernet1/0/15)][DOWN]----
 Port Protocol       :enabled
 Port Role           :CIST Disabled Port
 Port Priority       :128
 Port Cost(Legacy)   :Config=auto / Active=200000
 Desg. Bridge/Port   :32768.20fd-f124-480d / 128.15
 Port Edged          :Config=enabled / Active=enabled
 Point-to-point      :Config=auto / Active=false
 Transmit Limit      :10 packets/hello-time
 Protection Type     :None
 MST BPDU Format     :Config=auto / Active=legacy
 Port Config-             
 Digest-Snooping     :disabled
 Num of Vlans Mapped :1 
 PortTimes           :Hello 2s MaxAge 20s FwDly 15s MsgAge 0s RemHop 20
 BPDU Sent           :0             
          TCN: 0, Config: 0, RST: 0, MST: 0
 BPDU Received       :0             
          TCN: 0, Config: 0, RST: 0, MST: 0

----[Port16(GigabitEthernet1/0/16)][DOWN]----
 Port Protocol       :enabled
 Port Role           :CIST Disabled Port
 Port Priority       :128
 Port Cost(Legacy)   :Config=auto / Active=200000
 Desg. Bridge/Port   :32768.20fd-f124-480d / 128.16
 Port Edged          :Config=enabled / Active=enabled
 Point-to-point      :Config=auto / Active=false
 Transmit Limit      :10 packets/hello-time
 Protection Type     :None
 MST BPDU Format     :Config=auto / Active=legacy
 Port Config-             
 Digest-Snooping     :disabled
 Num of Vlans Mapped :1 
 PortTimes           :Hello 2s MaxAge 20s FwDly 15s MsgAge 0s RemHop 20
 BPDU Sent           :0             
          TCN: 0, Config: 0, RST: 0, MST: 0
 BPDU Received       :0             
          TCN: 0, Config: 0, RST: 0, MST: 0

----[Port17(GigabitEthernet1/0/17)][DOWN]----
 Port Protocol       :enabled
 Port Role           :CIST Disabled Port
 Port Priority       :128
 Port Cost(Legacy)   :Config=auto / Active=200000
 Desg. Bridge/Port   :32768.20fd-f124-480d / 128.17
 Port Edged          :Config=enabled / Active=enabled
 Point-to-point      :Config=auto / Active=false
 Transmit Limit      :10 packets/hello-time
 Protection Type     :None
 MST BPDU Format     :Config=auto / Active=legacy
 Port Config-             
 Digest-Snooping     :disabled
 Rapid transition    :true
 Num of Vlans Mapped :1 
 PortTimes           :Hello 2s MaxAge 20s FwDly 15s MsgAge 0s RemHop 20
 BPDU Sent           :194             
          TCN: 0, Config: 0, RST: 194, MST: 0
 BPDU Received       :0             
          TCN: 0, Config: 0, RST: 0, MST: 0

----[Port18(GigabitEthernet1/0/18)][DOWN]----
 Port Protocol       :enabled
 Port Role           :CIST Disabled Port
 Port Priority       :128
 Port Cost(Legacy)   :Config=auto / Active=200000
 Desg. Bridge/Port   :32768.20fd-f124-480d / 128.18
 Port Edged          :Config=enabled / Active=enabled
 Point-to-point      :Config=auto / Active=false
 Transmit Limit      :10 packets/hello-time
 Protection Type     :None
 MST BPDU Format     :Config=auto / Active=legacy
 Port Config-             
 Digest-Snooping     :disabled
 Rapid transition    :true
 Num of Vlans Mapped :1 
 PortTimes           :Hello 2s MaxAge 20s FwDly 15s MsgAge 0s RemHop 20
 BPDU Sent           :193             
          TCN: 0, Config: 0, RST: 193, MST: 0
 BPDU Received       :0             
          TCN: 0, Config: 0, RST: 0, MST: 0

----[Port19(GigabitEthernet1/0/19)][DOWN]----
 Port Protocol       :enabled
 Port Role           :CIST Disabled Port
 Port Priority       :128
 Port Cost(Legacy)   :Config=auto / Active=200000
 Desg. Bridge/Port   :32768.20fd-f124-480d / 128.19
 Port Edged          :Config=enabled / Active=enabled
 Point-to-point      :Config=auto / Active=false
 Transmit Limit      :10 packets/hello-time
 Protection Type     :None
 MST BPDU Format     :Config=auto / Active=legacy
 Port Config-             
 Digest-Snooping     :disabled
 Rapid transition    :true
 Num of Vlans Mapped :1 
 PortTimes           :Hello 2s MaxAge 20s FwDly 15s MsgAge 0s RemHop 20
 BPDU Sent           :203             
          TCN: 0, Config: 0, RST: 203, MST: 0
 BPDU Received       :0             
          TCN: 0, Config: 0, RST: 0, MST: 0

----[Port20(GigabitEthernet1/0/20)][DOWN]----
 Port Protocol       :enabled
 Port Role           :CIST Disabled Port
 Port Priority       :128
 Port Cost(Legacy)   :Config=auto / Active=200000
 Desg. Bridge/Port   :32768.20fd-f124-480d / 128.20
 Port Edged          :Config=enabled / Active=enabled
 Point-to-point      :Config=auto / Active=false
 Transmit Limit      :10 packets/hello-time
 Protection Type     :None
 MST BPDU Format     :Config=auto / Active=legacy
 Port Config-             
 Digest-Snooping     :disabled
 Rapid transition    :true
 Num of Vlans Mapped :1 
 PortTimes           :Hello 2s MaxAge 20s FwDly 15s MsgAge 0s RemHop 20
 BPDU Sent           :203             
          TCN: 0, Config: 0, RST: 203, MST: 0
 BPDU Received       :0             
          TCN: 0, Config: 0, RST: 0, MST: 0

----[Port21(GigabitEthernet1/0/21)][DOWN]----
 Port Protocol       :enabled
 Port Role           :CIST Disabled Port
 Port Priority       :128
 Port Cost(Legacy)   :Config=auto / Active=200000
 Desg. Bridge/Port   :32768.20fd-f124-480d / 128.21
 Port Edged          :Config=enabled / Active=enabled
 Point-to-point      :Config=auto / Active=false
 Transmit Limit      :10 packets/hello-time
 Protection Type     :None
 MST BPDU Format     :Config=auto / Active=legacy
 Port Config-             
 Digest-Snooping     :disabled
 Rapid transition    :true
 Num of Vlans Mapped :1 
 PortTimes           :Hello 2s MaxAge 20s FwDly 15s MsgAge 0s RemHop 20
 BPDU Sent           :25             
          TCN: 0, Config: 0, RST: 25, MST: 0
 BPDU Received       :0             
          TCN: 0, Config: 0, RST: 0, MST: 0

----[Port22(GigabitEthernet1/0/22)][DOWN]----
 Port Protocol       :enabled
 Port Role           :CIST Disabled Port
 Port Priority       :128
 Port Cost(Legacy)   :Config=auto / Active=200000
 Desg. Bridge/Port   :32768.20fd-f124-480d / 128.22
 Port Edged          :Config=enabled / Active=enabled
 Point-to-point      :Config=auto / Active=false
 Transmit Limit      :10 packets/hello-time
 Protection Type     :None
 MST BPDU Format     :Config=auto / Active=legacy
 Port Config-             
 Digest-Snooping     :disabled
 Rapid transition    :true
 Num of Vlans Mapped :1 
 PortTimes           :Hello 2s MaxAge 20s FwDly 15s MsgAge 0s RemHop 20
 BPDU Sent           :71             
          TCN: 0, Config: 0, RST: 71, MST: 0
 BPDU Received       :0             
          TCN: 0, Config: 0, RST: 0, MST: 0

----[Port23(GigabitEthernet1/0/23)][DOWN]----
 Port Protocol       :enabled
 Port Role           :CIST Disabled Port
 Port Priority       :128
 Port Cost(Legacy)   :Config=auto / Active=200000
 Desg. Bridge/Port   :32768.20fd-f124-480d / 128.23
 Port Edged          :Config=enabled / Active=enabled
 Point-to-point      :Config=auto / Active=false
 Transmit Limit      :10 packets/hello-time
 Protection Type     :None
 MST BPDU Format     :Config=auto / Active=legacy
 Port Config-             
 Digest-Snooping     :disabled
 Rapid transition    :true
 Num of Vlans Mapped :1 
 PortTimes           :Hello 2s MaxAge 20s FwDly 15s MsgAge 0s RemHop 20
 BPDU Sent           :32             
          TCN: 0, Config: 0, RST: 32, MST: 0
 BPDU Received       :0             
          TCN: 0, Config: 0, RST: 0, MST: 0

----[Port24(GigabitEthernet1/0/24)][DOWN]----
 Port Protocol       :enabled
 Port Role           :CIST Disabled Port
 Port Priority       :128
 Port Cost(Legacy)   :Config=auto / Active=200000
 Desg. Bridge/Port   :32768.20fd-f124-480d / 128.24
 Port Edged          :Config=enabled / Active=enabled
 Point-to-point      :Config=auto / Active=false
 Transmit Limit      :10 packets/hello-time
 Protection Type     :None
 MST BPDU Format     :Config=auto / Active=legacy
 Port Config-             
 Digest-Snooping     :disabled
 Rapid transition    :true
 Num of Vlans Mapped :1 
 PortTimes           :Hello 2s MaxAge 20s FwDly 15s MsgAge 0s RemHop 20
 BPDU Sent           :71             
          TCN: 0, Config: 0, RST: 71, MST: 0
 BPDU Received       :0             
          TCN: 0, Config: 0, RST: 0, MST: 0

----[Port25(GigabitEthernet1/0/25)][DOWN]----
 Port Protocol       :enabled
 Port Role           :CIST Disabled Port
 Port Priority       :128
 Port Cost(Legacy)   :Config=auto / Active=200000
 Desg. Bridge/Port   :32768.20fd-f124-480d / 128.25
 Port Edged          :Config=enabled / Active=enabled
 Point-to-point      :Config=auto / Active=false
 Transmit Limit      :10 packets/hello-time
 Protection Type     :None
 MST BPDU Format     :Config=auto / Active=legacy
 Port Config-             
 Digest-Snooping     :disabled
 Num of Vlans Mapped :1 
 PortTimes           :Hello 2s MaxAge 20s FwDly 15s MsgAge 0s RemHop 20
 BPDU Sent           :0             
          TCN: 0, Config: 0, RST: 0, MST: 0
 BPDU Received       :0             
          TCN: 0, Config: 0, RST: 0, MST: 0

----[Port26(GigabitEthernet1/0/26)][DOWN]----
 Port Protocol       :enabled
 Port Role           :CIST Disabled Port
 Port Priority       :128
 Port Cost(Legacy)   :Config=auto / Active=200000
 Desg. Bridge/Port   :32768.20fd-f124-480d / 128.26
 Port Edged          :Config=enabled / Active=enabled
 Point-to-point      :Config=auto / Active=false
 Transmit Limit      :10 packets/hello-time
 Protection Type     :None
 MST BPDU Format     :Config=auto / Active=legacy
 Port Config-             
 Digest-Snooping     :disabled
 Num of Vlans Mapped :1 
 PortTimes           :Hello 2s MaxAge 20s FwDly 15s MsgAge 0s RemHop 20
 BPDU Sent           :0             
          TCN: 0, Config: 0, RST: 0, MST: 0
 BPDU Received       :0             
          TCN: 0, Config: 0, RST: 0, MST: 0

----[Port27(GigabitEthernet1/0/27)][DOWN]----
 Port Protocol       :enabled
 Port Role           :CIST Disabled Port
 Port Priority       :128
 Port Cost(Legacy)   :Config=auto / Active=200000
 Desg. Bridge/Port   :32768.20fd-f124-480d / 128.27
 Port Edged          :Config=enabled / Active=enabled
 Point-to-point      :Config=auto / Active=false
 Transmit Limit      :10 packets/hello-time
 Protection Type     :None
 MST BPDU Format     :Config=auto / Active=legacy
 Port Config-             
 Digest-Snooping     :disabled
 Num of Vlans Mapped :1 
 PortTimes           :Hello 2s MaxAge 20s FwDly 15s MsgAge 0s RemHop 20
 BPDU Sent           :0             
          TCN: 0, Config: 0, RST: 0, MST: 0
 BPDU Received       :0             
          TCN: 0, Config: 0, RST: 0, MST: 0

----[Port28(GigabitEthernet1/0/28)][DOWN]----
 Port Protocol       :enabled
 Port Role           :CIST Disabled Port
 Port Priority       :128
 Port Cost(Legacy)   :Config=auto / Active=200000
 Desg. Bridge/Port   :32768.20fd-f124-480d / 128.28
 Port Edged          :Config=enabled / Active=enabled
 Point-to-point      :Config=auto / Active=false
 Transmit Limit      :10 packets/hello-time
 Protection Type     :None
 MST BPDU Format     :Config=auto / Active=legacy
 Port Config-             
 Digest-Snooping     :disabled
 Num of Vlans Mapped :1 
 PortTimes           :Hello 2s MaxAge 20s FwDly 15s MsgAge 0s RemHop 20
 BPDU Sent           :0             
          TCN: 0, Config: 0, RST: 0, MST: 0
 BPDU Received       :0             
          TCN: 0, Config: 0, RST: 0, MST: 0

----[Port29(GigabitEthernet1/0/29)][DOWN]----
 Port Protocol       :enabled
 Port Role           :CIST Disabled Port
 Port Priority       :128
 Port Cost(Legacy)   :Config=auto / Active=200000
 Desg. Bridge/Port   :32768.20fd-f124-480d / 128.29
 Port Edged          :Config=enabled / Active=enabled
 Point-to-point      :Config=auto / Active=false
 Transmit Limit      :10 packets/hello-time
 Protection Type     :None
 MST BPDU Format     :Config=auto / Active=legacy
 Port Config-             
 Digest-Snooping     :disabled
 Num of Vlans Mapped :1 
 PortTimes           :Hello 2s MaxAge 20s FwDly 15s MsgAge 0s RemHop 20
 BPDU Sent           :0             
          TCN: 0, Config: 0, RST: 0, MST: 0
 BPDU Received       :0             
          TCN: 0, Config: 0, RST: 0, MST: 0

----[Port30(GigabitEthernet1/0/30)][DOWN]----
 Port Protocol       :enabled
 Port Role           :CIST Disabled Port
 Port Priority       :128
 Port Cost(Legacy)   :Config=auto / Active=200000
 Desg. Bridge/Port   :32768.20fd-f124-480d / 128.30
 Port Edged          :Config=enabled / Active=enabled
 Point-to-point      :Config=auto / Active=false
 Transmit Limit      :10 packets/hello-time
 Protection Type     :None
 MST BPDU Format     :Config=auto / Active=legacy
 Port Config-             
 Digest-Snooping     :disabled
 Num of Vlans Mapped :1 
 PortTimes           :Hello 2s MaxAge 20s FwDly 15s MsgAge 0s RemHop 20
 BPDU Sent           :0             
          TCN: 0, Config: 0, RST: 0, MST: 0
 BPDU Received       :0             
          TCN: 0, Config: 0, RST: 0, MST: 0

----[Port31(GigabitEthernet1/0/31)][DOWN]----
 Port Protocol       :enabled
 Port Role           :CIST Disabled Port
 Port Priority       :128
 Port Cost(Legacy)   :Config=auto / Active=200000
 Desg. Bridge/Port   :32768.20fd-f124-480d / 128.31
 Port Edged          :Config=enabled / Active=enabled
 Point-to-point      :Config=auto / Active=false
 Transmit Limit      :10 packets/hello-time
 Protection Type     :None
 MST BPDU Format     :Config=auto / Active=legacy
 Port Config-             
 Digest-Snooping     :disabled
 Num of Vlans Mapped :1 
 PortTimes           :Hello 2s MaxAge 20s FwDly 15s MsgAge 0s RemHop 20
 BPDU Sent           :0             
          TCN: 0, Config: 0, RST: 0, MST: 0
 BPDU Received       :0             
          TCN: 0, Config: 0, RST: 0, MST: 0

----[Port32(GigabitEthernet1/0/32)][DOWN]----
 Port Protocol       :enabled
 Port Role           :CIST Disabled Port
 Port Priority       :128
 Port Cost(Legacy)   :Config=auto / Active=200000
 Desg. Bridge/Port   :32768.20fd-f124-480d / 128.32
 Port Edged          :Config=enabled / Active=enabled
 Point-to-point      :Config=auto / Active=false
 Transmit Limit      :10 packets/hello-time
 Protection Type     :None
 MST BPDU Format     :Config=auto / Active=legacy
 Port Config-             
 Digest-Snooping     :disabled
 Num of Vlans Mapped :1 
 PortTimes           :Hello 2s MaxAge 20s FwDly 15s MsgAge 0s RemHop 20
 BPDU Sent           :0             
          TCN: 0, Config: 0, RST: 0, MST: 0
 BPDU Received       :0             
          TCN: 0, Config: 0, RST: 0, MST: 0

----[Port33(GigabitEthernet1/0/33)][DOWN]----
 Port Protocol       :enabled
 Port Role           :CIST Disabled Port
 Port Priority       :128
 Port Cost(Legacy)   :Config=auto / Active=200000
 Desg. Bridge/Port   :32768.20fd-f124-480d / 128.33
 Port Edged          :Config=enabled / Active=enabled
 Point-to-point      :Config=auto / Active=false
 Transmit Limit      :10 packets/hello-time
 Protection Type     :None
 MST BPDU Format     :Config=auto / Active=legacy
 Port Config-             
 Digest-Snooping     :disabled
 Num of Vlans Mapped :1 
 PortTimes           :Hello 2s MaxAge 20s FwDly 15s MsgAge 0s RemHop 20
 BPDU Sent           :0             
          TCN: 0, Config: 0, RST: 0, MST: 0
 BPDU Received       :0             
          TCN: 0, Config: 0, RST: 0, MST: 0

----[Port34(GigabitEthernet1/0/34)][DOWN]----
 Port Protocol       :enabled
 Port Role           :CIST Disabled Port
 Port Priority       :128
 Port Cost(Legacy)   :Config=auto / Active=200000
 Desg. Bridge/Port   :32768.20fd-f124-480d / 128.34
 Port Edged          :Config=enabled / Active=enabled
 Point-to-point      :Config=auto / Active=false
 Transmit Limit      :10 packets/hello-time
 Protection Type     :None
 MST BPDU Format     :Config=auto / Active=legacy
 Port Config-             
 Digest-Snooping     :disabled
 Num of Vlans Mapped :1 
 PortTimes           :Hello 2s MaxAge 20s FwDly 15s MsgAge 0s RemHop 20
 BPDU Sent           :0             
          TCN: 0, Config: 0, RST: 0, MST: 0
 BPDU Received       :0             
          TCN: 0, Config: 0, RST: 0, MST: 0

----[Port35(GigabitEthernet1/0/35)][DOWN]----
 Port Protocol       :enabled
 Port Role           :CIST Disabled Port
 Port Priority       :128
 Port Cost(Legacy)   :Config=auto / Active=200000
 Desg. Bridge/Port   :32768.20fd-f124-480d / 128.35
 Port Edged          :Config=enabled / Active=enabled
 Point-to-point      :Config=auto / Active=false
 Transmit Limit      :10 packets/hello-time
 Protection Type     :None
 MST BPDU Format     :Config=auto / Active=legacy
 Port Config-             
 Digest-Snooping     :disabled
 Num of Vlans Mapped :1 
 PortTimes           :Hello 2s MaxAge 20s FwDly 15s MsgAge 0s RemHop 20
 BPDU Sent           :0             
          TCN: 0, Config: 0, RST: 0, MST: 0
 BPDU Received       :0             
          TCN: 0, Config: 0, RST: 0, MST: 0

----[Port36(GigabitEthernet1/0/36)][DOWN]----
 Port Protocol       :enabled
 Port Role           :CIST Disabled Port
 Port Priority       :128
 Port Cost(Legacy)   :Config=auto / Active=200000
 Desg. Bridge/Port   :32768.20fd-f124-480d / 128.36
 Port Edged          :Config=enabled / Active=enabled
 Point-to-point      :Config=auto / Active=false
 Transmit Limit      :10 packets/hello-time
 Protection Type     :None
 MST BPDU Format     :Config=auto / Active=legacy
 Port Config-             
 Digest-Snooping     :disabled
 Num of Vlans Mapped :1 
 PortTimes           :Hello 2s MaxAge 20s FwDly 15s MsgAge 0s RemHop 20
 BPDU Sent           :0             
          TCN: 0, Config: 0, RST: 0, MST: 0
 BPDU Received       :0             
          TCN: 0, Config: 0, RST: 0, MST: 0

----[Port37(GigabitEthernet1/0/37)][DOWN]----
 Port Protocol       :enabled
 Port Role           :CIST Disabled Port
 Port Priority       :128
 Port Cost(Legacy)   :Config=auto / Active=200000
 Desg. Bridge/Port   :32768.20fd-f124-480d / 128.37
 Port Edged          :Config=enabled / Active=enabled
 Point-to-point      :Config=auto / Active=false
 Transmit Limit      :10 packets/hello-time
 Protection Type     :None
 MST BPDU Format     :Config=auto / Active=legacy
 Port Config-             
 Digest-Snooping     :disabled
 Num of Vlans Mapped :1 
 PortTimes           :Hello 2s MaxAge 20s FwDly 15s MsgAge 0s RemHop 20
 BPDU Sent           :0             
          TCN: 0, Config: 0, RST: 0, MST: 0
 BPDU Received       :0             
          TCN: 0, Config: 0, RST: 0, MST: 0

----[Port38(GigabitEthernet1/0/38)][DOWN]----
 Port Protocol       :enabled
 Port Role           :CIST Disabled Port
 Port Priority       :128
 Port Cost(Legacy)   :Config=auto / Active=200000
 Desg. Bridge/Port   :32768.20fd-f124-480d / 128.38
 Port Edged          :Config=enabled / Active=enabled
 Point-to-point      :Config=auto / Active=false
 Transmit Limit      :10 packets/hello-time
 Protection Type     :None
 MST BPDU Format     :Config=auto / Active=legacy
 Port Config-             
 Digest-Snooping     :disabled
 Num of Vlans Mapped :1 
 PortTimes           :Hello 2s MaxAge 20s FwDly 15s MsgAge 0s RemHop 20
 BPDU Sent           :0             
          TCN: 0, Config: 0, RST: 0, MST: 0
 BPDU Received       :0             
          TCN: 0, Config: 0, RST: 0, MST: 0

----[Port39(GigabitEthernet1/0/39)][DOWN]----
 Port Protocol       :enabled
 Port Role           :CIST Disabled Port
 Port Priority       :128
 Port Cost(Legacy)   :Config=auto / Active=200000
 Desg. Bridge/Port   :32768.20fd-f124-480d / 128.39
 Port Edged          :Config=enabled / Active=enabled
 Point-to-point      :Config=auto / Active=false
 Transmit Limit      :10 packets/hello-time
 Protection Type     :None
 MST BPDU Format     :Config=auto / Active=legacy
 Port Config-             
 Digest-Snooping     :disabled
 Num of Vlans Mapped :1 
 PortTimes           :Hello 2s MaxAge 20s FwDly 15s MsgAge 0s RemHop 20
 BPDU Sent           :0             
          TCN: 0, Config: 0, RST: 0, MST: 0
 BPDU Received       :0             
          TCN: 0, Config: 0, RST: 0, MST: 0

----[Port40(GigabitEthernet1/0/40)][DOWN]----
 Port Protocol       :enabled
 Port Role           :CIST Disabled Port
 Port Priority       :128
 Port Cost(Legacy)   :Config=auto / Active=200000
 Desg. Bridge/Port   :32768.20fd-f124-480d / 128.40
 Port Edged          :Config=enabled / Active=enabled
 Point-to-point      :Config=auto / Active=false
 Transmit Limit      :10 packets/hello-time
 Protection Type     :None
 MST BPDU Format     :Config=auto / Active=legacy
 Port Config-             
 Digest-Snooping     :disabled
 Num of Vlans Mapped :1 
 PortTimes           :Hello 2s MaxAge 20s FwDly 15s MsgAge 0s RemHop 20
 BPDU Sent           :0             
          TCN: 0, Config: 0, RST: 0, MST: 0
 BPDU Received       :0             
          TCN: 0, Config: 0, RST: 0, MST: 0

----[Port41(GigabitEthernet1/0/41)][DOWN]----
 Port Protocol       :enabled
 Port Role           :CIST Disabled Port
 Port Priority       :128
 Port Cost(Legacy)   :Config=auto / Active=200000
 Desg. Bridge/Port   :32768.20fd-f124-480d / 128.41
 Port Edged          :Config=enabled / Active=enabled
 Point-to-point      :Config=auto / Active=false
 Transmit Limit      :10 packets/hello-time
 Protection Type     :None
 MST BPDU Format     :Config=auto / Active=legacy
 Port Config-             
 Digest-Snooping     :disabled
 Num of Vlans Mapped :1 
 PortTimes           :Hello 2s MaxAge 20s FwDly 15s MsgAge 0s RemHop 20
 BPDU Sent           :0             
          TCN: 0, Config: 0, RST: 0, MST: 0
 BPDU Received       :0             
          TCN: 0, Config: 0, RST: 0, MST: 0

----[Port42(GigabitEthernet1/0/42)][DOWN]----
 Port Protocol       :enabled
 Port Role           :CIST Disabled Port
 Port Priority       :128
 Port Cost(Legacy)   :Config=auto / Active=200000
 Desg. Bridge/Port   :32768.20fd-f124-480d / 128.42
 Port Edged          :Config=enabled / Active=enabled
 Point-to-point      :Config=auto / Active=false
 Transmit Limit      :10 packets/hello-time
 Protection Type     :None
 MST BPDU Format     :Config=auto / Active=legacy
 Port Config-             
 Digest-Snooping     :disabled
 Num of Vlans Mapped :1 
 PortTimes           :Hello 2s MaxAge 20s FwDly 15s MsgAge 0s RemHop 20
 BPDU Sent           :0             
          TCN: 0, Config: 0, RST: 0, MST: 0
 BPDU Received       :0             
          TCN: 0, Config: 0, RST: 0, MST: 0

----[Port43(GigabitEthernet1/0/43)][DOWN]----
 Port Protocol       :enabled
 Port Role           :CIST Disabled Port
 Port Priority       :128
 Port Cost(Legacy)   :Config=auto / Active=200000
 Desg. Bridge/Port   :32768.20fd-f124-480d / 128.43
 Port Edged          :Config=enabled / Active=enabled
 Point-to-point      :Config=auto / Active=false
 Transmit Limit      :10 packets/hello-time
 Protection Type     :None
 MST BPDU Format     :Config=auto / Active=legacy
 Port Config-             
 Digest-Snooping     :disabled
 Num of Vlans Mapped :1 
 PortTimes           :Hello 2s MaxAge 20s FwDly 15s MsgAge 0s RemHop 20
 BPDU Sent           :0             
          TCN: 0, Config: 0, RST: 0, MST: 0
 BPDU Received       :0             
          TCN: 0, Config: 0, RST: 0, MST: 0

----[Port44(GigabitEthernet1/0/44)][DOWN]----
 Port Protocol       :enabled
 Port Role           :CIST Disabled Port
 Port Priority       :128
 Port Cost(Legacy)   :Config=auto / Active=200000
 Desg. Bridge/Port   :32768.20fd-f124-480d / 128.44
 Port Edged          :Config=enabled / Active=enabled
 Point-to-point      :Config=auto / Active=false
 Transmit Limit      :10 packets/hello-time
 Protection Type     :None
 MST BPDU Format     :Config=auto / Active=legacy
 Port Config-             
 Digest-Snooping     :disabled
 Num of Vlans Mapped :1 
 PortTimes           :Hello 2s MaxAge 20s FwDly 15s MsgAge 0s RemHop 20
 BPDU Sent           :0             
          TCN: 0, Config: 0, RST: 0, MST: 0
 BPDU Received       :0             
          TCN: 0, Config: 0, RST: 0, MST: 0

----[Port45(GigabitEthernet1/0/45)][DOWN]----
 Port Protocol       :enabled
 Port Role           :CIST Disabled Port
 Port Priority       :128
 Port Cost(Legacy)   :Config=auto / Active=200000
 Desg. Bridge/Port   :32768.20fd-f124-480d / 128.45
 Port Edged          :Config=enabled / Active=enabled
 Point-to-point      :Config=auto / Active=false
 Transmit Limit      :10 packets/hello-time
 Protection Type     :None
 MST BPDU Format     :Config=auto / Active=legacy
 Port Config-             
 Digest-Snooping     :disabled
 Num of Vlans Mapped :1 
 PortTimes           :Hello 2s MaxAge 20s FwDly 15s MsgAge 0s RemHop 20
 BPDU Sent           :0             
          TCN: 0, Config: 0, RST: 0, MST: 0
 BPDU Received       :0             
          TCN: 0, Config: 0, RST: 0, MST: 0

----[Port46(GigabitEthernet1/0/46)][DOWN]----
 Port Protocol       :enabled
 Port Role           :CIST Disabled Port
 Port Priority       :128
 Port Cost(Legacy)   :Config=auto / Active=200000
 Desg. Bridge/Port   :32768.20fd-f124-480d / 128.46
 Port Edged          :Config=enabled / Active=enabled
 Point-to-point      :Config=auto / Active=false
 Transmit Limit      :10 packets/hello-time
 Protection Type     :None
 MST BPDU Format     :Config=auto / Active=legacy
 Port Config-             
 Digest-Snooping     :disabled
 Num of Vlans Mapped :1 
 PortTimes           :Hello 2s MaxAge 20s FwDly 15s MsgAge 0s RemHop 20
 BPDU Sent           :0             
          TCN: 0, Config: 0, RST: 0, MST: 0
 BPDU Received       :0             
          TCN: 0, Config: 0, RST: 0, MST: 0

----[Port47(GigabitEthernet1/0/47)][DOWN]----
 Port Protocol       :enabled
 Port Role           :CIST Disabled Port
 Port Priority       :128
 Port Cost(Legacy)   :Config=auto / Active=200000
 Desg. Bridge/Port   :32768.20fd-f124-480d / 128.47
 Port Edged          :Config=enabled / Active=enabled
 Point-to-point      :Config=auto / Active=false
 Transmit Limit      :10 packets/hello-time
 Protection Type     :None
 MST BPDU Format     :Config=auto / Active=legacy
 Port Config-             
 Digest-Snooping     :disabled
 Rapid transition    :true
 Num of Vlans Mapped :1 
 PortTimes           :Hello 2s MaxAge 20s FwDly 15s MsgAge 0s RemHop 20
 BPDU Sent           :308             
          TCN: 0, Config: 0, RST: 308, MST: 0
 BPDU Received       :0             
          TCN: 0, Config: 0, RST: 0, MST: 0

----[Port48(GigabitEthernet1/0/48)][DOWN]----
 Port Protocol       :enabled
 Port Role           :CIST Disabled Port
 Port Priority       :128
 Port Cost(Legacy)   :Config=auto / Active=200000
 Desg. Bridge/Port   :32768.20fd-f124-480d / 128.48
 Port Edged          :Config=enabled / Active=enabled
 Point-to-point      :Config=auto / Active=false
 Transmit Limit      :10 packets/hello-time
 Protection Type     :None
 MST BPDU Format     :Config=auto / Active=legacy
 Port Config-             
 Digest-Snooping     :disabled
 Num of Vlans Mapped :1 
 PortTimes           :Hello 2s MaxAge 20s FwDly 15s MsgAge 0s RemHop 20
 BPDU Sent           :0             
          TCN: 0, Config: 0, RST: 0, MST: 0
 BPDU Received       :0             
          TCN: 0, Config: 0, RST: 0, MST: 0

----[Port49(GigabitEthernet1/0/49)][DOWN]----
 Port Protocol       :enabled
 Port Role           :CIST Disabled Port
 Port Priority       :128
 Port Cost(Legacy)   :Config=auto / Active=200000
 Desg. Bridge/Port   :32768.20fd-f124-480d / 128.49
 Port Edged          :Config=enabled / Active=enabled
 Point-to-point      :Config=auto / Active=false
 Transmit Limit      :10 packets/hello-time
 Protection Type     :None
 MST BPDU Format     :Config=auto / Active=legacy
 Port Config-             
 Digest-Snooping     :disabled
 Num of Vlans Mapped :1 
 PortTimes           :Hello 2s MaxAge 20s FwDly 15s MsgAge 0s RemHop 20
 BPDU Sent           :0             
          TCN: 0, Config: 0, RST: 0, MST: 0
 BPDU Received       :0             
          TCN: 0, Config: 0, RST: 0, MST: 0

----[Port50(GigabitEthernet1/0/50)][DOWN]----
 Port Protocol       :enabled
 Port Role           :CIST Disabled Port
 Port Priority       :128
 Port Cost(Legacy)   :Config=auto / Active=200000
 Desg. Bridge/Port   :32768.20fd-f124-480d / 128.50
 Port Edged          :Config=enabled / Active=enabled
 Point-to-point      :Config=auto / Active=false
 Transmit Limit      :10 packets/hello-time
 Protection Type     :None
 MST BPDU Format     :Config=auto / Active=legacy
 Port Config-             
 Digest-Snooping     :disabled
 Num of Vlans Mapped :1 
 PortTimes           :Hello 2s MaxAge 20s FwDly 15s MsgAge 0s RemHop 20
 BPDU Sent           :0             
          TCN: 0, Config: 0, RST: 0, MST: 0
 BPDU Received       :0             
          TCN: 0, Config: 0, RST: 0, MST: 0

----[Port51(GigabitEthernet1/0/51)][DOWN]----
 Port Protocol       :enabled
 Port Role           :CIST Disabled Port
 Port Priority       :128
 Port Cost(Legacy)   :Config=auto / Active=200000
 Desg. Bridge/Port   :32768.20fd-f124-480d / 128.51
 Port Edged          :Config=enabled / Active=enabled
 Point-to-point      :Config=auto / Active=false
 Transmit Limit      :10 packets/hello-time
 Protection Type     :None
 MST BPDU Format     :Config=auto / Active=legacy
 Port Config-             
 Digest-Snooping     :disabled
 Num of Vlans Mapped :1 
 PortTimes           :Hello 2s MaxAge 20s FwDly 15s MsgAge 0s RemHop 20
 BPDU Sent           :0             
          TCN: 0, Config: 0, RST: 0, MST: 0
 BPDU Received       :0             
          TCN: 0, Config: 0, RST: 0, MST: 0

----[Port52(GigabitEthernet1/0/52)][DOWN]----
 Port Protocol       :enabled
 Port Role           :CIST Disabled Port
 Port Priority       :128
 Port Cost(Legacy)   :Config=auto / Active=200000
 Desg. Bridge/Port   :32768.20fd-f124-480d / 128.52
 Port Edged          :Config=enabled / Active=enabled
 Point-to-point      :Config=auto / Active=false
 Transmit Limit      :10 packets/hello-time
 Protection Type     :None
 MST BPDU Format     :Config=auto / Active=legacy
 Port Config-             
 Digest-Snooping     :disabled
 Num of Vlans Mapped :1 
 PortTimes           :Hello 2s MaxAge 20s FwDly 15s MsgAge 0s RemHop 20
 BPDU Sent           :0             
          TCN: 0, Config: 0, RST: 0, MST: 0
 BPDU Received       :0             
          TCN: 0, Config: 0, RST: 0, MST: 0
==========================================================
  ===============_display drv templimit===============
==========================================================
current parameter : LowerTMP=76,  UpperTMP=86
==========================================================
  ===============_display drv voicevlan===============
==========================================================
--g_ulOuiMacRangeCnt = 7
--g_ulOuiMacRangeCurrent = 0
--g_ulOuiMacCnt = 0
-------port status------------
--no ports voice vlan enabled 
------------------------------
--[0] 0001-e300-0000 mask ffff-ff00-0000
--[1] 0003-6b00-0000 mask ffff-ff00-0000
--[2] 0004-0d00-0000 mask ffff-ff00-0000
--[3] 0060-b900-0000 mask ffff-ff00-0000
--[4] 00d0-1e00-0000 mask ffff-ff00-0000
--[5] 00e0-7500-0000 mask ffff-ff00-0000
--[6] 00e0-bb00-0000 mask ffff-ff00-0000
============================================================
  ===============_display drv walkthrough===============
============================================================
 Counter                            Offset      Chip0      Chip1
 ============================== ========== ========== ==========
 Global security Breach filter     2040104          0          0
 Port/VLAN Security Breach Drop    2040108          0          0
 Bridge Filter Counter             2040150       9475          0
 ------------------------------ ---------- ---------- ----------
 Set<n> VLAN Ingress Filter    
  Set0                             20400e4          0          0
  Set1                             20400f8          0          0
 ------------------------------ ---------- ---------- ----------
 ------------------------------ ---------- ---------- ----------
 Set<n> Security Filter        
  Set0                             20400e8          0          0
  Set1                             20400fc          0          0
 ------------------------------ ---------- ---------- ----------
 ------------------------------ ---------- ---------- ----------
 Set<n> Bridge Filter          
  Set0                             20400ec         93          0
  Set1                             2040100         93          0
 ------------------------------ ---------- ---------- ----------
 ------------------------------ ---------- ---------- ----------
 Set<n> Incoming Packet        
  Set0                             20400e0   10360864          0
  Set1                             20400f4   10360864          0
 ------------------------------ ---------- ---------- ----------
 Ingress Drop                      b000040      14448          0
 ------------------------------ ---------- ---------- ----------
 Receive SDMA<n> Packet        
  Set0                                2820          0          0
  Set1                                2824          0          0
  Set2                                2828          0          0
  Set3                                282c          0          0
  Set4                                2830          0          0
  Set5                                2834          0          0
  Set6                                2838          0          0
  Set7                                283c          0          0
 ------------------------------ ---------- ---------- ----------
 ------------------------------ ---------- ---------- ----------
 Receive SDMA<n> Byte          
  Set0                                2840          0          0
  Set1                                2844          0          0
  Set2                                2848          0          0
  Set3                                284c          0          0
  Set4                                2850          0          0
  Set5                                2854          0          0
  Set6                                2858          0          0
  Set7                                285c          0          0
 ------------------------------ ---------- ---------- ----------
 ------------------------------ ---------- ---------- ----------
 Receive SDMA Resource Error   
  Set0                                2860          0          0
  Set1                                2864          0          0
 ------------------------------ ---------- ---------- ----------
 ------------------------------ ---------- ---------- ----------
 Set<n> Outgoing Unicast       
  Set0                             1b40144   10358046          0
  Set1                             1b40164   10358046          0
 ------------------------------ ---------- ---------- ----------
 ------------------------------ ---------- ---------- ----------
 Set<n> Outgoing Multicast     
  Set0                             1b40148       3474          0
  Set1                             1b40168       3474          0
 ------------------------------ ---------- ---------- ----------
 ------------------------------ ---------- ---------- ----------
 Set<n> Outgoing Broadcast     
  Set0                             1b4014c       1270          0
  Set1                             1b4016c       1270          0
 ------------------------------ ---------- ---------- ----------
 ------------------------------ ---------- ---------- ----------
 Set<n> Bridge Egress Filter   
  Set0                             1b40150          0          0
  Set1                             1b40170          0          0
 ------------------------------ ---------- ---------- ----------
 ------------------------------ ---------- ---------- ----------
 Set<n> Tail Dropped           
  Set0                             1b40154         74          0
  Set1                             1b40174         74          0
 ------------------------------ ---------- ---------- ----------
 ------------------------------ ---------- ---------- ----------
 Set<n> Control Packet         
  Set0                             1b40158       5343          0
  Set1                             1b40178       5343          0
 ------------------------------ ---------- ---------- ----------
 ------------------------------ ---------- ---------- ----------
 Set<n> Egress Forward Restrict
  Set0                             1b4015c          0          0
  Set1                             1b4017c          0          0
 ------------------------------ ---------- ---------- ----------
 ------------------------------ ---------- ---------- ----------
 Set<n> Multicast FIFO Dropped 
  Set0                             1b40180          0       2399
  Set1                             1b40184          0       2399
 ------------------------------ ---------- ---------- ----------
================================================
  ===============display cpu ===============
================================================
Unit CPU usage: 
      47% in last 5 seconds
       1% in last 1 minute
       1% in last 5 minutes

====================================================
  ===============display cpu task===============
====================================================
===== Current CPU usage info =====
CPU Usage Stat. Cycle: 8 (Second)
CPU Usage            : 72%
CPU Usage Stat. Time : 2000-04-27  14:36:54
CPU Usage Stat. Tick : 0x1175(CPU Tick High) 0xcf12e56f(CPU Tick Low)
Actual Stat. Cycle   : 0x0(CPU Tick High) 0x61377993(CPU Tick Low)

TaskName        CPU        Runtime(CPU Tick High/CPU Tick Low)
VIDL            28%               0/1bedbf56
TICK             0%               0/  e262ba
STMR             0%               0/   57b2e
SYSM             0%               0/   2ebef
 LED             0%               0/  322ffb
LED3             0%               0/   c05f1
RxMi             0%               0/   b1237
LPDT             0%               0/    705a
AtkT             0%               0/    48f9
IPCM             0%               0/   281d1
 DEV             0%               0/   9222e
STND             0%               0/   9948a
SOCK             0%               0/   53bd5
ADJ4             0%               0/   2d0e4
 ACL             0%               0/   11060
LAGG             0%               0/   7ed82
MSTP             0%               0/  110d11
CLST             0%               0/   60e96
 NDP             0%               0/   321a7
NTDP             0%               0/   2c27d
HABP             0%               0/   252ba
LLDP             0%               0/   270db
 ARP             0%               0/   956ea
  IP             0%               0/  206fd3
FSLH             0%               0/   259f5
FSLR             0%               0/  15c940
HTTP             0%               0/   15e06
NTPT             0%               0/   29caf
VTYD             0%               0/  1c254c
DT1X             0%               0/   2c51b
 ACM             0%               0/   efa03
  LS             0%               0/  146396
RDSO             0%               0/   65e1f
 RDS             0%               0/    cd2c
  SC             0%               0/   72a65
IPGD             0%               0/  106bcf
PSEC             0%               0/   27c26
ROUT             0%               0/  f8b037
IFNT             0%               0/   30715
WEBS             0%               0/   29f36
HDQ0            67%               0/41d6a527
PrdT             0%               0/  3b5d4c
DrvT             0%               0/  13252b

=======================================================
  ===============display cpu history===============
=======================================================
100%|                                                            
 95%|                                                            
 90%|                                                            
 85%|                                                            
 80%|                                                            
 75%|                                                            
 70%|                                                            
 65%|                                                            
 60%|                                                            
 55%|                                                            
 50%|                                                            
 45%|                                                            
 40%|                                                            
 35%|                                                            
 30%|                                                            
 25%|                                                            
 20%|                                                            
 15%|                                                            
 10%|          #                                                 
  5%|         ##  ##            ###                             #
     ------------------------------------------------------------
              10        20        30        40        50        60  (minutes)
                      cpu-usage last 60 minutes(SYSTEM)
==========================================================
  ===============_display memory core 0===============
==========================================================
Slice Memory Usage:

Block Size    32	Free     865	Used   21279	Total   22144
Block Size    64	Free     259	Used    2622	Total    2881
Block Size   128	Free     186	Used    2830	Total    3016
Block Size   256	Free      19	Used    2156	Total    2175
Block Size   512	Free      16	Used    1184	Total    1200
Block Size  1024	Free      48	Used     393	Total     441
Block Size  2048	Free      49	Used     455	Total     504
Block Size  4096	Free      10	Used     730	Total     740
-----------------------------Summary--------------------------------
Used(Byte) 6693472 	Free    1452	Used   31649	Total   33101
Total Slice Allocated Size: 8297680 bytes 	Used Ratio: 80

Total Slice Memory(Include Control Data and Free Slice): 8297680 bytes
Raw Slice Memory Usage:
  Total Used Size: 26370861 bytes  Num: 428 
  Total Raw Slice Size (Include Control Data and Free Slice): 28627548 bytes  Used Ratio: 92


Partition 0 Total Memory(bytes): 82243280 

===================================================================
  ===============_display memory 32 group core 0===============
===================================================================
(0106,      136) (010d,       27) (cc74,      815) (1234,     4072)
(0214,     1682) (cc15,        6) (cc1a,        3) (cc31,        1)
(cc51,     8359) (021a,       60) (0341,      603) (0213,      773)
(0216,     2449) (cc42,       10) (0805,        5) (0831,      161)
(0830,      140) (0828,       26) (0833,        5) (0826,        7)
(0240,       72) (0230,      100) (0524,        3) (0900,      404)
(0215,      100) (0340,        5) (cc02,        2) (0360,        1)
(0311,        8) (041e,      122) (0518,        2) (0920,       79)
(0846,       55) (0910,       59) (0538,        2) (0217,        4)
(0241,        2) (0277,        4) (0263,        3) (0260,        1)
(0446,       58) (0467,        1) (040c,       59) (0528,        7)
(0342,        8) (04e3,        7) (04e4,       56) (02b5,        3)
(0501,       20) (0320,      474) (04e5,        2) (0349,        2)
(0321,        6) (0420,        1) (0504,        1) (0483,        1)
(0502,        1) (043a,        7) (0904,        2) (0801,        2)
(034c,       54) (0508,        5) (051a,        2) (051b,        3)
(04a0,        7) (051c,       21) (0516,        4) (cc33,        1)
(0930,       11) (0514,        8) (0911,       63) (0600,        1)
(0537,        2) (0809,        4) (0813,        3) (0844,        6)
===================================================================
  ===============_display memory 64 group core 0===============
===================================================================
(cc74,      333) (cc31,        9) (cc51,       61) (cc34,        1)
(0214,      887) (cc38,        1) (cc32,        1) (cc3a,        1)
(cc37,        1) (034c,        1) (0260,        3) (0805,        4)
(0920,      357) (0830,        1) (0216,      315) (0240,      290)
(0846,        1) (0518,        1) (0900,        8) (0340,       61)
(011e,       26) (04e3,        3) (0213,       25) (043a,        4)
(0525,        1) (0483,        1) (0813,        1) (0532,        1)
(041e,       14) (0610,        1) (03a3,       48) (021a,       10)
(0218,        2) (0341,        1) (0514,        1) (051d,        1)
(04a0,      137) (0910,        1) (0930,        7) (0000,        0)
====================================================================
  ===============_display memory 128 group core 0===============
====================================================================
(cc74,       81) (cc31,        6) (cc33,        3) (cc01,        1)
(cc51,      513) (cc41,        1) (cc32,        1) (cc15,        6)
(cc14,        1) (cc19,        1) (0830,        2) (0290,        1)
(0214,      379) (0216,      666) (0240,      153) (0218,        3)
(0833,        1) (0846,        1) (0213,      112) (0342,      167)
(04e3,        1) (0501,        3) (0515,        1) (0446,       58)
(0230,       55) (04a0,      146) (0801,       52) (0340,        1)
(0920,      398) (0525,        1) (0900,        4) (0341,        8)
(051c,        1) (051d,        1) (041e,        1) (0000,        0)
====================================================================
  ===============_display memory 256 group core 0===============
====================================================================
(cc74,       35) (cc31,        8) (cc33,        2) (cc32,        2)
(cc51,        4) (cc41,        1) (cc38,        1) (cc3b,        1)
(02f0,        1) (0830,        1) (0213,      193) (0283,        1)
(0214,      991) (0216,       81) (040c,        2) (0341,      502)
(0102,        2) (011c,        5) (0342,       57) (043a,        1)
(0320,       64) (0502,        1) (0420,        1) (0504,        1)
(0240,      178) (0101,        3) (0600,        1) (cc42,        9)
(010c,        1) (cc15,        1) (cc72,        1) (0911,        2)
(0519,        2) (0000,        0) (0000,        0) (0000,        0)
====================================================================
  ===============_display memory 512 group core 0===============
====================================================================
(0117,        1) (010d,        1) (cc74,       12) (cc41,        2)
(cc31,      485) (cc3c,        1) (cc33,        1) (cc21,        1)
(cc51,        1) (cc13,        1) (0341,        1) (cc34,        1)
(0216,       14) (0342,        7) (0360,        1) (041e,        1)
(0532,        1) (0260,        1) (040c,        5) (0230,        3)
(04e3,        1) (011e,        2) (0215,        1) (04e4,        1)
(0213,        1) (04e5,        1) (0240,        6) (0102,        1)
(0501,        3) (04a0,      284) (051d,        1) (0801,       52)
(0920,      114) (0508,        1) (0214,      170) (051c,        2)
(0516,        1) (0910,        1) (0000,        0) (0000,        0)
=====================================================================
  ===============_display memory 1024 group core 0===============
=====================================================================
(010d,       24) (cc74,       17) (1234,        4) (cc31,        7)
(cc33,        7) (cc32,        1) (cc51,        3) (cc41,        5)
(cc14,        1) (0160,        2) (0290,        1) (0216,      112)
(0240,        1) (04a0,        2) (0900,        1) (041e,        3)
(051c,       11) (0910,        2) (0214,        3) (0260,        1)
(021c,        3) (0805,        1) (0102,        2) (040c,        2)
(0101,        3) (0602,        7) (0844,        1) (0000,        1)
(0320,       52) (0518,       10) (0215,      105) (0000,        0)
=====================================================================
  ===============_display memory 2048 group core 0===============
=====================================================================
(0101,        1) (010d,       21) (0102,       31) (cc74,       13)
(1234,        5) (cc31,        3) (cc3c,        1) (cc21,        3)
(cc51,      107) (cc03,        2) (cc42,        1) (0821,        2)
(0283,       11) (0260,        1) (0218,       19) (0910,        1)
(0216,       10) (040c,        2) (cc35,        1) (0342,        1)
(0420,        1) (0502,        1) (0504,        1) (0516,        1)
(043a,        1) (0602,        9) (0600,        1) (0349,       52)
(010f,        2) (0525,        1) (04a0,        5) (0805,        1)
(cc72,      137) (0820,        4) (cc41,        1) (0519,        1)
=====================================================================
  ===============_display memory 4096 group core 0===============
=====================================================================
(0160,        1) (010d,        2) (cc74,        9) (cc33,        1)
(cc51,        6) (cc35,        1) (010f,        1) (0804,        1)
(0822,        3) (0813,        3) (0290,        1) (01ff,      670)
(0102,        3) (0911,        1) (0230,        1) (0342,        1)
(0321,        2) (0216,        2) (0501,        1) (0805,        4)
(0602,        5) (0240,        2) (04a0,        7) (011e,        1)
(021b,        1) (0000,        0) (0000,        0) (0000,        0)
===================================================================
  ===============_display memory raw all core 0 ===============
===================================================================
[userMid, totalNum, totalLen](Hex)
[0102,  61,  427840]   [0218,   1,    1ca8]   [0910,   1,    2000]   
[0216,   6,   5c000]   [04a0,   1,    120c]   [0101,  1d,   75118]   
[011c,   5,  1b4800]   [0602,   5,    eb40]   [010b,   1,    2000]   
[043a,   2,    2008]   [0240,   1,    3ff8]   [0900,   1,    4614]   
[0514,   2,    40c0]   [cc72,   2,   28074]   [0920,   1,   1f800]   
[0660,   1,    5000]   [0661,   2,    fff0]   [0000,   1,    3024]   
[0805,   1,    55f8]   [011e,   2,    6840]   [0904,   5,   37ce8]   
[0501,   1,    4000]   [0516,   1,    2000]   [0321,   3,    c024]   
[0342,   3,    3784]   [cc35,   1,    2b78]   [034c,   2,    4000]   
[040c,   5,   19000]   [0230,   3,   7bf84]   [0467,   3,    c000]   
[0214,   1,   32008]   [0804,   1,    2800]   [04cb,   1,   13fec]   
[041e,   2,    c000]   [0311,   1,    5dc0]   [0498,   1,    3ffc]   
[0341,   1,    2004]   [0518,   1,    201c]   [0213,   1,  100000]   
[0821,   1,   6e880]   [0813,   9,   9fffc]   [0822,   1,    1064]   
[0820,   3,    72a0]   [010f,   1,    13b0]   [cc15,   1,    3ffc]   
[cc32,   1,    4100]   [cc41,   1,    2ee0]   [cc51,  71,  282354]   
[cc21,   2,    dff8]   [cc33,   3,    93a8]   [cc3c,   1,    1380]   
[cc31,   1,    3260]   [cc74,  57,  bc7334]   [010d,   3,    7000]   
[0117,   1,    3600]   
Total 0x1926350 bytes  428  blocks. 

Raw memory free info:
[userInfo,     len](Hex)
[010b1000,  111c64] [02160240,     130] [cc740000,     39c] 
[cc720000,     4bc] [010d02d6,     560] [06020000,     818] 
[cc740000,     9d0] [cd0b0001,     dd8] [02400000,     f9c] 
[cc720000,    2a60] [01020105,    6af0] [02160240,    8000] 
[043a0201,   11ff4] [03600000,   12528] [09110000,   d74c0] 
Total 0x222c2c bytes 15 blocks.
======================================================================
  ===============_display memory-allocation-failure===============
======================================================================
No memory allocation failure information stored.
========================================================
  ===============_display om cpu-high===============
========================================================
CPU usage high module is disabled.
Current monitor threshold is 80%.
No CPU usage high information stored.
============================================================
  ===============_display om error-packet===============
============================================================
Error packet information record module is disabled.
No error packet information stored.
====================================================
  ===============_display om task===============
====================================================
No task information stored.
===============================================================
  ===============display deadloop 10 verbose===============
===============================================================
===========================================================================
  ===============display deadloop 10 verbose from-device===============
===========================================================================
================================================================
  ===============display exception 10 verbose===============
================================================================
============================================================================
  ===============display exception 10 verbose from-device===============
============================================================================
======================================================================
  ===============display reboot-information verbose===============
======================================================================
====================================================================================
  ===============display reboot-information verbose from-device 5===============
====================================================================================
=======================================================
  ===============display boot-loader===============
=======================================================
 Current boot app is: flash:/S2900-CMW520-R1101P10.bin
 Next main boot app is: flash:/S2900-CMW520-R1101P10.bin
 Next backup boot app is: 
===========================================================
  ===============display device manuinfo===============
===========================================================
DEVICE_NAME          : 3CRBSG5293
DEVICE_SERIAL_NUMBER : 927FDCS24480D
MAC_ADDRESS          : 20FD-F124-480D
MANUFACTURING_DATE   : 2010-11-15
VENDOR_NAME          : 3COM
=======================================================
  ===============_disp reserved-area===============
=======================================================
=======Begin===============Reaserved area information====================
    The Type of area is   :  High memory
    The version of area is:  1.0
    The size of area is   :  3895920(Byte)
    The number of mod is  :  6
    The unused offset is  :  353228
    Reaserved area status :  Valid
=======End===============Reaserved area information====================

  =======Begin========Module 1 information============================
      Module ID     :  0xcd050001
      Module name   :  lastver
      Module version:  1.0
      Module size   :  2088(Byte)
      Module status :  Valid
  =======End==========Module 1 information============================

  =======Begin========Module 2 information============================
      Module ID     :  0xcd040001
      Module name   :  historycmd
      Module version:  1.0
      Module size   :  38456(Byte)
      Module status :  Valid
  =======End==========Module 2 information============================

  =======Begin========Module 3 information============================
      Module ID     :  0xcd060001
      Module name   :  memfail
      Module version:  1.0
      Module size   :  18368(Byte)
      Module status :  Valid
  =======End==========Module 3 information============================

  =======Begin========Module 4 information============================
      Module ID     :  0xcd090001
      Module name   :  cpuhigh
      Module version:  1.0
      Module size   :  151896(Byte)
      Module status :  Valid
  =======End==========Module 4 information============================

  =======Begin========Module 5 information============================
      Module ID     :  0xcd0a0001
      Module name   :  errpkt
      Module version:  1.0
      Module size   :  4056(Byte)
      Module status :  Valid
  =======End==========Module 5 information============================

  =======Begin========Module 6 information============================
      Module ID     :  0xcd0b0001
      Module name   :  spch_task
      Module version:  1.0
      Module size   :  138344(Byte)
      Module status :  Valid
  =======End==========Module 6 information============================

======================================================
  ===============_disp last-version===============
======================================================
No last version information stored.
============================================================================
  ===============_disp memory-allocation-failure reserved===============
============================================================================
No memory allocation failure information stored.
==============================================================
  ===============_disp om cpu-high reserved===============
==============================================================
CPU usage high module is disabled.
Current monitor threshold is 80%.
No CPU usage high information stored.
=====================================================================
  ===============_display om error-packet reserved===============
=====================================================================
Error packet information record module is disabled.
No error packet information stored.
============================================================
  ===============_display history-command===============
============================================================
No last cmd information stored.
=============================================================
  ===============_display om task reserved===============
=============================================================
No task information stored.
=============================================================
  ===============_dis drv ni interrupt all===============
=============================================================
 Dev: 0 Display all Interrupt information.
 Dev: 1 Display all Interrupt information.
===============================================================
  ===============local logbuffer display all===============
===============================================================

Apr 26 2000 12:00:13:
LINE:3958, File ./../../../platform_mvp/drv/qacl/source/drv_qacl_intf.c-TASK:CFM:


 COMP_GetVTable failed!

Apr 26 2000 12:00:13:
LINE:2669, File ./../../../platform_mvp/drv/l3/ip/source/drv_ipv4_intf.c-TASK:RDSO:

 Drv_IPv4_EnableSpecialIpMcToCpu:Drv_Ipv4GetProtocolType(0xffffffff,0x2593ebc) return 0x8


Apr 26 2000 12:00:34:
LINE:67, File ./../../../platform_mvp/drv/poe/source/drv_poe_intf.c-TASK:LLDP:
DRV_IOCTL_COMMON_POE_CAPABILITY_GET error!

Apr 26 2000 12:00:38:
LINE:2695, File ./../../../platform_mvp/drv/ni/source/drv_ni_snd.c-TASK:DHCC:

DRV_Mac_SetPortMaxAddrLearningNum: call IF_GetDataByIfIndex(ulIfIndex 0x0,IF_IFTYPE,0x2533440) fail!


Apr 26 2000 13:11:11:
LINE:2719, File ./../../../platform_mvp/drv/ni/source/drv_ni_snd.c-TASK:IP:

 NI_Tx: ulTrunkId 66 has no member port!

Apr 26 2000 13:19:05:
LINE:1566, File ./../../../platform_mvp/drv/l3/ip/source/drv_vlanif.c-TASK:HDQ0:

 Invalid Table type! type=2

Apr 26 2000 13:19:05:
LINE:883, File ./../../../platform_mvp/drv/l3/ip/source/drv_vlanif.c-TASK:HDQ0:

 Drv_VLANIF_GetMibPhyInfo return error!

Apr 26 2000 15:13:04:
LINE:1097, File ./../../../platform_mvp/drv/l2/port/source/drv_port_lpt.c-TASK:HDQ0:

Drv_Port_LoopBackTest: recieve packets 0 is not more than 2

Apr 26 2000 15:13:04:
LINE:745, File ./../../../platform_mvp/drv/l2/port/source/drv_port_lpt.c-TASK:HDQ0:
Drv_Port_LoopBack  err in Drv_Port_LoopBackTest
Total 9 Records
=================================================================
  ===============_display drv qacl global-info===============
=================================================================

*********************************************************

 Global ACl Info:

  1st Ingress PceIndex = 0   PceNumber(s) = 6

  There are no ACL rules in 2nd lookup of ingress!

  There are no ACL rules in 1st lookup of egress!

  There are no ACL rules in 2nd lookup of egress!

---------------------------------------------------------

 Vlan ACl Info:

  There are no ACL rules!

*********************************************************

 VlanInterface ACl Info:

  There are no ACL rules in 1st lookup of ingress!

  There are no ACL rules in 2nd lookup of ingress!

  There are no ACL rules in 1st lookup of egress!

  There are no ACL rules in 2nd lookup of egress!

---------------------------------------------------------

 Slot1 Ingress PclLkupIndex = -1, Egress PclLkupIndex = -1, 

 Total PceNumber(s) = 6

*********************************************************
==================================================================
  ===============_display drv qacl summary-info===============
==================================================================

*****************************************************************

 HardWare Resource PclNumbers = 256, PceNumbers = 1024

-----------------------------------------------------------------

 FirstLookup:Global & Vlan Ingress PclLkupIndex = 0, PceNumber = 6

 FirstLookup:Global & Vlan Egress  PclLkupIndex = Invalid, PceNumber = 0

 SecendLookup:Global & Vlan Ingress PclLkupIndex = Invalid, PceNumber = 0

 SecendLookup:Global & Vlan Egress  PclLkupIndex = Invalid, PceNumber = 0

-----------------------------------------------------------------

  Port0  Ingress 1st Lookup PclLkupIndex = 1   PceNumber(s) = 1    

  Port1  Ingress 1st Lookup PclLkupIndex = 2   PceNumber(s) = 1    

  Port2  Ingress 1st Lookup PclLkupIndex = 3   PceNumber(s) = 1    

  Port3  Ingress 1st Lookup PclLkupIndex = 4   PceNumber(s) = 1    

  Port4  Ingress 1st Lookup PclLkupIndex = 5   PceNumber(s) = 1    

  Port5  Ingress 1st Lookup PclLkupIndex = 6   PceNumber(s) = 1    

  Port6  Ingress 1st Lookup PclLkupIndex = 7   PceNumber(s) = 1    

  Port7  Ingress 1st Lookup PclLkupIndex = 8   PceNumber(s) = 1    

  Port8  Ingress 1st Lookup PclLkupIndex = 9   PceNumber(s) = 1    

  Port9  Ingress 1st Lookup PclLkupIndex = 10  PceNumber(s) = 1    

  Port10 Ingress 1st Lookup PclLkupIndex = 11  PceNumber(s) = 1    

  Port11 Ingress 1st Lookup PclLkupIndex = 12  PceNumber(s) = 1    

  Port12 Ingress 1st Lookup PclLkupIndex = 13  PceNumber(s) = 1    

  Port13 Ingress 1st Lookup PclLkupIndex = 14  PceNumber(s) = 1    

  Port14 Ingress 1st Lookup PclLkupIndex = 15  PceNumber(s) = 1    

  Port15 Ingress 1st Lookup PclLkupIndex = 16  PceNumber(s) = 1    

  Port16 Ingress 1st Lookup PclLkupIndex = 17  PceNumber(s) = 2    

  Port17 Ingress 1st Lookup PclLkupIndex = 18  PceNumber(s) = 2    

  Port18 Ingress 1st Lookup PclLkupIndex = 19  PceNumber(s) = 2    

  Port19 Ingress 1st Lookup PclLkupIndex = 20  PceNumber(s) = 2    

  Port20 Ingress 1st Lookup PclLkupIndex = 21  PceNumber(s) = 1    

  Port21 Ingress 1st Lookup PclLkupIndex = 22  PceNumber(s) = 1    

  Port22 Ingress 1st Lookup PclLkupIndex = 23  PceNumber(s) = 1    

  Port23 Ingress 1st Lookup PclLkupIndex = 24  PceNumber(s) = 1    

  Port24 Ingress 1st Lookup PclLkupIndex = 25  PceNumber(s) = 1    

  Port25 Ingress 1st Lookup PclLkupIndex = 26  PceNumber(s) = 1    

  Port26 Ingress 1st Lookup PclLkupIndex = 27  PceNumber(s) = 1    

  Port27 Ingress 1st Lookup PclLkupIndex = 28  PceNumber(s) = 1    

  Port28 Ingress 1st Lookup PclLkupIndex = 29  PceNumber(s) = 1    

  Port29 Ingress 1st Lookup PclLkupIndex = 30  PceNumber(s) = 1    

  Port30 Ingress 1st Lookup PclLkupIndex = 31  PceNumber(s) = 1    

  Port31 Ingress 1st Lookup PclLkupIndex = 32  PceNumber(s) = 1    

  Port32 Ingress 1st Lookup PclLkupIndex = 33  PceNumber(s) = 1    

  Port33 Ingress 1st Lookup PclLkupIndex = 34  PceNumber(s) = 1    

  Port34 Ingress 1st Lookup PclLkupIndex = 35  PceNumber(s) = 1    

  Port35 Ingress 1st Lookup PclLkupIndex = 36  PceNumber(s) = 1    

  Port36 Ingress 1st Lookup PclLkupIndex = 37  PceNumber(s) = 1    

  Port37 Ingress 1st Lookup PclLkupIndex = 38  PceNumber(s) = 1    

  Port38 Ingress 1st Lookup PclLkupIndex = 39  PceNumber(s) = 1    

  Port39 Ingress 1st Lookup PclLkupIndex = 40  PceNumber(s) = 1    

  Port40 Ingress 1st Lookup PclLkupIndex = 41  PceNumber(s) = 1    

  Port41 Ingress 1st Lookup PclLkupIndex = 42  PceNumber(s) = 1    

  Port42 Ingress 1st Lookup PclLkupIndex = 43  PceNumber(s) = 1    

  Port43 Ingress 1st Lookup PclLkupIndex = 44  PceNumber(s) = 1    

  Port44 Ingress 1st Lookup PclLkupIndex = 45  PceNumber(s) = 1    

  Port45 Ingress 1st Lookup PclLkupIndex = 46  PceNumber(s) = 1    

  Port46 Ingress 1st Lookup PclLkupIndex = 47  PceNumber(s) = 1    

  Port47 Ingress 1st Lookup PclLkupIndex = 48  PceNumber(s) = 1    

  Port48 Ingress 1st Lookup PclLkupIndex = 49  PceNumber(s) = 1    

  Port49 Ingress 1st Lookup PclLkupIndex = 50  PceNumber(s) = 1    

  Port50 Ingress 1st Lookup PclLkupIndex = 51  PceNumber(s) = 1    

  Port51 Ingress 1st Lookup PclLkupIndex = 52  PceNumber(s) = 1    

-----------------------------------------------------------------

 Used Resource PclNumber(s) = 53, PceNumber(s) = 62

*****************************************************************
===================================================================
  ===============_display drv qacl template-info===============
===================================================================

--2 flowtemplate in system!


Get IPV4 profile failed from DB!

*********************************************

Get IPV4 profile failed from DB!

*********************************************
==================================================================
  ===============_display drv qacl port-info 1 ===============
==================================================================

**********************************************************************

  Direction ingress, searchslot FirstLookup !

  LACP_RULES              has been set! PceIndex = 0     PceNumber = 1   


  Ingress First Lookup PclLkupIndex = 1, PceNumber = 1 

----------------------------------------------------------------------

  Direction ingress, searchslot SecondLookup !

  There are no ACL rules in Port 1 !

----------------------------------------------------------------------

  Direction Egress, Searchslot FirstLookup !

  There are no ACL rules in Port 1 !

----------------------------------------------------------------------

 Port total PceNumber = 1

**********************************************************************
==================================================================
  ===============_display drv qacl port-info 2 ===============
==================================================================

**********************************************************************

  Direction ingress, searchslot FirstLookup !

  LACP_RULES              has been set! PceIndex = 0     PceNumber = 1   


  Ingress First Lookup PclLkupIndex = 2, PceNumber = 1 

----------------------------------------------------------------------

  Direction ingress, searchslot SecondLookup !

  There are no ACL rules in Port 2 !

----------------------------------------------------------------------

  Direction Egress, Searchslot FirstLookup !

  There are no ACL rules in Port 2 !

----------------------------------------------------------------------

 Port total PceNumber = 1

**********************************************************************
==================================================================
  ===============_display drv qacl port-info 3 ===============
==================================================================

**********************************************************************

  Direction ingress, searchslot FirstLookup !

  LACP_RULES              has been set! PceIndex = 0     PceNumber = 1   


  Ingress First Lookup PclLkupIndex = 3, PceNumber = 1 

----------------------------------------------------------------------

  Direction ingress, searchslot SecondLookup !

  There are no ACL rules in Port 3 !

----------------------------------------------------------------------

  Direction Egress, Searchslot FirstLookup !

  There are no ACL rules in Port 3 !

----------------------------------------------------------------------

 Port total PceNumber = 1

**********************************************************************
==================================================================
  ===============_display drv qacl port-info 4 ===============
==================================================================

**********************************************************************

  Direction ingress, searchslot FirstLookup !

  LACP_RULES              has been set! PceIndex = 0     PceNumber = 1   


  Ingress First Lookup PclLkupIndex = 4, PceNumber = 1 

----------------------------------------------------------------------

  Direction ingress, searchslot SecondLookup !

  There are no ACL rules in Port 4 !

----------------------------------------------------------------------

  Direction Egress, Searchslot FirstLookup !

  There are no ACL rules in Port 4 !

----------------------------------------------------------------------

 Port total PceNumber = 1

**********************************************************************
==================================================================
  ===============_display drv qacl port-info 5 ===============
==================================================================

**********************************************************************

  Direction ingress, searchslot FirstLookup !

  LACP_RULES              has been set! PceIndex = 0     PceNumber = 1   


  Ingress First Lookup PclLkupIndex = 5, PceNumber = 1 

----------------------------------------------------------------------

  Direction ingress, searchslot SecondLookup !

  There are no ACL rules in Port 5 !

----------------------------------------------------------------------

  Direction Egress, Searchslot FirstLookup !

  There are no ACL rules in Port 5 !

----------------------------------------------------------------------

 Port total PceNumber = 1

**********************************************************************
==================================================================
  ===============_display drv qacl port-info 6 ===============
==================================================================

**********************************************************************

  Direction ingress, searchslot FirstLookup !

  LACP_RULES              has been set! PceIndex = 0     PceNumber = 1   


  Ingress First Lookup PclLkupIndex = 6, PceNumber = 1 

----------------------------------------------------------------------

  Direction ingress, searchslot SecondLookup !

  There are no ACL rules in Port 6 !

----------------------------------------------------------------------

  Direction Egress, Searchslot FirstLookup !

  There are no ACL rules in Port 6 !

----------------------------------------------------------------------

 Port total PceNumber = 1

**********************************************************************
==================================================================
  ===============_display drv qacl port-info 7 ===============
==================================================================

**********************************************************************

  Direction ingress, searchslot FirstLookup !

  LACP_RULES              has been set! PceIndex = 0     PceNumber = 1   


  Ingress First Lookup PclLkupIndex = 7, PceNumber = 1 

----------------------------------------------------------------------

  Direction ingress, searchslot SecondLookup !

  There are no ACL rules in Port 7 !

----------------------------------------------------------------------

  Direction Egress, Searchslot FirstLookup !

  There are no ACL rules in Port 7 !

----------------------------------------------------------------------

 Port total PceNumber = 1

**********************************************************************
==================================================================
  ===============_display drv qacl port-info 8 ===============
==================================================================

**********************************************************************

  Direction ingress, searchslot FirstLookup !

  LACP_RULES              has been set! PceIndex = 0     PceNumber = 1   


  Ingress First Lookup PclLkupIndex = 8, PceNumber = 1 

----------------------------------------------------------------------

  Direction ingress, searchslot SecondLookup !

  There are no ACL rules in Port 8 !

----------------------------------------------------------------------

  Direction Egress, Searchslot FirstLookup !

  There are no ACL rules in Port 8 !

----------------------------------------------------------------------

 Port total PceNumber = 1

**********************************************************************
==================================================================
  ===============_display drv qacl port-info 9 ===============
==================================================================

**********************************************************************

  Direction ingress, searchslot FirstLookup !

  LACP_RULES              has been set! PceIndex = 0     PceNumber = 1   


  Ingress First Lookup PclLkupIndex = 9, PceNumber = 1 

----------------------------------------------------------------------

  Direction ingress, searchslot SecondLookup !

  There are no ACL rules in Port 9 !

----------------------------------------------------------------------

  Direction Egress, Searchslot FirstLookup !

  There are no ACL rules in Port 9 !

----------------------------------------------------------------------

 Port total PceNumber = 1

**********************************************************************
===================================================================
  ===============_display drv qacl port-info 10 ===============
===================================================================

**********************************************************************

  Direction ingress, searchslot FirstLookup !

  LACP_RULES              has been set! PceIndex = 0     PceNumber = 1   


  Ingress First Lookup PclLkupIndex = 10, PceNumber = 1 

----------------------------------------------------------------------

  Direction ingress, searchslot SecondLookup !

  There are no ACL rules in Port 10 !

----------------------------------------------------------------------

  Direction Egress, Searchslot FirstLookup !

  There are no ACL rules in Port 10 !

----------------------------------------------------------------------

 Port total PceNumber = 1

**********************************************************************
===================================================================
  ===============_display drv qacl port-info 11 ===============
===================================================================

**********************************************************************

  Direction ingress, searchslot FirstLookup !

  LACP_RULES              has been set! PceIndex = 0     PceNumber = 1   


  Ingress First Lookup PclLkupIndex = 11, PceNumber = 1 

----------------------------------------------------------------------

  Direction ingress, searchslot SecondLookup !

  There are no ACL rules in Port 11 !

----------------------------------------------------------------------

  Direction Egress, Searchslot FirstLookup !

  There are no ACL rules in Port 11 !

----------------------------------------------------------------------

 Port total PceNumber = 1

**********************************************************************
===================================================================
  ===============_display drv qacl port-info 12 ===============
===================================================================

**********************************************************************

  Direction ingress, searchslot FirstLookup !

  LACP_RULES              has been set! PceIndex = 0     PceNumber = 1   


  Ingress First Lookup PclLkupIndex = 12, PceNumber = 1 

----------------------------------------------------------------------

  Direction ingress, searchslot SecondLookup !

  There are no ACL rules in Port 12 !

----------------------------------------------------------------------

  Direction Egress, Searchslot FirstLookup !

  There are no ACL rules in Port 12 !

----------------------------------------------------------------------

 Port total PceNumber = 1

**********************************************************************
===================================================================
  ===============_display drv qacl port-info 13 ===============
===================================================================

**********************************************************************

  Direction ingress, searchslot FirstLookup !

  LACP_RULES              has been set! PceIndex = 0     PceNumber = 1   


  Ingress First Lookup PclLkupIndex = 13, PceNumber = 1 

----------------------------------------------------------------------

  Direction ingress, searchslot SecondLookup !

  There are no ACL rules in Port 13 !

----------------------------------------------------------------------

  Direction Egress, Searchslot FirstLookup !

  There are no ACL rules in Port 13 !

----------------------------------------------------------------------

 Port total PceNumber = 1

**********************************************************************
===================================================================
  ===============_display drv qacl port-info 14 ===============
===================================================================

**********************************************************************

  Direction ingress, searchslot FirstLookup !

  LACP_RULES              has been set! PceIndex = 0     PceNumber = 1   


  Ingress First Lookup PclLkupIndex = 14, PceNumber = 1 

----------------------------------------------------------------------

  Direction ingress, searchslot SecondLookup !

  There are no ACL rules in Port 14 !

----------------------------------------------------------------------

  Direction Egress, Searchslot FirstLookup !

  There are no ACL rules in Port 14 !

----------------------------------------------------------------------

 Port total PceNumber = 1

**********************************************************************
===================================================================
  ===============_display drv qacl port-info 15 ===============
===================================================================

**********************************************************************

  Direction ingress, searchslot FirstLookup !

  LACP_RULES              has been set! PceIndex = 0     PceNumber = 1   


  Ingress First Lookup PclLkupIndex = 15, PceNumber = 1 

----------------------------------------------------------------------

  Direction ingress, searchslot SecondLookup !

  There are no ACL rules in Port 15 !

----------------------------------------------------------------------

  Direction Egress, Searchslot FirstLookup !

  There are no ACL rules in Port 15 !

----------------------------------------------------------------------

 Port total PceNumber = 1

**********************************************************************
===================================================================
  ===============_display drv qacl port-info 16 ===============
===================================================================

**********************************************************************

  Direction ingress, searchslot FirstLookup !

  LACP_RULES              has been set! PceIndex = 0     PceNumber = 1   


  Ingress First Lookup PclLkupIndex = 16, PceNumber = 1 

----------------------------------------------------------------------

  Direction ingress, searchslot SecondLookup !

  There are no ACL rules in Port 16 !

----------------------------------------------------------------------

  Direction Egress, Searchslot FirstLookup !

  There are no ACL rules in Port 16 !

----------------------------------------------------------------------

 Port total PceNumber = 1

**********************************************************************
===================================================================
  ===============_display drv qacl port-info 17 ===============
===================================================================

**********************************************************************

  Direction ingress, searchslot FirstLookup !

  LACP_RULES              has been set! PceIndex = 0     PceNumber = 1   

  STP_RULES               has been set! PceIndex = 1     PceNumber = 1   


  Ingress First Lookup PclLkupIndex = 17, PceNumber = 2 

----------------------------------------------------------------------

  Direction ingress, searchslot SecondLookup !

  There are no ACL rules in Port 17 !

----------------------------------------------------------------------

  Direction Egress, Searchslot FirstLookup !

  There are no ACL rules in Port 17 !

----------------------------------------------------------------------

 Port total PceNumber = 2

**********************************************************************
===================================================================
  ===============_display drv qacl port-info 18 ===============
===================================================================

**********************************************************************

  Direction ingress, searchslot FirstLookup !

  LACP_RULES              has been set! PceIndex = 0     PceNumber = 1   

  STP_RULES               has been set! PceIndex = 1     PceNumber = 1   


  Ingress First Lookup PclLkupIndex = 18, PceNumber = 2 

----------------------------------------------------------------------

  Direction ingress, searchslot SecondLookup !

  There are no ACL rules in Port 18 !

----------------------------------------------------------------------

  Direction Egress, Searchslot FirstLookup !

  There are no ACL rules in Port 18 !

----------------------------------------------------------------------

 Port total PceNumber = 2

**********************************************************************
===================================================================
  ===============_display drv qacl port-info 19 ===============
===================================================================

**********************************************************************

  Direction ingress, searchslot FirstLookup !

  LACP_RULES              has been set! PceIndex = 0     PceNumber = 1   

  STP_RULES               has been set! PceIndex = 1     PceNumber = 1   


  Ingress First Lookup PclLkupIndex = 19, PceNumber = 2 

----------------------------------------------------------------------

  Direction ingress, searchslot SecondLookup !

  There are no ACL rules in Port 19 !

----------------------------------------------------------------------

  Direction Egress, Searchslot FirstLookup !

  There are no ACL rules in Port 19 !

----------------------------------------------------------------------

 Port total PceNumber = 2

**********************************************************************
===================================================================
  ===============_display drv qacl port-info 20 ===============
===================================================================

**********************************************************************

  Direction ingress, searchslot FirstLookup !

  LACP_RULES              has been set! PceIndex = 0     PceNumber = 1   

  STP_RULES               has been set! PceIndex = 1     PceNumber = 1   


  Ingress First Lookup PclLkupIndex = 20, PceNumber = 2 

----------------------------------------------------------------------

  Direction ingress, searchslot SecondLookup !

  There are no ACL rules in Port 20 !

----------------------------------------------------------------------

  Direction Egress, Searchslot FirstLookup !

  There are no ACL rules in Port 20 !

----------------------------------------------------------------------

 Port total PceNumber = 2

**********************************************************************
===================================================================
  ===============_display drv qacl port-info 21 ===============
===================================================================

**********************************************************************

  Direction ingress, searchslot FirstLookup !

  LACP_RULES              has been set! PceIndex = 0     PceNumber = 1   


  Ingress First Lookup PclLkupIndex = 21, PceNumber = 1 

----------------------------------------------------------------------

  Direction ingress, searchslot SecondLookup !

  There are no ACL rules in Port 21 !

----------------------------------------------------------------------

  Direction Egress, Searchslot FirstLookup !

  There are no ACL rules in Port 21 !

----------------------------------------------------------------------

 Port total PceNumber = 1

**********************************************************************
===================================================================
  ===============_display drv qacl port-info 22 ===============
===================================================================

**********************************************************************

  Direction ingress, searchslot FirstLookup !

  LACP_RULES              has been set! PceIndex = 0     PceNumber = 1   


  Ingress First Lookup PclLkupIndex = 22, PceNumber = 1 

----------------------------------------------------------------------

  Direction ingress, searchslot SecondLookup !

  There are no ACL rules in Port 22 !

----------------------------------------------------------------------

  Direction Egress, Searchslot FirstLookup !

  There are no ACL rules in Port 22 !

----------------------------------------------------------------------

 Port total PceNumber = 1

**********************************************************************
===================================================================
  ===============_display drv qacl port-info 23 ===============
===================================================================

**********************************************************************

  Direction ingress, searchslot FirstLookup !

  LACP_RULES              has been set! PceIndex = 0     PceNumber = 1   


  Ingress First Lookup PclLkupIndex = 23, PceNumber = 1 

----------------------------------------------------------------------

  Direction ingress, searchslot SecondLookup !

  There are no ACL rules in Port 23 !

----------------------------------------------------------------------

  Direction Egress, Searchslot FirstLookup !

  There are no ACL rules in Port 23 !

----------------------------------------------------------------------

 Port total PceNumber = 1

**********************************************************************
===================================================================
  ===============_display drv qacl port-info 24 ===============
===================================================================

**********************************************************************

  Direction ingress, searchslot FirstLookup !

  LACP_RULES              has been set! PceIndex = 0     PceNumber = 1   


  Ingress First Lookup PclLkupIndex = 24, PceNumber = 1 

----------------------------------------------------------------------

  Direction ingress, searchslot SecondLookup !

  There are no ACL rules in Port 24 !

----------------------------------------------------------------------

  Direction Egress, Searchslot FirstLookup !

  There are no ACL rules in Port 24 !

----------------------------------------------------------------------

 Port total PceNumber = 1

**********************************************************************
===================================================================
  ===============_display drv qacl port-info 25 ===============
===================================================================

**********************************************************************

  Direction ingress, searchslot FirstLookup !

  LACP_RULES              has been set! PceIndex = 0     PceNumber = 1   


  Ingress First Lookup PclLkupIndex = 25, PceNumber = 1 

----------------------------------------------------------------------

  Direction ingress, searchslot SecondLookup !

  There are no ACL rules in Port 25 !

----------------------------------------------------------------------

  Direction Egress, Searchslot FirstLookup !

  There are no ACL rules in Port 25 !

----------------------------------------------------------------------

 Port total PceNumber = 1

**********************************************************************
===================================================================
  ===============_display drv qacl port-info 26 ===============
===================================================================

**********************************************************************

  Direction ingress, searchslot FirstLookup !

  LACP_RULES              has been set! PceIndex = 0     PceNumber = 1   


  Ingress First Lookup PclLkupIndex = 26, PceNumber = 1 

----------------------------------------------------------------------

  Direction ingress, searchslot SecondLookup !

  There are no ACL rules in Port 26 !

----------------------------------------------------------------------

  Direction Egress, Searchslot FirstLookup !

  There are no ACL rules in Port 26 !

----------------------------------------------------------------------

 Port total PceNumber = 1

**********************************************************************
===================================================================
  ===============_display drv qacl port-info 27 ===============
===================================================================

**********************************************************************

  Direction ingress, searchslot FirstLookup !

  LACP_RULES              has been set! PceIndex = 0     PceNumber = 1   


  Ingress First Lookup PclLkupIndex = 27, PceNumber = 1 

----------------------------------------------------------------------

  Direction ingress, searchslot SecondLookup !

  There are no ACL rules in Port 27 !

----------------------------------------------------------------------

  Direction Egress, Searchslot FirstLookup !

  There are no ACL rules in Port 27 !

----------------------------------------------------------------------

 Port total PceNumber = 1

**********************************************************************
===================================================================
  ===============_display drv qacl port-info 28 ===============
===================================================================

**********************************************************************

  Direction ingress, searchslot FirstLookup !

  LACP_RULES              has been set! PceIndex = 0     PceNumber = 1   


  Ingress First Lookup PclLkupIndex = 28, PceNumber = 1 

----------------------------------------------------------------------

  Direction ingress, searchslot SecondLookup !

  There are no ACL rules in Port 28 !

----------------------------------------------------------------------

  Direction Egress, Searchslot FirstLookup !

  There are no ACL rules in Port 28 !

----------------------------------------------------------------------

 Port total PceNumber = 1

**********************************************************************
===================================================================
  ===============_display drv qacl port-info 29 ===============
===================================================================

**********************************************************************

  Direction ingress, searchslot FirstLookup !

  LACP_RULES              has been set! PceIndex = 0     PceNumber = 1   


  Ingress First Lookup PclLkupIndex = 29, PceNumber = 1 

----------------------------------------------------------------------

  Direction ingress, searchslot SecondLookup !

  There are no ACL rules in Port 29 !

----------------------------------------------------------------------

  Direction Egress, Searchslot FirstLookup !

  There are no ACL rules in Port 29 !

----------------------------------------------------------------------

 Port total PceNumber = 1

**********************************************************************
===================================================================
  ===============_display drv qacl port-info 30 ===============
===================================================================

**********************************************************************

  Direction ingress, searchslot FirstLookup !

  LACP_RULES              has been set! PceIndex = 0     PceNumber = 1   


  Ingress First Lookup PclLkupIndex = 30, PceNumber = 1 

----------------------------------------------------------------------

  Direction ingress, searchslot SecondLookup !

  There are no ACL rules in Port 30 !

----------------------------------------------------------------------

  Direction Egress, Searchslot FirstLookup !

  There are no ACL rules in Port 30 !

----------------------------------------------------------------------

 Port total PceNumber = 1

**********************************************************************
===================================================================
  ===============_display drv qacl port-info 31 ===============
===================================================================

**********************************************************************

  Direction ingress, searchslot FirstLookup !

  LACP_RULES              has been set! PceIndex = 0     PceNumber = 1   


  Ingress First Lookup PclLkupIndex = 31, PceNumber = 1 

----------------------------------------------------------------------

  Direction ingress, searchslot SecondLookup !

  There are no ACL rules in Port 31 !

----------------------------------------------------------------------

  Direction Egress, Searchslot FirstLookup !

  There are no ACL rules in Port 31 !

----------------------------------------------------------------------

 Port total PceNumber = 1

**********************************************************************
===================================================================
  ===============_display drv qacl port-info 32 ===============
===================================================================

**********************************************************************

  Direction ingress, searchslot FirstLookup !

  LACP_RULES              has been set! PceIndex = 0     PceNumber = 1   


  Ingress First Lookup PclLkupIndex = 32, PceNumber = 1 

----------------------------------------------------------------------

  Direction ingress, searchslot SecondLookup !

  There are no ACL rules in Port 32 !

----------------------------------------------------------------------

  Direction Egress, Searchslot FirstLookup !

  There are no ACL rules in Port 32 !

----------------------------------------------------------------------

 Port total PceNumber = 1

**********************************************************************
===================================================================
  ===============_display drv qacl port-info 33 ===============
===================================================================

**********************************************************************

  Direction ingress, searchslot FirstLookup !

  LACP_RULES              has been set! PceIndex = 0     PceNumber = 1   


  Ingress First Lookup PclLkupIndex = 33, PceNumber = 1 

----------------------------------------------------------------------

  Direction ingress, searchslot SecondLookup !

  There are no ACL rules in Port 33 !

----------------------------------------------------------------------

  Direction Egress, Searchslot FirstLookup !

  There are no ACL rules in Port 33 !

----------------------------------------------------------------------

 Port total PceNumber = 1

**********************************************************************
===================================================================
  ===============_display drv qacl port-info 34 ===============
===================================================================

**********************************************************************

  Direction ingress, searchslot FirstLookup !

  LACP_RULES              has been set! PceIndex = 0     PceNumber = 1   


  Ingress First Lookup PclLkupIndex = 34, PceNumber = 1 

----------------------------------------------------------------------

  Direction ingress, searchslot SecondLookup !

  There are no ACL rules in Port 34 !

----------------------------------------------------------------------

  Direction Egress, Searchslot FirstLookup !

  There are no ACL rules in Port 34 !

----------------------------------------------------------------------

 Port total PceNumber = 1

**********************************************************************
===================================================================
  ===============_display drv qacl port-info 35 ===============
===================================================================

**********************************************************************

  Direction ingress, searchslot FirstLookup !

  LACP_RULES              has been set! PceIndex = 0     PceNumber = 1   


  Ingress First Lookup PclLkupIndex = 35, PceNumber = 1 

----------------------------------------------------------------------

  Direction ingress, searchslot SecondLookup !

  There are no ACL rules in Port 35 !

----------------------------------------------------------------------

  Direction Egress, Searchslot FirstLookup !

  There are no ACL rules in Port 35 !

----------------------------------------------------------------------

 Port total PceNumber = 1

**********************************************************************
===================================================================
  ===============_display drv qacl port-info 36 ===============
===================================================================

**********************************************************************

  Direction ingress, searchslot FirstLookup !

  LACP_RULES              has been set! PceIndex = 0     PceNumber = 1   


  Ingress First Lookup PclLkupIndex = 36, PceNumber = 1 

----------------------------------------------------------------------

  Direction ingress, searchslot SecondLookup !

  There are no ACL rules in Port 36 !

----------------------------------------------------------------------

  Direction Egress, Searchslot FirstLookup !

  There are no ACL rules in Port 36 !

----------------------------------------------------------------------

 Port total PceNumber = 1

**********************************************************************
===================================================================
  ===============_display drv qacl port-info 37 ===============
===================================================================

**********************************************************************

  Direction ingress, searchslot FirstLookup !

  LACP_RULES              has been set! PceIndex = 0     PceNumber = 1   


  Ingress First Lookup PclLkupIndex = 37, PceNumber = 1 

----------------------------------------------------------------------

  Direction ingress, searchslot SecondLookup !

  There are no ACL rules in Port 37 !

----------------------------------------------------------------------

  Direction Egress, Searchslot FirstLookup !

  There are no ACL rules in Port 37 !

----------------------------------------------------------------------

 Port total PceNumber = 1

**********************************************************************
===================================================================
  ===============_display drv qacl port-info 38 ===============
===================================================================

**********************************************************************

  Direction ingress, searchslot FirstLookup !

  LACP_RULES              has been set! PceIndex = 0     PceNumber = 1   


  Ingress First Lookup PclLkupIndex = 38, PceNumber = 1 

----------------------------------------------------------------------

  Direction ingress, searchslot SecondLookup !

  There are no ACL rules in Port 38 !

----------------------------------------------------------------------

  Direction Egress, Searchslot FirstLookup !

  There are no ACL rules in Port 38 !

----------------------------------------------------------------------

 Port total PceNumber = 1

**********************************************************************
===================================================================
  ===============_display drv qacl port-info 39 ===============
===================================================================

**********************************************************************

  Direction ingress, searchslot FirstLookup !

  LACP_RULES              has been set! PceIndex = 0     PceNumber = 1   


  Ingress First Lookup PclLkupIndex = 39, PceNumber = 1 

----------------------------------------------------------------------

  Direction ingress, searchslot SecondLookup !

  There are no ACL rules in Port 39 !

----------------------------------------------------------------------

  Direction Egress, Searchslot FirstLookup !

  There are no ACL rules in Port 39 !

----------------------------------------------------------------------

 Port total PceNumber = 1

**********************************************************************
===================================================================
  ===============_display drv qacl port-info 40 ===============
===================================================================

**********************************************************************

  Direction ingress, searchslot FirstLookup !

  LACP_RULES              has been set! PceIndex = 0     PceNumber = 1   


  Ingress First Lookup PclLkupIndex = 40, PceNumber = 1 

----------------------------------------------------------------------

  Direction ingress, searchslot SecondLookup !

  There are no ACL rules in Port 40 !

----------------------------------------------------------------------

  Direction Egress, Searchslot FirstLookup !

  There are no ACL rules in Port 40 !

----------------------------------------------------------------------

 Port total PceNumber = 1

**********************************************************************
===================================================================
  ===============_display drv qacl port-info 41 ===============
===================================================================

**********************************************************************

  Direction ingress, searchslot FirstLookup !

  LACP_RULES              has been set! PceIndex = 0     PceNumber = 1   


  Ingress First Lookup PclLkupIndex = 41, PceNumber = 1 

----------------------------------------------------------------------

  Direction ingress, searchslot SecondLookup !

  There are no ACL rules in Port 41 !

----------------------------------------------------------------------

  Direction Egress, Searchslot FirstLookup !

  There are no ACL rules in Port 41 !

----------------------------------------------------------------------

 Port total PceNumber = 1

**********************************************************************
===================================================================
  ===============_display drv qacl port-info 42 ===============
===================================================================

**********************************************************************

  Direction ingress, searchslot FirstLookup !

  LACP_RULES              has been set! PceIndex = 0     PceNumber = 1   


  Ingress First Lookup PclLkupIndex = 42, PceNumber = 1 

----------------------------------------------------------------------

  Direction ingress, searchslot SecondLookup !

  There are no ACL rules in Port 42 !

----------------------------------------------------------------------

  Direction Egress, Searchslot FirstLookup !

  There are no ACL rules in Port 42 !

----------------------------------------------------------------------

 Port total PceNumber = 1

**********************************************************************
===================================================================
  ===============_display drv qacl port-info 43 ===============
===================================================================

**********************************************************************

  Direction ingress, searchslot FirstLookup !

  LACP_RULES              has been set! PceIndex = 0     PceNumber = 1   


  Ingress First Lookup PclLkupIndex = 43, PceNumber = 1 

----------------------------------------------------------------------

  Direction ingress, searchslot SecondLookup !

  There are no ACL rules in Port 43 !

----------------------------------------------------------------------

  Direction Egress, Searchslot FirstLookup !

  There are no ACL rules in Port 43 !

----------------------------------------------------------------------

 Port total PceNumber = 1

**********************************************************************
===================================================================
  ===============_display drv qacl port-info 44 ===============
===================================================================

**********************************************************************

  Direction ingress, searchslot FirstLookup !

  LACP_RULES              has been set! PceIndex = 0     PceNumber = 1   


  Ingress First Lookup PclLkupIndex = 44, PceNumber = 1 

----------------------------------------------------------------------

  Direction ingress, searchslot SecondLookup !

  There are no ACL rules in Port 44 !

----------------------------------------------------------------------

  Direction Egress, Searchslot FirstLookup !

  There are no ACL rules in Port 44 !

----------------------------------------------------------------------

 Port total PceNumber = 1

**********************************************************************
===================================================================
  ===============_display drv qacl port-info 45 ===============
===================================================================

**********************************************************************

  Direction ingress, searchslot FirstLookup !

  LACP_RULES              has been set! PceIndex = 0     PceNumber = 1   


  Ingress First Lookup PclLkupIndex = 45, PceNumber = 1 

----------------------------------------------------------------------

  Direction ingress, searchslot SecondLookup !

  There are no ACL rules in Port 45 !

----------------------------------------------------------------------

  Direction Egress, Searchslot FirstLookup !

  There are no ACL rules in Port 45 !

----------------------------------------------------------------------

 Port total PceNumber = 1

**********************************************************************
===================================================================
  ===============_display drv qacl port-info 46 ===============
===================================================================

**********************************************************************

  Direction ingress, searchslot FirstLookup !

  LACP_RULES              has been set! PceIndex = 0     PceNumber = 1   


  Ingress First Lookup PclLkupIndex = 46, PceNumber = 1 

----------------------------------------------------------------------

  Direction ingress, searchslot SecondLookup !

  There are no ACL rules in Port 46 !

----------------------------------------------------------------------

  Direction Egress, Searchslot FirstLookup !

  There are no ACL rules in Port 46 !

----------------------------------------------------------------------

 Port total PceNumber = 1

**********************************************************************
===================================================================
  ===============_display drv qacl port-info 47 ===============
===================================================================

**********************************************************************

  Direction ingress, searchslot FirstLookup !

  LACP_RULES              has been set! PceIndex = 0     PceNumber = 1   


  Ingress First Lookup PclLkupIndex = 47, PceNumber = 1 

----------------------------------------------------------------------

  Direction ingress, searchslot SecondLookup !

  There are no ACL rules in Port 47 !

----------------------------------------------------------------------

  Direction Egress, Searchslot FirstLookup !

  There are no ACL rules in Port 47 !

----------------------------------------------------------------------

 Port total PceNumber = 1

**********************************************************************
===================================================================
  ===============_display drv qacl port-info 48 ===============
===================================================================

**********************************************************************

  Direction ingress, searchslot FirstLookup !

  LACP_RULES              has been set! PceIndex = 0     PceNumber = 1   


  Ingress First Lookup PclLkupIndex = 48, PceNumber = 1 

----------------------------------------------------------------------

  Direction ingress, searchslot SecondLookup !

  There are no ACL rules in Port 48 !

----------------------------------------------------------------------

  Direction Egress, Searchslot FirstLookup !

  There are no ACL rules in Port 48 !

----------------------------------------------------------------------

 Port total PceNumber = 1

**********************************************************************
===================================================================
  ===============_display drv qacl port-info 49 ===============
===================================================================

**********************************************************************

  Direction ingress, searchslot FirstLookup !

  LACP_RULES              has been set! PceIndex = 0     PceNumber = 1   


  Ingress First Lookup PclLkupIndex = 49, PceNumber = 1 

----------------------------------------------------------------------

  Direction ingress, searchslot SecondLookup !

  There are no ACL rules in Port 49 !

----------------------------------------------------------------------

  Direction Egress, Searchslot FirstLookup !

  There are no ACL rules in Port 49 !

----------------------------------------------------------------------

 Port total PceNumber = 1

**********************************************************************
===================================================================
  ===============_display drv qacl port-info 50 ===============
===================================================================

**********************************************************************

  Direction ingress, searchslot FirstLookup !

  LACP_RULES              has been set! PceIndex = 0     PceNumber = 1   


  Ingress First Lookup PclLkupIndex = 50, PceNumber = 1 

----------------------------------------------------------------------

  Direction ingress, searchslot SecondLookup !

  There are no ACL rules in Port 50 !

----------------------------------------------------------------------

  Direction Egress, Searchslot FirstLookup !

  There are no ACL rules in Port 50 !

----------------------------------------------------------------------

 Port total PceNumber = 1

**********************************************************************
===================================================================
  ===============_display drv qacl port-info 51 ===============
===================================================================

**********************************************************************

  Direction ingress, searchslot FirstLookup !

  LACP_RULES              has been set! PceIndex = 0     PceNumber = 1   


  Ingress First Lookup PclLkupIndex = 51, PceNumber = 1 

----------------------------------------------------------------------

  Direction ingress, searchslot SecondLookup !

  There are no ACL rules in Port 51 !

----------------------------------------------------------------------

  Direction Egress, Searchslot FirstLookup !

  There are no ACL rules in Port 51 !

----------------------------------------------------------------------

 Port total PceNumber = 1

**********************************************************************
===================================================================
  ===============_display drv qacl port-info 52 ===============
===================================================================

**********************************************************************

  Direction ingress, searchslot FirstLookup !

  LACP_RULES              has been set! PceIndex = 0     PceNumber = 1   


  Ingress First Lookup PclLkupIndex = 52, PceNumber = 1 

----------------------------------------------------------------------

  Direction ingress, searchslot SecondLookup !

  There are no ACL rules in Port 52 !

----------------------------------------------------------------------

  Direction Egress, Searchslot FirstLookup !

  There are no ACL rules in Port 52 !

----------------------------------------------------------------------

 Port total PceNumber = 1

**********************************************************************
========================================================
  ===============display  mac-address===============
========================================================
MAC ADDR        VLAN ID  STATE           PORT INDEX                AGING TIME(s)
1cc1-de7b-226c  1        LEARNED         Bridge-Aggregation1       AGING
d485-6444-19f0  1        LEARNED         Bridge-Aggregation1       AGING
d485-645b-f6ca  1        LEARNED         Bridge-Aggregation2       AGING


  ---  3 MAC address(es) found  ---
============================================================
  ===============display ip routing-table===============
============================================================
Routing Tables: Public
	Destinations : 4	Routes : 4

Destination/Mask    Proto  Pre  Cost         NextHop         Interface

127.0.0.0/8         Direct 0    0            127.0.0.1       InLoop0
127.0.0.1/32        Direct 0    0            127.0.0.1       InLoop0
192.168.250.0/24    Direct 0    0            192.168.250.10  Vlan1
192.168.250.10/32   Direct 0    0            127.0.0.1       InLoop0
