SQM ( 10.252.64.144 ) Server: 
# alias memcstm='echo '\''selclass qualifier memory;info;wait;infolog'\'' |cstm ' 
# memcstm 
Running Command File (/usr/sbin/stm/ui/config/.stmrc). 
-- Information -- 
Support Tools Manager 
Version C.54.10 
Product Number B4708AA 
(C) Copyright Hewlett Packard Co. 1995-2006 
All Rights Reserved 
Use of this program is subject to the licensing restrictions described 
in "Help-->On Version". HP shall not be liable for any damages resulting 
from misuse or unauthorized use of this program. 
cstm>selclass qualifier memory;info;wait;infolog 
^-- Unknown list entry. -- 
The list entry (memory) is undefined. 
^-- (Information) is currently disabled. -- 
^-- (InfoLog) is currently disabled. -- 
cstm>#. 
=========================== 
# machinfo 
CPU info: 
Number of CPUs = 6 
Clock speed = 1600 MHz 
Bus speed = 400 MT/s 
CPUID registers 
vendor information = "GenuineIntel" 
processor serial number = 0x0000000000000000 
processor version info = 0x0000000020000704 
architecture revision: 0 
processor family: 32 Intel(R) Itanium 2 9000 series 
processor model: 0 Intel(R) Itanium 2 9000 series 
processor revision: 7 Stepping C2 
largest CPUID reg: 4 
processor capabilities = 0x0000000000000005 
implements long branch: 1 
implements 16-byte atomic operations: 1 
Bus features 
implemented = 0xbdf0000020000000 
selected = 0x0000000000000000 
Cache info (per core): 
L1 Instruction: size = 16 KB, associativity = 4 
L1 Data: size = 16 KB, associativity = 4 
L2 Instruction: size = 1024 KB, associativity = 8 
L2 Data: size = 256 KB, associativity = 8 
L3 Unified: size = 9216 KB, associativity = 9 
Memory = 24546 MB (23.970703 GB) 
Firmware info: 
Firmware revision = 04.21 
FP SWA driver revision: 1.18 
IPMI is supported on this system. 
BMC version: 4.05 
Platform info: 
model string = "ia64 hp" 
machine id number = b22999da-efc2-11db-9ebb-30843f8fc140 
machine serial number = SGH471153D 
OS info: 
sysname = HP-UX 
nodename = SQM 
release = B.11.23 
version = U (unlimited-user license) 
machine = ia64 
idnumber = 2989070810 
vmunix _release_version: 
@(#) $Revision: vmunix: B11.23_LR FLAVOR=perf Fri Aug 29 22:35:38 PDT 2003 $ 
SQMDD ( 10.252.65.84 ) Server: 
# alias memcstm='echo '\''selclass qualifier memory;info;wait;infolog'\'' |cstm ' 
# memcstm 
Running Command File (/usr/sbin/stm/ui/config/.stmrc). 
-- Information -- 
Support Tools Manager 
Version C.62.00 
Product Number B4708AA 
(C) Copyright Hewlett Packard Co. 1995-2008 
All Rights Reserved 
Use of this program is subject to the licensing restrictions described 
in "Help-->On Version". HP shall not be liable for any damages resulting 
from misuse or unauthorized use of this program. 
cstm>selclass qualifier memory;info;wait;infolog 
-- Updating Map -- 
Updating Map... 
-- Converting a (5540) byte raw log file to text. -- 
Preparing the Information Tool Log for IPF_MEMORY on path memory File ... 
.... sqmdd : 10.252.65.84 .... 
-- Information Tool Log for IPF_MEMORY on path memory -- 
Log creation time: Thu Jun 4 03:22:46 2009 
Hardware path: memory 
Basic Memory Description 
Module Type: MEMORY 
Page Size: 4096 Bytes 
Total Physical Memory: N/A 
Total Configured Memory: 65536 MB 
Total Deconfigured Memory: N/A 
Memory Board Inventory 
DIMM Location Size(MB) DIMM Location Size(MB) 
-------------------- -------- -------------------- -------- 
Ext 0 DIMM 0A 2048 Ext 0 DIMM 0B 2048 
Ext 0 DIMM 0C 2048 Ext 0 DIMM 0D 2048 
Ext 0 DIMM 1A 2048 Ext 0 DIMM 1B 2048 
Ext 0 DIMM 1C 2048 Ext 0 DIMM 1D 2048 
Ext 0 DIMM 2A 2048 Ext 0 DIMM 2B 2048 
Ext 0 DIMM 2C 2048 Ext 0 DIMM 2D 2048 
Ext 0 DIMM 3A 2048 Ext 0 DIMM 3B 2048 
Ext 0 DIMM 3C 2048 Ext 0 DIMM 3D 2048 
Ext 0 DIMM 4A ---- Ext 0 DIMM 4B ---- 
Ext 0 DIMM 4C ---- Ext 0 DIMM 4D ---- 
Ext 0 DIMM 5A ---- Ext 0 DIMM 5B ---- 
Ext 0 DIMM 5C ---- Ext 0 DIMM 5D ---- 
Ext 0 Total: 32768 (MB) 
=========================================================================== 
DIMM Location Size(MB) DIMM Location Size(MB) 
-------------------- -------- -------------------- -------- 
Ext 1 DIMM 0A 2048 Ext 1 DIMM 0B 2048 
Ext 1 DIMM 0C 2048 Ext 1 DIMM 0D 2048 
Ext 1 DIMM 1A 2048 Ext 1 DIMM 1B 2048 
Ext 1 DIMM 1C 2048 Ext 1 DIMM 1D 2048 
Ext 1 DIMM 2A 2048 Ext 1 DIMM 2B 2048 
Ext 1 DIMM 2C 2048 Ext 1 DIMM 2D 2048 
Ext 1 DIMM 3A 2048 Ext 1 DIMM 3B 2048 
Ext 1 DIMM 3C 2048 Ext 1 DIMM 3D 2048 
Ext 1 DIMM 4A ---- Ext 1 DIMM 4B ---- 
Ext 1 DIMM 4C ---- Ext 1 DIMM 4D ---- 
Ext 1 DIMM 5A ---- Ext 1 DIMM 5B ---- 
Ext 1 DIMM 5C ---- Ext 1 DIMM 5D ---- 
Ext 1 Total: 32768 (MB) 
=========================================================================== 
Memory Error Log Summary 
The memory error log is empty. 
Page Deallocation Table (PDT) 
The Page Deallocation Table is empty. 
PDT Entries Used: 0 
PDT Entries Free: 100 
PDT Total Size: 100 
-- Information Tool Log for IPF_MEMORY on path memory -- 
View - To View the file. 
Print - To Print the file. 
SaveAs - To Save the file. 
Enter Done, Help, Print, SaveAs, or View: [Done] #. 
=========================== 
# machinfo 
CPU info: 
Number of CPUs = 8 
Clock speed = 1595 MHz 
Bus speed = 532 MT/s 
CPUID registers 
vendor information = "GenuineIntel" 
processor serial number = 0x0000000000000000 
processor version info = 0x0000000020010104 
architecture revision: 0 
processor family: 32 Intel(R) Itanium 2 9100 series 
processor model: 1 Intel(R) Itanium 2 9100 series 
processor revision: 1 Stepping A1 
largest CPUID reg: 4 
processor capabilities = 0x0000000000000005 
implements long branch: 1 
implements 16-byte atomic operations: 1 
Bus features 
implemented = 0xbdf0000020000000 
selected = 0x0000000000000000 
Cache info (per core): 
L1 Instruction: size = 16 KB, associativity = 4 
L1 Data: size = 16 KB, associativity = 4 
L2 Instruction: size = 1024 KB, associativity = 8 
L2 Data: size = 256 KB, associativity = 8 
L3 Unified: size = 12288 KB, associativity = 12 
Memory = 65505 MB (63.969727 GB) 
Firmware info: 
Firmware revision = 04.03 
FP SWA driver revision: 1.18 
IPMI is supported on this system. 
ERROR: Unable to obtain manageability firmware revision info. 
Platform info: 
model string = "ia64 hp server rx6600" 
machine id number = 4006773f-25ec-11de-a8f1-d93cc4a97c5a 
machine serial number = SGH4910LH2 
OS info: 
sysname = HP-UX 
nodename = sqmdd 
release = B.11.23 
version = U (unlimited-user license) 
machine = ia64 
idnumber = 1074165567 
vmunix _release_version: 
@(#) $Revision: vmunix: B11.23_LR FLAVOR=perf Fri Aug 29 22:35:38 PDT 2003 $