>------------ Event Monitoring Service Event Notification ------------<

Notification Time: Tue Jun 23 13:25:05 2009

qhcha2 sent Event Monitor notification information:

/adapters/events/ql_adapter/0_2_1_0_4_0 is >= 3.
Its current value is CRITICAL(5).

Event data from monitor:

Event Time..........: Tue Jun 23 13:25:05 2009
Severity............: CRITICAL
Monitor.............: dm_ql_adapter
Event #.............: 48                  
System..............: qhcha2

Summary:
     Adapter at hardware path 0/2/1/0/4/0 : For backward compatibility
domain 8
     (private loop) is not allowed. 

Description of Error:

 lbolt value: 1075502644 

   For backward compatibility domain 8 (private loop) is not allowed. 

Probable Cause / Recommended Action:

   Configure the switch to assign a domain value other than 8.
   Domains > 8 will not be recognized till this problem is fixed.

Additional Event Data: 
     System IP Address...: 10.100.45.11
     Event Id............: 0x4a410ff100000000
     Monitor Version.....: B.02.00
     Event Class.........: I/O
     Client Configuration File...........:
     /var/stm/config/tools/monitor/default_dm_ql_adapter.clcfg 
     Client Configuration File Version...: A.02.00 
          Qualification criteria met.
               Number of events..: 1 
     Associated OS error log entry id(s): 
          0x4a410fed00000000
     Additional System Data:
          System Model Number.............: ia64 hp server rx4640 
          OS Version......................: B.11.23 
          EMS Version.....................: A.04.10 
          STM Version.....................: C.46.00 
     Latest information on this event:
 
http://docs.hp.com/hpux/content/hardware/ems/dm_ql_adapter.htm#48

v-v-v-v-v-v-v-v-v-v-v-v-v    D  E  T  A  I  L  S
v-v-v-v-v-v-v-v-v-v-v-v-v

Component Data: 
    Physical Device Path....: 0/2/1/0/4/0

I/O Log Event Data: 

     Driver Status Code..................: 0x00000030 
     Length of Logged Hardware Status....: 0 bytes. 
     Offset to Logged Manager Information: 0 bytes. 
     Length of Logged Manager Information: 65 bytes. 

Manager-Specific Information: 

Raw data from FCMS Adapter driver:  
00000001 401ADE34 00000000 00000001 2F75782F 636F7265 2F697375 2F464344 
2F6B6572 6E2F7372 632F636F 6D6D6F6E 2F777369 6F2F6663 645F7072 6F62652E 
63

>---------- End Event Monitoring Service Event Notification ----------<

--------------------------------------------------------------------------------------------------------------

root@qhcha2#ioscan -fnC disk
Class     I  H/W Path       Driver     S/W State   H/W Type     Description
============================================================================
disk      0  0/0/3/0.0.0.0  sdisk      CLAIMED     DEVICE       TEAC    DV-28E-C
                           /dev/dsk/c0t0d0   /dev/rdsk/c0t0d0
disk     10  0/1/1/0.0.0    sdisk      CLAIMED     DEVICE       HP 73.4GST373453LC
                           /dev/dsk/c2t0d0     /dev/dsk/c2t0d0s2   /dev/rdsk/c2t0d0    /dev/rdsk/c2t0d0s2
                           /dev/dsk/c2t0d0s1   /dev/dsk/c2t0d0s3   /dev/rdsk/c2t0d0s1  /dev/rdsk/c2t0d0s3
disk     11  0/1/1/0.1.0    sdisk      CLAIMED     DEVICE       HP 73.4GST373453LC
                           /dev/dsk/c2t1d0     /dev/dsk/c2t1d0s2   /dev/rdsk/c2t1d0    /dev/rdsk/c2t1d0s2
                           /dev/dsk/c2t1d0s1   /dev/dsk/c2t1d0s3   /dev/rdsk/c2t1d0s1  /dev/rdsk/c2t1d0s3
disk      1  0/2/1/0/4/0.2.0.0.0.0.0   sdisk      CLAIMED     DEVICE       DGC     CX500WDR10
                           /dev/dsk/c4t0d0   /dev/rdsk/c4t0d0
disk      2  0/2/1/0/4/0.2.0.0.0.0.1   sdisk      CLAIMED     DEVICE       DGC     CX500WDR10
                           /dev/dsk/c4t0d1   /dev/rdsk/c4t0d1
disk      3  0/2/1/0/4/0.2.0.0.0.0.2   sdisk      CLAIMED     DEVICE       DGC     CX500WDR5
                           /dev/dsk/c4t0d2   /dev/rdsk/c4t0d2
disk     12  0/2/1/0/4/0.2.0.0.0.0.3   sdisk      CLAIMED     DEVICE       DGC     CX500WDR1
                           /dev/dsk/c4t0d3   /dev/rdsk/c4t0d3
disk     29  0/2/1/0/4/0.2.0.0.0.0.4   sdisk      CLAIMED     DEVICE       DGC     CX500WDR5
                           /dev/dsk/c4t0d4   /dev/rdsk/c4t0d4
disk     34  0/2/1/0/4/0.2.0.0.0.0.5   sdisk      CLAIMED     DEVICE       DGC     CX500WDR5
                           /dev/dsk/c4t0d5   /dev/rdsk/c4t0d5
disk     37  0/2/1/0/4/0.2.0.0.0.0.6   sdisk      CLAIMED     DEVICE       DGC     CX500WDR5
                           /dev/dsk/c4t0d6   /dev/rdsk/c4t0d6
disk     19  0/2/1/0/4/0.2.8.0.0.0.0   sdisk      CLAIMED     DEVICE       DGC     CX500WDR10
                           /dev/dsk/c13t0d0   /dev/rdsk/c13t0d0
disk     18  0/2/1/0/4/0.2.8.0.0.0.1   sdisk      CLAIMED     DEVICE       DGC     CX500WDR10
                           /dev/dsk/c13t0d1   /dev/rdsk/c13t0d1
disk     20  0/2/1/0/4/0.2.8.0.0.0.2   sdisk      CLAIMED     DEVICE       DGC     CX500WDR5
                           /dev/dsk/c13t0d2   /dev/rdsk/c13t0d2
disk     21  0/2/1/0/4/0.2.8.0.0.0.3   sdisk      CLAIMED     DEVICE       DGC     CX500WDR1
                           /dev/dsk/c13t0d3   /dev/rdsk/c13t0d3
disk     30  0/2/1/0/4/0.2.8.0.0.0.4   sdisk      CLAIMED     DEVICE       DGC     CX500WDR5
                           /dev/dsk/c13t0d4   /dev/rdsk/c13t0d4
disk     33  0/2/1/0/4/0.2.8.0.0.0.5   sdisk      CLAIMED     DEVICE       DGC     CX500WDR5
                           /dev/dsk/c13t0d5   /dev/rdsk/c13t0d5
disk     38  0/2/1/0/4/0.2.8.0.0.0.6   sdisk      CLAIMED     DEVICE       DGC     CX500WDR5
                           /dev/dsk/c13t0d6   /dev/rdsk/c13t0d6
disk      5  0/5/1/0/4/0.1.0.0.0.0.0   sdisk      CLAIMED     DEVICE       DGC     CX500WDR10
                           /dev/dsk/c6t0d0   /dev/rdsk/c6t0d0
disk      6  0/5/1/0/4/0.1.0.0.0.0.1   sdisk      CLAIMED     DEVICE       DGC     CX500WDR10
                           /dev/dsk/c6t0d1   /dev/rdsk/c6t0d1
disk      8  0/5/1/0/4/0.1.0.0.0.0.2   sdisk      CLAIMED     DEVICE       DGC     CX500WDR5
                           /dev/dsk/c6t0d2   /dev/rdsk/c6t0d2
disk     13  0/5/1/0/4/0.1.0.0.0.0.3   sdisk      CLAIMED     DEVICE       DGC     CX500WDR1
                           /dev/dsk/c6t0d3   /dev/rdsk/c6t0d3
disk     32  0/5/1/0/4/0.1.0.0.0.0.4   sdisk      CLAIMED     DEVICE       DGC     CX500WDR5
                           /dev/dsk/c6t0d4   /dev/rdsk/c6t0d4
disk     35  0/5/1/0/4/0.1.0.0.0.0.5   sdisk      CLAIMED     DEVICE       DGC     CX500WDR5
                           /dev/dsk/c6t0d5   /dev/rdsk/c6t0d5
disk     40  0/5/1/0/4/0.1.0.0.0.0.6   sdisk      CLAIMED     DEVICE       DGC     CX500WDR5
                           /dev/dsk/c6t0d6   /dev/rdsk/c6t0d6
disk     16  0/5/1/0/4/0.1.8.0.0.0.0   sdisk      CLAIMED     DEVICE       DGC     CX500WDR10
                           /dev/dsk/c14t0d0   /dev/rdsk/c14t0d0
disk     23  0/5/1/0/4/0.1.8.0.0.0.1   sdisk      CLAIMED     DEVICE       DGC     CX500WDR10
                           /dev/dsk/c14t0d1   /dev/rdsk/c14t0d1
disk     25  0/5/1/0/4/0.1.8.0.0.0.2   sdisk      CLAIMED     DEVICE       DGC     CX500WDR5
                           /dev/dsk/c14t0d2   /dev/rdsk/c14t0d2
disk     27  0/5/1/0/4/0.1.8.0.0.0.3   sdisk      CLAIMED     DEVICE       DGC     CX500WDR1
                           /dev/dsk/c14t0d3   /dev/rdsk/c14t0d3
disk     31  0/5/1/0/4/0.1.8.0.0.0.4   sdisk      CLAIMED     DEVICE       DGC     CX500WDR5
                           /dev/dsk/c14t0d4   /dev/rdsk/c14t0d4
disk     36  0/5/1/0/4/0.1.8.0.0.0.5   sdisk      CLAIMED     DEVICE       DGC     CX500WDR5
                           /dev/dsk/c14t0d5   /dev/rdsk/c14t0d5
disk     39  0/5/1/0/4/0.1.8.0.0.0.6   sdisk      CLAIMED     DEVICE       DGC     CX500WDR5
                           /dev/dsk/c14t0d6   /dev/rdsk/c14t0d6
disk      4  0/5/1/0/4/0.3.0.0.0.0.0   sdisk      CLAIMED     DEVICE       DGC     CX4-240WDUNB
                           /dev/dsk/c8t0d0   /dev/rdsk/c8t0d0
disk     42  0/5/1/0/4/0.3.0.0.0.0.7   sdisk      CLAIMED     DEVICE       DGC     CX4-240WDVR
                           /dev/dsk/c8t0d7   /dev/rdsk/c8t0d7
disk     44  0/5/1/0/4/0.3.0.0.0.1.0   sdisk      CLAIMED     DEVICE       DGC     CX4-240WDVR
                           /dev/dsk/c8t1d0   /dev/rdsk/c8t1d0
disk     46  0/5/1/0/4/0.3.0.0.0.1.1   sdisk      CLAIMED     DEVICE       DGC     CX4-240WDVR
                           /dev/dsk/c8t1d1   /dev/rdsk/c8t1d1
disk     47  0/5/1/0/4/0.3.0.0.0.1.2   sdisk      CLAIMED     DEVICE       DGC     CX4-240WDVR
                           /dev/dsk/c8t1d2   /dev/rdsk/c8t1d2
disk     49  0/5/1/0/4/0.3.0.0.0.1.3   sdisk      CLAIMED     DEVICE       DGC     CX4-240WDVR
                           /dev/dsk/c8t1d3   /dev/rdsk/c8t1d3
disk     41  0/5/1/0/4/0.3.10.0.0.0.0  sdisk      CLAIMED     DEVICE       DGC     CX4-240WDUNB
                           /dev/dsk/c16t0d0   /dev/rdsk/c16t0d0
disk     43  0/5/1/0/4/0.3.10.0.0.0.7  sdisk      CLAIMED     DEVICE       DGC     CX4-240WDVR
                           /dev/dsk/c16t0d7   /dev/rdsk/c16t0d7
disk     45  0/5/1/0/4/0.3.10.0.0.1.0  sdisk      CLAIMED     DEVICE       DGC     CX4-240WDVR
                           /dev/dsk/c16t1d0   /dev/rdsk/c16t1d0
disk     48  0/5/1/0/4/0.3.10.0.0.1.1  sdisk      CLAIMED     DEVICE       DGC     CX4-240WDVR
                           /dev/dsk/c16t1d1   /dev/rdsk/c16t1d1
disk     50  0/5/1/0/4/0.3.10.0.0.1.2  sdisk      CLAIMED     DEVICE       DGC     CX4-240WDVR
                           /dev/dsk/c16t1d2   /dev/rdsk/c16t1d2
disk     51  0/5/1/0/4/0.3.10.0.0.1.3  sdisk      CLAIMED     DEVICE       DGC     CX4-240WDVR
                           /dev/dsk/c16t1d3   /dev/rdsk/c16t1d3