XFree86 Version 4.0.3 / X Window System
(protocol Version 11, revision 0, vendor release 6400)
Release Date: 16 March 2001
	If the server is older than 6-12 months, or if your card is
	newer than the above date, look for a newer version before
	reporting problems.  (See <http://www.XFree86.Org/FAQ>) Operating System: Linux 2.2.17-8smp i686 [ELF] 
Module Loader present
(==) Log file: "/var/log/XFree86.0.log", Time: Tue Apr  2 09:26:32 2002
(==) Using config file: "/etc/X11/XF86Config-4"
Markers: (--) probed, (**) from config file, (==) default setting,
         (++) from command line, (!!) notice, (II) informational,
         (WW) warning, (EE) error, (??) unknown.
(==) ServerLayout "Anaconda Configured"
(**) |-->Screen "Screen0" (0)
(**) |   |-->Monitor "Monitor0"
(**) |   |-->Device "ATI Mach64"
(**) |-->Input Device "Mouse0"
(**) |-->Input Device "Keyboard0"
(**) XKB: rules: "xfree86"
(**) XKB: model: "pc101"
(**) XKB: layout: "us"
(**) FontPath set to "unix/:7100"
(**) RgbPath set to "/usr/X11R6/lib/X11/rgb"
(==) ModulePath set to "/usr/X11R6/lib/modules"
(--) using VT number 7

(II) Loading /usr/X11R6/lib/modules/fonts/libbitmap.a
(II) Module bitmap: vendor="The XFree86 Project"
	compiled for 4.0.3, module version = 1.0.0
(II) Loading /usr/X11R6/lib/modules/libpcidata.a
(II) Module pcidata: vendor="The XFree86 Project"
	compiled for 4.0.3, module version = 0.1.0
(II) Loading /usr/X11R6/lib/modules/libscanpci.a
(II) Module scanpci: vendor="The XFree86 Project"
	compiled for 4.0.3, module version = 0.1.0
(II) Unloading /usr/X11R6/lib/modules/libscanpci.a
(--) PCI:*(1:0:0) ATI Mach64 GM rev 39, Mem @ 0xfd000000/24, 0xfe4ff000/12, I/O @ 0xa800/8
(II) Loading /usr/X11R6/lib/modules/extensions/libGLcore.a
(II) Module GLcore: vendor="The XFree86 Project"
	compiled for 4.0.3, module version = 1.0.0
(II) Loading /usr/X11R6/lib/modules/extensions/libdbe.a
(II) Module dbe: vendor="The XFree86 Project"
	compiled for 4.0.3, module version = 1.0.0
(II) Loading /usr/X11R6/lib/modules/extensions/libextmod.a
(II) Module extmod: vendor="The XFree86 Project"
	compiled for 4.0.3, module version = 1.0.0
(II) Loading /usr/X11R6/lib/modules/linux/libfbdevhw.a
(II) Module fbdevhw: vendor="The XFree86 Project"
	compiled for 4.0.3, module version = 0.0.2
(II) Loading /usr/X11R6/lib/modules/extensions/libpex5.a
(II) Module pex5: vendor="The XFree86 Project"
	compiled for 4.0.3, module version = 1.0.0
(II) Loading /usr/X11R6/lib/modules/extensions/libdri.a
(II) Module dri: vendor="The XFree86 Project"
	compiled for 4.0.3, module version = 1.0.0
(II) Loading /usr/X11R6/lib/modules/linux/libdrm.a
(II) Module drm: vendor="The XFree86 Project"
	compiled for 4.0.3, module version = 1.0.0
(II) Loading /usr/X11R6/lib/modules/extensions/libglx.a
(II) Module glx: vendor="The XFree86 Project"
	compiled for 4.0.3, module version = 1.0.0
(II) Loading /usr/X11R6/lib/modules/extensions/librecord.a
(II) Module record: vendor="The XFree86 Project"
	compiled for 4.0.3, module version = 1.13.0
(II) Loading /usr/X11R6/lib/modules/extensions/libxie.a
(II) Module xie: vendor="The XFree86 Project"
	compiled for 4.0.3, module version = 1.0.0
(II) Loading /usr/X11R6/lib/modules/drivers/ati_drv.o
(II) Module ati: vendor="The XFree86 Project"
	compiled for 4.0.3, module version = 6.2.3
(II) Loading /usr/X11R6/lib/modules/input/mouse_drv.o
(II) Module mouse: vendor="The XFree86 Project"
	compiled for 4.0.3, module version = 1.0.0
(II) ATI: ATI driver (version 6.2.3) for chipsets: ati, ativga
(II) R128: Driver for ATI Rage 128 chipsets: ATI Rage 128 RE (PCI),
	ATI Rage 128 RF (AGP), ATI Rage 128 RG (AGP), ATI Rage 128 RK (PCI),
	ATI Rage 128 RL (AGP), ATI Rage 128 Pro PD (AGP),
	ATI Rage 128 Pro PF (AGP), ATI Rage 128 Mobility LE (PCI),
	ATI Rage 128 Mobility LF (AGP), ATI Rage 128 Mobility MF (AGP),
	ATI Rage 128 Mobility ML (AGP)
(II) RADEON: Driver for ATI Radeon chipsets: ATI Radeon QD (AGP),
	ATI Radeon QE (AGP), ATI Radeon QF (AGP), ATI Radeon QG (AGP)
(II) Loading /usr/X11R6/lib/modules/drivers/atimisc_drv.o
(II) Module ati: vendor="The XFree86 Project"
	compiled for 4.0.3, module version = 6.2.3
(==) ATI(0): Chipset:  "ati".
(**) ATI(0): Depth 16, (--) framebuffer bpp 16
(II) Loading /usr/X11R6/lib/modules/linux/libint10.a
(II) Module int10: vendor="The XFree86 Project"
	compiled for 4.0.3, module version = 1.0.0
(II) ATI(0): Primary V_BIOS segment is: 0xc000
(II) Loading /usr/X11R6/lib/modules/libddc.a
(II) Module ddc: vendor="The XFree86 Project"
	compiled for 4.0.3, module version = 1.0.0
(II) Loading /usr/X11R6/lib/modules/libvbe.a
(II) Module vbe: vendor="The XFree86 Project"
	compiled for 4.0.3, module version = 1.0.0
(II) ATI(0): VESA BIOS detected
(II) ATI(0): VESA VBE DDC supported
(--) ATI(0): ATI 3D Rage XL or XC graphics controller detected.
(--) ATI(0): Chip type 474D "GM", version 7, foundry TSMC, class 0, revision 0x00.
(--) ATI(0): AGP bus interface detected;  block I/O base is 0xA800.
(--) ATI(0): ATI Mach64 adapter detected.
(--) ATI(0): Internal RAMDAC (subtype 1) detected.
(==) ATI(0): RGB weight 565
(==) ATI(0): Default visual is TrueColor
(==) ATI(0): Using gamma correction (1.0, 1.0, 1.0)
(II) ATI(0): Using Mach64 accelerator CRTC.
(II) ATI(0): Using 8 MB linear aperture at 0xFD000000.
(II) ATI(0): Using Block 0 MMIO aperture at 0xFE4FF400.
(II) ATI(0): Using Block 1 MMIO aperture at 0xFE4FF000.
(WW) ATI(0): Failed to set up write-combining range (0xfd000000,0x800000)
(II) ATI(0): MMIO write caching enabled.
(--) ATI(0): 8192 kB of SGRAM (2:1) 32-bit detected.
(WW) ATI(0): Cannot shadow an accelerated frame buffer.
(--) ATI(0): Internal programmable clock generator detected.
(--) ATI(0): Reference clock 157.5/11 (14.318) MHz.
(II) ATI(0): Monitor0: Using hsync range of 30.00-65.00 kHz
(II) ATI(0): Monitor0: Using vrefresh range of 50.00-100.00 Hz
(II) ATI(0): Maximum clock: 230.00 MHz
(WW) ATI(0): Mode "1400x1050" deleted (hsync out of range)
(WW) ATI(0): Mode "1400x1050" deleted (hsync out of range)
(WW) ATI(0): Mode "1400x1050" deleted (hsync out of range)
(WW) ATI(0): Mode "1400x1050" deleted (hsync out of range)
(WW) ATI(0): Default mode "1024x768" deleted (hsync out of range)
(WW) ATI(0): Default mode "1152x864" deleted (hsync out of range)
(WW) ATI(0): Default mode "1280x960" deleted (hsync out of range)
(WW) ATI(0): Default mode "1280x1024" deleted (hsync out of range)
(WW) ATI(0): Default mode "1280x1024" deleted (hsync out of range)
(WW) ATI(0): Default mode "1600x1200" deleted (hsync out of range)
(WW) ATI(0): Default mode "1600x1200" deleted (hsync out of range)
(WW) ATI(0): Default mode "1600x1200" deleted (hsync out of range)
(WW) ATI(0): Default mode "1600x1200" deleted (hsync out of range)
(WW) ATI(0): Default mode "1600x1200" deleted (hsync out of range)
(WW) ATI(0): Default mode "1792x1344" deleted (hsync out of range)
(WW) ATI(0): Default mode "1792x1344" deleted (bad mode clock/interlace/doublescan)
(WW) ATI(0): Default mode "1856x1392" deleted (hsync out of range)
(WW) ATI(0): Default mode "1856x1392" deleted (bad mode clock/interlace/doublescan)
(WW) ATI(0): Default mode "1920x1440" deleted (bad mode clock/interlace/doublescan)
(WW) ATI(0): Default mode "1920x1440" deleted (bad mode clock/interlace/doublescan)
(--) ATI(0): Virtual size is 1024x768 (pitch 1024)
(**) ATI(0): Default mode "1024x768": 78.8 MHz, 60.1 kHz, 75.1 Hz
(==) ATI(0): DPI set to (75, 75)
(II) Loading /usr/X11R6/lib/modules/libxaa.a
(II) Module xaa: vendor="The XFree86 Project"
	compiled for 4.0.3, module version = 1.0.0
(II) Loading /usr/X11R6/lib/modules/libcfb16.a
(II) Module cfb16: vendor="The XFree86 Project"
	compiled for 4.0.3, module version = 1.0.0
(II) Loading /usr/X11R6/lib/modules/libcfb.a
(II) Module cfb: vendor="The XFree86 Project"
	compiled for 4.0.3, module version = 1.0.0
(II) Loading /usr/X11R6/lib/modules/libmfb.a
(II) Module mfb: vendor="The XFree86 Project"
	compiled for 4.0.3, module version = 1.0.0
(WW) ATI(0): Failed to set up write-combining range (0xfd000000,0x800000)
(II) ATI(0): Using XFree86 Acceleration Architecture (XAA)
	Screen to screen bit blits
	Solid filled rectangles
	8x8 mono pattern filled rectangles
	Indirect CPU to Screen color expansion
	Solid Lines
	Offscreen Pixmaps
	Setting up tile and stipple cache:
		32 128x128 slots
		20 256x256 slots
		6 512x512 slots
(==) ATI(0): Backing store disabled
(**) Mouse0: Protocol: "PS/2"
(**) Mouse0: Core Pointer
(==) Mouse0: Buttons: 3
(**) Mouse0: ZAxisMapping: buttons 4 and 5
(II) Keyboard "Keyboard0" handled by legacy driver
(II) XINPUT: Adding extended input device "Mouse0" (type: MOUSE)
AUDIT: Tue Apr  2 09:26:34 2002: 1474 X: client 2 rejected from local host
tset: standard error: Inappropriate ioctl for device
stty: standard input: Inappropriate ioctl for device
stty: standard input: Inappropriate ioctl for device
/bin/bash: tabs: command not found
xdm error (pid 1591): pseudoReset timeout
X Error of failed request:  BadValue (integer parameter out of range for operation)
  Major opcode of failed request:  113 (X_KillClient)
  Value in failed request:  0x30
  Serial number of failed request:  143683
  Current serial number in output stream:  143686