CACHE2::DISK$INFSYS:[RJHEARN]_>
CACHE2::DISK$INFSYS:[RJHEARN]_>show queue/all/full    pqau
Printer queue PQAU, idle, on CACHE1::NLP17:, mounted form DEFAULT
  <LPD queue on PQAU.VTMEDNET.ORG TEXT>
  /BASE_PRIORITY=4 /DEFAULT=(FORM=DEFAULT) /LIBRARY=HPLASERJET_III Lowercase /OWNER=[SYSTEM,MANAGER] 
  /PROCESSOR=MULTINET_LPD_SYMBIONT /PROTECTION=(S:M,O:D,G:R,W:S)
CACHE2::DISK$INFSYS:[RJHEARN]_>
CACHE2::DISK$INFSYS:[RJHEARN]_>show dev/full  nlp17:

Printer NLP17:, device type LP11, is online, record-oriented device, carriage
    control, device is spooled through an intermediate device.

    Error count                    0    Operations completed                  0
    Owner process                 ""    Owner UIC                         [1,4]
    Owner process ID        00000000    Dev Prot              S:RWPL,O:RWPL,G,W
    Reference count                0    Default buffer size                   0
    Page width                     0    Page Length                          66
    No Carriage_return  Formfeed        Lowercase
    No Passall          No Wrap         No Printall
    No Fallback         Tab             Truncate
    No Sixels           No Bitmapped            No Polled
    Unidirectional
    Intermediate device: $1$DGA60:
    Associated queue:    PQAU

CACHE2::DISK$INFSYS:[RJHEARN]_>
CACHE2::DISK$INFSYS:[RJHEARN]_>show time
  18-JAN-2010 08:59:12
CACHE2::DISK$INFSYS:[RJHEARN]_>

_