Example of SNMP settings:

Example SNMP settings for a managed server:

HPSIM Server Nodename: hpsim
HPSIM Server FQDN: hpsim.domain.com

Security Tab-->

Send authentication trap: On

Accepted Community Names:
Community   		Rights
public      		READ ONLY
private     		READ WRITE

Accepted Hosts: Accept any SNMP packets from any host

Traps Tab-->

Community Name	Trap Destinations
public			hpsim.domain.com

Following settings unique to the HPSIM CMS SERVER ONLY:

HPSIM Server Nodename: hpsim
HPSIM Server FQDN: hpsim.domain.com

Security Tab-->

Send authentication trap: On

Accepted Community Names:
Community   		Rights
public      		READ ONLY
private     		READ WRITE

Accepted Hosts: Accept any SNMP packets from any host

Traps Tab-->

Community Name   	Trap Destinations
public           		127.0.0.1